#MicroXplorer Configuration settings - do not modify
Dma.Request0=USART2_TX
Dma.RequestsNb=1
Dma.USART2_TX.0.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART2_TX.0.EventEnable=DISABLE
Dma.USART2_TX.0.Instance=DMA1_Channel5
Dma.USART2_TX.0.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_TX.0.MemInc=DMA_MINC_ENABLE
Dma.USART2_TX.0.Mode=DMA_NORMAL
Dma.USART2_TX.0.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_TX.0.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_TX.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.USART2_TX.0.Priority=DMA_PRIORITY_LOW
Dma.USART2_TX.0.RequestNumber=1
Dma.USART2_TX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.USART2_TX.0.SignalID=NONE
Dma.USART2_TX.0.SyncEnable=DISABLE
Dma.USART2_TX.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.USART2_TX.0.SyncRequestNumber=1
Dma.USART2_TX.0.SyncSignalID=NONE
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.CPN=STM32WLE5CBU6
Mcu.Family=STM32WL
Mcu.IP0=ADV_TRACE
Mcu.IP1=DMA
Mcu.IP10=TIMER
Mcu.IP11=TINY_LPM
Mcu.IP12=USART2
Mcu.IP2=MISC
Mcu.IP3=NVIC
Mcu.IP4=RCC
Mcu.IP5=RTC
Mcu.IP6=SEQUENCER
Mcu.IP7=SUBGHZ
Mcu.IP8=SUBGHZ_PHY
Mcu.IP9=SYS
Mcu.IPNb=13
Mcu.Name=STM32WLE5CBUx
Mcu.Package=UFQFPN48
Mcu.Pin0=PB3
Mcu.Pin1=PB4
Mcu.Pin10=VP_ADV_TRACE_VS_ADV_TRACE
Mcu.Pin11=VP_MISC_VS_MISC
Mcu.Pin12=VP_RTC_VS_RTC_Activate
Mcu.Pin13=VP_RTC_VS_RTC_Calendar
Mcu.Pin14=VP_RTC_VS_RTC_Alarm_A_Intern
Mcu.Pin15=VP_SEQUENCER_VS_SEQUENCER
Mcu.Pin16=VP_SUBGHZ_VS_SUBGHZ
Mcu.Pin17=VP_SUBGHZ_PHY_VS_SubGhzPhy
Mcu.Pin18=VP_SYS_VS_None
Mcu.Pin19=VP_TIMER_VS_TIMER
Mcu.Pin2=PB5
Mcu.Pin20=VP_TINY_LPM_VS_TINY_LPM
Mcu.Pin3=PA0
Mcu.Pin4=PA2
Mcu.Pin5=PA3
Mcu.Pin6=OSC_IN
Mcu.Pin7=OSC_OUT
Mcu.Pin8=PC14-OSC32_IN
Mcu.Pin9=PC15-OSC32_OUT
Mcu.PinsNb=21
Mcu.ThirdPartyNb=0
Mcu.UserConstants=RTC_N_PREDIV_S,10;RTC_PREDIV_S,((1<<RTC_N_PREDIV_S)-1);RTC_PREDIV_A,((1<<(15-RTC_N_PREDIV_S))-1)
Mcu.UserName=STM32WLE5CBUx
MxCube.Version=6.6.1
MxDb.Version=DB.6.0.60
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DMA1_Channel5_IRQn=true\:2\:0\:true\:false\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.EXTI0_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.RTC_Alarm_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:true
NVIC.SUBGHZ_Radio_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:true
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:false
NVIC.TAMP_STAMP_LSECSS_SSRU_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:true
NVIC.TimeBase=None
NVIC.USART2_IRQn=true\:2\:0\:true\:false\:true\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
OSC_IN.Mode=HSE-External-Oscillator
OSC_IN.Signal=RCC_OSC_IN
OSC_OUT.Locked=true
OSC_OUT.Mode=HSE-External-Oscillator
OSC_OUT.Signal=RCC_OSC_OUT
PA0.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI,GPIO_PuPd
PA0.GPIO_Label=BUT1
PA0.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PA0.GPIO_PuPd=GPIO_PULLUP
PA0.Locked=true
PA0.Signal=GPXTI0
PA2.GPIOParameters=GPIO_Label,GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd
PA2.GPIO_Label=USARTx_TX
PA2.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA2.GPIO_PuPd=GPIO_PULLUP
PA2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA2.Locked=true
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Label,GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd
PA3.GPIO_Label=USARTx_RX
PA3.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA3.GPIO_PuPd=GPIO_PULLUP
PA3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA3.Locked=true
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=LED2
PB3.Locked=true
PB3.Signal=GPIO_Output
PB4.GPIOParameters=GPIO_Label
PB4.GPIO_Label=LED3
PB4.Locked=true
PB4.Signal=GPIO_Output
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=LED1
PB5.Locked=true
PB5.Signal=GPIO_Output
PC14-OSC32_IN.Locked=true
PC14-OSC32_IN.Mode=LSE-External-Oscillator
PC14-OSC32_IN.Signal=RCC_OSC32_IN
PC15-OSC32_OUT.Locked=true
PC15-OSC32_OUT.Mode=LSE-External-Oscillator
PC15-OSC32_OUT.Signal=RCC_OSC32_OUT
PCC.SUBGHZ.FrequencyBand=High
PCC.SUBGHZ.Modulation=FSK
PCC.SUBGHZ.OptionalSettings=false
PCC.SUBGHZ.Output.Power=14
PCC.SUBGHZ.PowerAmplifier=Low Power
PCC.SUBGHZ.RxBoosted=false
PCC.SUBGHZ.SMPS=Off
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32WLE5CBUx
ProjectManager.Example=SubGHz_Phy_PingPong
ProjectManager.ExampleSource=CubeFw
ProjectManager.FirmwarePackage=STM32Cube FW_WL V1.2.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=0
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=SubGHz_Phy_PingPong.ioc
ProjectManager.ProjectName=SubGHz_Phy_PingPong
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x800
ProjectManager.TargetToolchain=MDK-ARM V5.32
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-false,2-MX_DMA_Init-DMA-true-HAL-false,3-SystemClock_Config-RCC-false-HAL-false,4-MX_RTC_Init-RTC-true-HAL-false,5-MX_USART2_UART_Init-USART2-true-HAL-false,6-MX_SubGHz_Phy_Init-SUBGHZ_PHY-false-HAL-false,7-MX_SUBGHZ_Init-SUBGHZ-true-HAL-false
RCC.AHBFreq_Value=48000000
RCC.APB1Freq_Value=48000000
RCC.APB1TimFreq_Value=48000000
RCC.APB2Freq_Value=48000000
RCC.APB2TimFreq_Value=48000000
RCC.APB3Freq_Value=48000000
RCC.CortexFreq_Value=48000000
RCC.FCLKCortexFreq_Value=48000000
RCC.FLatency=FLASH_LATENCY_2
RCC.FamilyName=M
RCC.HCLK3Freq_Value=48000000
RCC.HCLKFreq_Value=48000000
RCC.HSE_VALUE=8000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=48000000
RCC.I2C2Freq_Value=48000000
RCC.I2C3Freq_Value=48000000
RCC.I2S2Freq_Value=16000000
RCC.IPParameters=AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,APB3Freq_Value,CortexFreq_Value,FCLKCortexFreq_Value,FLatency,FamilyName,HCLK3Freq_Value,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2S2Freq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIM3Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_Drive_Capability,LSE_VALUE,MCO1PinFreq_Value,MSIClockRange,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PWRFreq_Value,PWR_Regulator_Voltage_Scale,RNGFreq_Value,RTCClockSelection,RTCFreq_Value,SYSCLKFreq_VALUE,USART1Freq_Value,USART2CLockSelection,USART2Freq_Value,VCOInputFreq_Value,VCOOutputFreq_Value
RCC.LPTIM1Freq_Value=48000000
RCC.LPTIM2Freq_Value=48000000
RCC.LPTIM3Freq_Value=48000000
RCC.LPUART1Freq_Value=48000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_Drive_Capability=RCC_LSEDRIVE_LOW
RCC.LSE_VALUE=32768
RCC.MCO1PinFreq_Value=48000000
RCC.MSIClockRange=RCC_MSIRANGE_11
RCC.PLLPoutputFreq_Value=192000000
RCC.PLLQoutputFreq_Value=192000000
RCC.PLLRCLKFreq_Value=192000000
RCC.PWRFreq_Value=48000000
RCC.PWR_Regulator_Voltage_Scale=PWR_REGULATOR_VOLTAGE_SCALE1
RCC.RNGFreq_Value=32000
RCC.RTCClockSelection=RCC_RTCCLKSOURCE_LSE
RCC.RTCFreq_Value=32768
RCC.SYSCLKFreq_VALUE=48000000
RCC.USART1Freq_Value=48000000
RCC.USART2CLockSelection=RCC_USART2CLKSOURCE_SYSCLK
RCC.USART2Freq_Value=48000000
RCC.VCOInputFreq_Value=48000000
RCC.VCOOutputFreq_Value=384000000
RTC.Alarm-Alarm\ A=RTC_ALARM_A
RTC.AlarmSubSecondMask-Alarm\ A=RTC_ALARMSUBSECONDBINMASK_NONE
RTC.AsynchPrediv=RTC_PREDIV_A
RTC.BinMode=RTC_BINARY_ONLY
RTC.BinaryAutoClr_A-Alarm\ A=RTC_ALARMSUBSECONDBIN_AUTOCLR_NO
RTC.IPParameters=AsynchPrediv,BinMode,SubSeconds_A-Alarm A,BinaryAutoClr_A-Alarm A,AlarmSubSecondMask-Alarm A,Alarm-Alarm A
RTC.SubSeconds_A-Alarm\ A=0
SH.GPXTI0.0=GPIO_EXTI0
SH.GPXTI0.ConfNb=1
SUBGHZ.BaudratePrescaler=SUBGHZSPI_BAUDRATEPRESCALER_4
SUBGHZ.IPParameters=BaudratePrescaler
SUBGHZ_PHY.APP_LOG_ENABLED=true
SUBGHZ_PHY.Activate_DEBUG_LINE=false
SUBGHZ_PHY.Activate_RADIO_BOARD_INTERFACE=Bsp
SUBGHZ_PHY.IPParameters=IS_TCXO_SUPPORTED,IS_DCDC_SUPPORTED,Activate_DEBUG_LINE,SUBGHZ_APPLICATION,Activate_RADIO_BOARD_INTERFACE,TX_RFO_CONFIG,VERBOSE_LEVEL,APP_LOG_ENABLED,LOW_POWER_DISABLE,MODEM_USED,REGION,LORA_BANDWIDTH,LORA_SPREADING_FACTOR,LORA_CODINGRATE,LORA_PREAMBLE_LENGTH,LORA_SYMBOL_TIMEOUT,LORA_FIX_LENGTH_PAYLOAD_ON,LORA_IQ_INVERSION_ON,PAYLOAD_LEN,RF_WAKEUP_TIME,MW_LOG_ENABLED
SUBGHZ_PHY.IS_DCDC_SUPPORTED=true
SUBGHZ_PHY.IS_TCXO_SUPPORTED=true
SUBGHZ_PHY.LORA_BANDWIDTH=0
SUBGHZ_PHY.LORA_CODINGRATE=1
SUBGHZ_PHY.LORA_FIX_LENGTH_PAYLOAD_ON=false
SUBGHZ_PHY.LORA_IQ_INVERSION_ON=false
SUBGHZ_PHY.LORA_PREAMBLE_LENGTH=8
SUBGHZ_PHY.LORA_SPREADING_FACTOR=10
SUBGHZ_PHY.LORA_SYMBOL_TIMEOUT=5
SUBGHZ_PHY.LOW_POWER_DISABLE=true
SUBGHZ_PHY.MODEM_USED=USE_MODEM_LORA
SUBGHZ_PHY.MW_LOG_ENABLED=true
SUBGHZ_PHY.PAYLOAD_LEN=32
SUBGHZ_PHY.REGION=REGION_CN470
SUBGHZ_PHY.RF_WAKEUP_TIME=1
SUBGHZ_PHY.SUBGHZ_APPLICATION=SUBGHZ_ADV_APPLICATION
SUBGHZ_PHY.TX_RFO_CONFIG=RBI_CONF_RFO_LP_HP
SUBGHZ_PHY.VERBOSE_LEVEL=VLEVEL_M
SubGHz_Phy.BSP.number=2
SubGHz_Phy0.BSP.STBoard=false
SubGHz_Phy0.BSP.api=Unknown
SubGHz_Phy0.BSP.component=
SubGHz_Phy0.BSP.condition=\!SEM_SUBGHZ_USER_APPLICATION | SEM_SUBGHZ_USE_RTC
SubGHz_Phy0.BSP.instance=RTC
SubGHz_Phy0.BSP.ip=RTC
SubGHz_Phy0.BSP.mode=RTC Enabled
SubGHz_Phy0.BSP.name=RTC
SubGHz_Phy0.BSP.semaphore=
SubGHz_Phy0.BSP.solution=RTC
SubGHz_Phy1.BSP.STBoard=false
SubGHz_Phy1.BSP.api=Unknown
SubGHz_Phy1.BSP.component=
SubGHz_Phy1.BSP.condition=\!SEM_SUBGHZ_USER_APPLICATION | SEM_SUBGHZ_USE_UART
SubGHz_Phy1.BSP.instance=USART2
SubGHz_Phy1.BSP.ip=(LPU|US)ART
SubGHz_Phy1.BSP.mode=Asynchronous
SubGHz_Phy1.BSP.name=USART
SubGHz_Phy1.BSP.semaphore=
SubGHz_Phy1.BSP.solution=USART2
USART2.AutoBaudRateEnableParam=UART_ADVFEATURE_AUTOBAUDRATE_DISABLE
USART2.BaudRate=115200
USART2.ClockPrescaler=PRESCALER_DIV1
USART2.DMADisableonRxErrorParam=ADVFEATURE_DMA_ENABLEONRXERROR
USART2.DataInvertParam=ADVFEATURE_DATAINV_DISABLE
USART2.FIFOMode=FIFOMODE_ENABLE
USART2.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,OneBitSampling,ClockPrescaler,FIFOMode,TXFIFOThreshold,RXFIFOThreshold,AutoBaudRateEnableParam,TxPinLevelInvertParam,RxPinLevelInvertParam,DataInvertParam,SwapParam,OverrunDisableParam,DMADisableonRxErrorParam,MSBFirstParam,VirtualMode-Asynchronous
USART2.MSBFirstParam=ADVFEATURE_MSBFIRST_DISABLE
USART2.Mode=MODE_TX_RX
USART2.OneBitSampling=UART_ONE_BIT_SAMPLE_DISABLE
USART2.OverSampling=UART_OVERSAMPLING_16
USART2.OverrunDisableParam=ADVFEATURE_OVERRUN_ENABLE
USART2.Parity=PARITY_NONE
USART2.RXFIFOThreshold=RXFIFO_THRESHOLD_1EIGHTHFULL
USART2.RxPinLevelInvertParam=ADVFEATURE_RXINV_DISABLE
USART2.StopBits=STOPBITS_1
USART2.SwapParam=ADVFEATURE_SWAP_DISABLE
USART2.TXFIFOThreshold=TXFIFO_THRESHOLD_1EIGHTHFULL
USART2.TxPinLevelInvertParam=ADVFEATURE_TXINV_DISABLE
USART2.VirtualMode-Asynchronous=VM_ASYNC
USART2.WordLength=WORDLENGTH_8B
VP_ADV_TRACE_VS_ADV_TRACE.Mode=ADV_TRACE_Enabled
VP_ADV_TRACE_VS_ADV_TRACE.Signal=ADV_TRACE_VS_ADV_TRACE
VP_MISC_VS_MISC.Mode=MISC_Enabled
VP_MISC_VS_MISC.Signal=MISC_VS_MISC
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_RTC_VS_RTC_Alarm_A_Intern.Mode=Alarm A
VP_RTC_VS_RTC_Alarm_A_Intern.Signal=RTC_VS_RTC_Alarm_A_Intern
VP_RTC_VS_RTC_Calendar.Mode=RTC_Calendar
VP_RTC_VS_RTC_Calendar.Signal=RTC_VS_RTC_Calendar
VP_SEQUENCER_VS_SEQUENCER.Mode=SEQUENCER_Enabled
VP_SEQUENCER_VS_SEQUENCER.Signal=SEQUENCER_VS_SEQUENCER
VP_SUBGHZ_PHY_VS_SubGhzPhy.Mode=SubGhzPhy_Enabled
VP_SUBGHZ_PHY_VS_SubGhzPhy.Signal=SUBGHZ_PHY_VS_SubGhzPhy
VP_SUBGHZ_VS_SUBGHZ.Mode=SUBGHZ_Activate
VP_SUBGHZ_VS_SUBGHZ.Signal=SUBGHZ_VS_SUBGHZ
VP_SYS_VS_None.Mode=None
VP_SYS_VS_None.Signal=SYS_VS_None
VP_TIMER_VS_TIMER.Mode=TIMER_Enabled
VP_TIMER_VS_TIMER.Signal=TIMER_VS_TIMER
VP_TINY_LPM_VS_TINY_LPM.Mode=TINY_LPM_Enabled
VP_TINY_LPM_VS_TINY_LPM.Signal=TINY_LPM_VS_TINY_LPM
board=NUCLEO-WL55JC1
