Component: ARM Compiler 5.05 update 1 (build 106) Tool: armlink [4d0efa]

==============================================================================

Section Cross References

    startup_stm32wle5xx.o(STACK) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_stm32wle5xx.o(HEAP) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_stm32wle5xx.o(RESET) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_stm32wle5xx.o(RESET) refers to startup_stm32wle5xx.o(STACK) for __initial_sp
    startup_stm32wle5xx.o(RESET) refers to startup_stm32wle5xx.o(.text) for Reset_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.NMI_Handler) for NMI_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.HardFault_Handler) for HardFault_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.MemManage_Handler) for MemManage_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.BusFault_Handler) for BusFault_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.UsageFault_Handler) for UsageFault_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.SVC_Handler) for SVC_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.DebugMon_Handler) for DebugMon_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.PendSV_Handler) for PendSV_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.SysTick_Handler) for SysTick_Handler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.TAMP_STAMP_LSECSS_SSRU_IRQHandler) for TAMP_STAMP_LSECSS_SSRU_IRQHandler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.EXTI0_IRQHandler) for EXTI0_IRQHandler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.DMA1_Channel5_IRQHandler) for DMA1_Channel5_IRQHandler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.USART2_IRQHandler) for USART2_IRQHandler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.RTC_Alarm_IRQHandler) for RTC_Alarm_IRQHandler
    startup_stm32wle5xx.o(RESET) refers to stm32wlxx_it.o(i.SUBGHZ_Radio_IRQHandler) for SUBGHZ_Radio_IRQHandler
    startup_stm32wle5xx.o(.text) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_stm32wle5xx.o(.text) refers to system_stm32wlxx.o(i.SystemInit) for SystemInit
    startup_stm32wle5xx.o(.text) refers to __main.o(!!!main) for __main
    startup_stm32wle5xx.o(.text) refers to startup_stm32wle5xx.o(HEAP) for Heap_Mem
    startup_stm32wle5xx.o(.text) refers to startup_stm32wle5xx.o(STACK) for Stack_Mem
    main.o(i.SystemClock_Config) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    main.o(i.SystemClock_Config) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess) for HAL_PWR_EnableBkUpAccess
    main.o(i.SystemClock_Config) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) for HAL_RCC_OscConfig
    main.o(i.SystemClock_Config) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) for HAL_RCC_ClockConfig
    main.o(i.main) refers to stm32wlxx_hal.o(i.HAL_Init) for HAL_Init
    main.o(i.main) refers to main.o(i.SystemClock_Config) for SystemClock_Config
    main.o(i.main) refers to gpio.o(i.MX_GPIO_Init) for MX_GPIO_Init
    main.o(i.main) refers to app_subghz_phy.o(i.MX_SubGHz_Phy_Init) for MX_SubGHz_Phy_Init
    gpio.o(i.MX_GPIO_Init) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    gpio.o(i.MX_GPIO_Init) refers to gpio.o(i.LL_AHB2_GRP1_EnableClock) for LL_AHB2_GRP1_EnableClock
    gpio.o(i.MX_GPIO_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    gpio.o(i.MX_GPIO_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    gpio.o(i.MX_GPIO_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    gpio.o(i.MX_GPIO_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    dma.o(i.MX_DMA_Init) refers to dma.o(i.LL_AHB1_GRP1_EnableClock) for LL_AHB1_GRP1_EnableClock
    dma.o(i.MX_DMA_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    dma.o(i.MX_DMA_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    rtc.o(i.HAL_RTC_MspDeInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    rtc.o(i.HAL_RTC_MspInit) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    rtc.o(i.HAL_RTC_MspInit) refers to stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) for HAL_RCCEx_PeriphCLKConfig
    rtc.o(i.HAL_RTC_MspInit) refers to main.o(i.Error_Handler) for Error_Handler
    rtc.o(i.HAL_RTC_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    rtc.o(i.HAL_RTC_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    rtc.o(i.MX_RTC_Init) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    rtc.o(i.MX_RTC_Init) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_Init) for HAL_RTC_Init
    rtc.o(i.MX_RTC_Init) refers to main.o(i.Error_Handler) for Error_Handler
    rtc.o(i.MX_RTC_Init) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSSRU_IT) for HAL_RTCEx_SetSSRU_IT
    rtc.o(i.MX_RTC_Init) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) for HAL_RTC_SetAlarm_IT
    rtc.o(i.MX_RTC_Init) refers to rtc.o(.bss) for .bss
    subghz.o(i.HAL_SUBGHZ_MspDeInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    subghz.o(i.HAL_SUBGHZ_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    subghz.o(i.HAL_SUBGHZ_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    subghz.o(i.MX_SUBGHZ_Init) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) for HAL_SUBGHZ_Init
    subghz.o(i.MX_SUBGHZ_Init) refers to main.o(i.Error_Handler) for Error_Handler
    subghz.o(i.MX_SUBGHZ_Init) refers to subghz.o(.bss) for .bss
    stm32_lpm_if.o(i.PWR_EnterSleepMode) refers to stm32wlxx_hal.o(i.HAL_SuspendTick) for HAL_SuspendTick
    stm32_lpm_if.o(i.PWR_EnterSleepMode) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode) for HAL_PWR_EnterSLEEPMode
    stm32_lpm_if.o(i.PWR_EnterStopMode) refers to stm32wlxx_hal.o(i.HAL_SuspendTick) for HAL_SuspendTick
    stm32_lpm_if.o(i.PWR_EnterStopMode) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP2Mode) for HAL_PWREx_EnterSTOP2Mode
    stm32_lpm_if.o(i.PWR_ExitSleepMode) refers to stm32wlxx_hal.o(i.HAL_ResumeTick) for HAL_ResumeTick
    stm32_lpm_if.o(i.PWR_ExitStopMode) refers to stm32wlxx_hal.o(i.HAL_ResumeTick) for HAL_ResumeTick
    stm32_lpm_if.o(i.PWR_ExitStopMode) refers to usart_if.o(i.vcom_Resume) for vcom_Resume
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_EnterSleepMode) for PWR_EnterSleepMode
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_ExitSleepMode) for PWR_ExitSleepMode
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_EnterStopMode) for PWR_EnterStopMode
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_ExitStopMode) for PWR_ExitStopMode
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_EnterOffMode) for PWR_EnterOffMode
    stm32_lpm_if.o(.constdata) refers to stm32_lpm_if.o(i.PWR_ExitOffMode) for PWR_ExitOffMode
    sys_app.o(i.HAL_Delay) refers to timer_if.o(i.TIMER_IF_DelayMs) for TIMER_IF_DelayMs
    sys_app.o(i.HAL_GetTick) refers to timer_if.o(i.TIMER_IF_GetTimerValue) for TIMER_IF_GetTimerValue
    sys_app.o(i.HAL_GetTick) refers to sys_app.o(.data) for .data
    sys_app.o(i.SystemApp_Init) refers to stm32_timer.o(i.UTIL_TIMER_Init) for UTIL_TIMER_Init
    sys_app.o(i.SystemApp_Init) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init) for UTIL_ADV_TRACE_Init
    sys_app.o(i.SystemApp_Init) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_RegisterTimeStampFunction) for UTIL_ADV_TRACE_RegisterTimeStampFunction
    sys_app.o(i.SystemApp_Init) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetVerboseLevel) for UTIL_ADV_TRACE_SetVerboseLevel
    sys_app.o(i.SystemApp_Init) refers to stm32_lpm.o(i.UTIL_LPM_Init) for UTIL_LPM_Init
    sys_app.o(i.SystemApp_Init) refers to stm32_lpm.o(i.UTIL_LPM_SetOffMode) for UTIL_LPM_SetOffMode
    sys_app.o(i.SystemApp_Init) refers to stm32_lpm.o(i.UTIL_LPM_SetStopMode) for UTIL_LPM_SetStopMode
    sys_app.o(i.SystemApp_Init) refers to sys_app.o(.data) for .data
    sys_app.o(i.SystemApp_Init) refers to sys_app.o(i.TimestampNow) for TimestampNow
    sys_app.o(i.TimestampNow) refers to stm32_systime.o(i.SysTimeGet) for SysTimeGet
    sys_app.o(i.TimestampNow) refers to sys_app.o(i.tiny_snprintf_like) for tiny_snprintf_like
    sys_app.o(i.TimestampNow) refers to strlen.o(.text) for strlen
    sys_app.o(i.UTIL_ADV_TRACE_PostSendHook) refers to stm32_lpm.o(i.UTIL_LPM_SetStopMode) for UTIL_LPM_SetStopMode
    sys_app.o(i.UTIL_ADV_TRACE_PreSendHook) refers to stm32_lpm.o(i.UTIL_LPM_SetStopMode) for UTIL_LPM_SetStopMode
    sys_app.o(i.UTIL_SEQ_Idle) refers to stm32_lpm.o(i.UTIL_LPM_EnterLowPower) for UTIL_LPM_EnterLowPower
    sys_app.o(i.tiny_snprintf_like) refers to stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like) for tiny_vsnprintf_like
    sys_debug.o(i.DBG_Init) refers to stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGSleepMode) for HAL_DBGMCU_DisableDBGSleepMode
    sys_debug.o(i.DBG_Init) refers to stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGStopMode) for HAL_DBGMCU_DisableDBGStopMode
    sys_debug.o(i.DBG_Init) refers to stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGStandbyMode) for HAL_DBGMCU_DisableDBGStandbyMode
    timer_if.o(i.HAL_RTCEx_SSRUEventCallback) refers to timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks) for TIMER_IF_BkUp_Read_MSBticks
    timer_if.o(i.HAL_RTCEx_SSRUEventCallback) refers to timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks) for TIMER_IF_BkUp_Write_MSBticks
    timer_if.o(i.HAL_RTC_AlarmAEventCallback) refers to stm32_timer.o(i.UTIL_TIMER_IRQ_Handler) for UTIL_TIMER_IRQ_Handler
    timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead) for HAL_RTCEx_BKUPRead
    timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_BkUp_Read_Seconds) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead) for HAL_RTCEx_BKUPRead
    timer_if.o(i.TIMER_IF_BkUp_Read_Seconds) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_BkUp_Read_SubSeconds) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead) for HAL_RTCEx_BKUPRead
    timer_if.o(i.TIMER_IF_BkUp_Read_SubSeconds) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite) for HAL_RTCEx_BKUPWrite
    timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_BkUp_Write_Seconds) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite) for HAL_RTCEx_BKUPWrite
    timer_if.o(i.TIMER_IF_BkUp_Write_Seconds) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_BkUp_Write_SubSeconds) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite) for HAL_RTCEx_BKUPWrite
    timer_if.o(i.TIMER_IF_BkUp_Write_SubSeconds) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_Convert_ms2Tick) refers to lludivv7m.o(.text) for __aeabi_uldivmod
    timer_if.o(i.TIMER_IF_DelayMs) refers to timer_if.o(i.TIMER_IF_Convert_ms2Tick) for TIMER_IF_Convert_ms2Tick
    timer_if.o(i.TIMER_IF_DelayMs) refers to timer_if.o(i.GetTimerTicks) for GetTimerTicks
    timer_if.o(i.TIMER_IF_GetTime) refers to timer_if.o(i.GetTimerTicks) for GetTimerTicks
    timer_if.o(i.TIMER_IF_GetTime) refers to timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks) for TIMER_IF_BkUp_Read_MSBticks
    timer_if.o(i.TIMER_IF_GetTime) refers to timer_if.o(i.TIMER_IF_Convert_Tick2ms) for TIMER_IF_Convert_Tick2ms
    timer_if.o(i.TIMER_IF_GetTimerContext) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_GetTimerElapsedTime) refers to timer_if.o(i.GetTimerTicks) for GetTimerTicks
    timer_if.o(i.TIMER_IF_GetTimerElapsedTime) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_GetTimerValue) refers to timer_if.o(i.GetTimerTicks) for GetTimerTicks
    timer_if.o(i.TIMER_IF_GetTimerValue) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_Init) refers to rtc.o(i.MX_RTC_Init) for MX_RTC_Init
    timer_if.o(i.TIMER_IF_Init) refers to timer_if.o(i.TIMER_IF_StopTimer) for TIMER_IF_StopTimer
    timer_if.o(i.TIMER_IF_Init) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm) for HAL_RTC_DeactivateAlarm
    timer_if.o(i.TIMER_IF_Init) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_EnableBypassShadow) for HAL_RTCEx_EnableBypassShadow
    timer_if.o(i.TIMER_IF_Init) refers to timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks) for TIMER_IF_BkUp_Write_MSBticks
    timer_if.o(i.TIMER_IF_Init) refers to timer_if.o(i.TIMER_IF_SetTimerContext) for TIMER_IF_SetTimerContext
    timer_if.o(i.TIMER_IF_Init) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_Init) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_SetTimerContext) refers to timer_if.o(i.GetTimerTicks) for GetTimerTicks
    timer_if.o(i.TIMER_IF_SetTimerContext) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_StartTimer) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    timer_if.o(i.TIMER_IF_StartTimer) refers to timer_if.o(i.TIMER_IF_StopTimer) for TIMER_IF_StopTimer
    timer_if.o(i.TIMER_IF_StartTimer) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) for HAL_RTC_SetAlarm_IT
    timer_if.o(i.TIMER_IF_StartTimer) refers to main.o(i.Error_Handler) for Error_Handler
    timer_if.o(i.TIMER_IF_StartTimer) refers to timer_if.o(.data) for .data
    timer_if.o(i.TIMER_IF_StartTimer) refers to rtc.o(.bss) for hrtc
    timer_if.o(i.TIMER_IF_StopTimer) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm) for HAL_RTC_DeactivateAlarm
    timer_if.o(i.TIMER_IF_StopTimer) refers to rtc.o(.bss) for hrtc
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_Init) for TIMER_IF_Init
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_StartTimer) for TIMER_IF_StartTimer
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_StopTimer) for TIMER_IF_StopTimer
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_SetTimerContext) for TIMER_IF_SetTimerContext
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_GetTimerContext) for TIMER_IF_GetTimerContext
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_GetTimerElapsedTime) for TIMER_IF_GetTimerElapsedTime
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_GetTimerValue) for TIMER_IF_GetTimerValue
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_GetMinimumTimeout) for TIMER_IF_GetMinimumTimeout
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_Convert_ms2Tick) for TIMER_IF_Convert_ms2Tick
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_Convert_Tick2ms) for TIMER_IF_Convert_Tick2ms
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_BkUp_Write_Seconds) for TIMER_IF_BkUp_Write_Seconds
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_BkUp_Read_Seconds) for TIMER_IF_BkUp_Read_Seconds
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_BkUp_Write_SubSeconds) for TIMER_IF_BkUp_Write_SubSeconds
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_BkUp_Read_SubSeconds) for TIMER_IF_BkUp_Read_SubSeconds
    timer_if.o(.constdata) refers to timer_if.o(i.TIMER_IF_GetTime) for TIMER_IF_GetTime
    usart_if.o(i.HAL_UART_RxCpltCallback) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Receive_IT) for HAL_UART_Receive_IT
    usart_if.o(i.HAL_UART_RxCpltCallback) refers to usart_if.o(.data) for .data
    usart_if.o(i.HAL_UART_TxCpltCallback) refers to usart_if.o(.data) for .data
    usart_if.o(i.vcom_DeInit) refers to usart.o(i.HAL_UART_MspDeInit) for HAL_UART_MspDeInit
    usart_if.o(i.vcom_DeInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    usart_if.o(i.vcom_DeInit) refers to usart.o(.bss) for huart2
    usart_if.o(i.vcom_Init) refers to dma.o(i.MX_DMA_Init) for MX_DMA_Init
    usart_if.o(i.vcom_Init) refers to usart.o(i.MX_USART2_UART_Init) for MX_USART2_UART_Init
    usart_if.o(i.vcom_Init) refers to usart_if.o(.data) for .data
    usart_if.o(i.vcom_ReceiveInit) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_StopModeWakeUpSourceConfig) for HAL_UARTEx_StopModeWakeUpSourceConfig
    usart_if.o(i.vcom_ReceiveInit) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableStopMode) for HAL_UARTEx_EnableStopMode
    usart_if.o(i.vcom_ReceiveInit) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Receive_IT) for HAL_UART_Receive_IT
    usart_if.o(i.vcom_ReceiveInit) refers to usart_if.o(.data) for .data
    usart_if.o(i.vcom_ReceiveInit) refers to usart.o(.bss) for huart2
    usart_if.o(i.vcom_Resume) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Init) for HAL_UART_Init
    usart_if.o(i.vcom_Resume) refers to main.o(i.Error_Handler) for Error_Handler
    usart_if.o(i.vcom_Resume) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Init) for HAL_DMA_Init
    usart_if.o(i.vcom_Resume) refers to usart.o(.bss) for huart2
    usart_if.o(i.vcom_Trace) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Transmit) for HAL_UART_Transmit
    usart_if.o(i.vcom_Trace) refers to usart.o(.bss) for huart2
    usart_if.o(i.vcom_Trace_DMA) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA) for HAL_UART_Transmit_DMA
    usart_if.o(i.vcom_Trace_DMA) refers to usart.o(.bss) for huart2
    usart_if.o(.constdata) refers to usart_if.o(i.vcom_Init) for vcom_Init
    usart_if.o(.constdata) refers to usart_if.o(i.vcom_DeInit) for vcom_DeInit
    usart_if.o(.constdata) refers to usart_if.o(i.vcom_ReceiveInit) for vcom_ReceiveInit
    usart_if.o(.constdata) refers to usart_if.o(i.vcom_Trace_DMA) for vcom_Trace_DMA
    usart.o(i.HAL_UART_MspDeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    usart.o(i.HAL_UART_MspDeInit) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_DeInit) for HAL_DMA_DeInit
    usart.o(i.HAL_UART_MspDeInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    usart.o(i.HAL_UART_MspInit) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    usart.o(i.HAL_UART_MspInit) refers to stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) for HAL_RCCEx_PeriphCLKConfig
    usart.o(i.HAL_UART_MspInit) refers to main.o(i.Error_Handler) for Error_Handler
    usart.o(i.HAL_UART_MspInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    usart.o(i.HAL_UART_MspInit) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Init) for HAL_DMA_Init
    usart.o(i.HAL_UART_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    usart.o(i.HAL_UART_MspInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    usart.o(i.HAL_UART_MspInit) refers to usart.o(.bss) for .bss
    usart.o(i.MX_USART2_UART_Init) refers to stm32wlxx_hal_uart.o(i.HAL_UART_Init) for HAL_UART_Init
    usart.o(i.MX_USART2_UART_Init) refers to main.o(i.Error_Handler) for Error_Handler
    usart.o(i.MX_USART2_UART_Init) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetTxFifoThreshold) for HAL_UARTEx_SetTxFifoThreshold
    usart.o(i.MX_USART2_UART_Init) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetRxFifoThreshold) for HAL_UARTEx_SetRxFifoThreshold
    usart.o(i.MX_USART2_UART_Init) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableFifoMode) for HAL_UARTEx_EnableFifoMode
    usart.o(i.MX_USART2_UART_Init) refers to usart.o(.bss) for .bss
    stm32wlxx_it.o(i.DMA1_Channel5_IRQHandler) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_IRQHandler) for HAL_DMA_IRQHandler
    stm32wlxx_it.o(i.DMA1_Channel5_IRQHandler) refers to usart.o(.bss) for hdma_usart2_tx
    stm32wlxx_it.o(i.EXTI0_IRQHandler) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler) for HAL_GPIO_EXTI_IRQHandler
    stm32wlxx_it.o(i.RTC_Alarm_IRQHandler) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler) for HAL_RTC_AlarmIRQHandler
    stm32wlxx_it.o(i.RTC_Alarm_IRQHandler) refers to rtc.o(.bss) for hrtc
    stm32wlxx_it.o(i.SUBGHZ_Radio_IRQHandler) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) for HAL_SUBGHZ_IRQHandler
    stm32wlxx_it.o(i.SUBGHZ_Radio_IRQHandler) refers to subghz.o(.bss) for hsubghz
    stm32wlxx_it.o(i.TAMP_STAMP_LSECSS_SSRU_IRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SSRUIRQHandler) for HAL_RTCEx_SSRUIRQHandler
    stm32wlxx_it.o(i.TAMP_STAMP_LSECSS_SSRU_IRQHandler) refers to rtc.o(.bss) for hrtc
    stm32wlxx_it.o(i.USART2_IRQHandler) refers to stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) for HAL_UART_IRQHandler
    stm32wlxx_it.o(i.USART2_IRQHandler) refers to usart.o(.bss) for huart2
    app_subghz_phy.o(i.MX_SubGHz_Phy_Init) refers to sys_app.o(i.SystemApp_Init) for SystemApp_Init
    app_subghz_phy.o(i.MX_SubGHz_Phy_Init) refers to subghz_phy_app.o(i.SubghzApp_Init) for SubghzApp_Init
    app_subghz_phy.o(i.MX_SubGHz_Phy_Process) refers to stm32_seq.o(i.UTIL_SEQ_Run) for UTIL_SEQ_Run
    subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback) refers to stm32wlxx_lm40x.o(i.BSP_LED_Toggle) for BSP_LED_Toggle
    subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback) refers to sys_app.o(i.HAL_Delay) for HAL_Delay
    subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnRxDone) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnRxDone) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    subghz_phy_app.o(i.OnRxDone) refers to rt_memcpy_v6.o(.text) for __aeabi_memcpy
    subghz_phy_app.o(i.OnRxDone) refers to stm32_seq.o(i.UTIL_SEQ_SetTask) for UTIL_SEQ_SetTask
    subghz_phy_app.o(i.OnRxDone) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.OnRxDone) refers to subghz_phy_app.o(.bss) for .bss
    subghz_phy_app.o(i.OnRxError) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnRxError) refers to stm32_seq.o(i.UTIL_SEQ_SetTask) for UTIL_SEQ_SetTask
    subghz_phy_app.o(i.OnRxError) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.OnRxTimeout) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnRxTimeout) refers to stm32_seq.o(i.UTIL_SEQ_SetTask) for UTIL_SEQ_SetTask
    subghz_phy_app.o(i.OnRxTimeout) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.OnTxDone) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnTxDone) refers to stm32_seq.o(i.UTIL_SEQ_SetTask) for UTIL_SEQ_SetTask
    subghz_phy_app.o(i.OnTxDone) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.OnTxTimeout) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnTxTimeout) refers to stm32_seq.o(i.UTIL_SEQ_SetTask) for UTIL_SEQ_SetTask
    subghz_phy_app.o(i.OnTxTimeout) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.OnledEvent) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_TogglePin) for HAL_GPIO_TogglePin
    subghz_phy_app.o(i.OnledEvent) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.OnledEvent) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    subghz_phy_app.o(i.OnledEvent) refers to subghz_phy_app.o(.bss) for .bss
    subghz_phy_app.o(i.OnledEvent) refers to radio.o(.constdata) for Radio
    subghz_phy_app.o(i.PingPong_Process) refers to strncmp.o(.text) for strncmp
    subghz_phy_app.o(i.PingPong_Process) refers to stm32_timer.o(i.UTIL_TIMER_Stop) for UTIL_TIMER_Stop
    subghz_phy_app.o(i.PingPong_Process) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    subghz_phy_app.o(i.PingPong_Process) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_TogglePin) for HAL_GPIO_TogglePin
    subghz_phy_app.o(i.PingPong_Process) refers to sys_app.o(i.HAL_Delay) for HAL_Delay
    subghz_phy_app.o(i.PingPong_Process) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.PingPong_Process) refers to radio.o(.constdata) for Radio
    subghz_phy_app.o(i.PingPong_Process) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.PingPong_Process) refers to subghz_phy_app.o(.bss) for .bss
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32_timer.o(i.UTIL_TIMER_Create) for UTIL_TIMER_Create
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32wlxx_lm40x.o(i.BSP_LED_Init) for BSP_LED_Init
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32wlxx_lm40x.o(i.BSP_PB_Init) for BSP_PB_Init
    subghz_phy_app.o(i.SubghzApp_Init) refers to rt_memclr.o(.text) for __aeabi_memclr
    subghz_phy_app.o(i.SubghzApp_Init) refers to stm32_seq.o(i.UTIL_SEQ_RegTask) for UTIL_SEQ_RegTask
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnledEvent) for OnledEvent
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(.bss) for .bss
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnTxDone) for OnTxDone
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnRxDone) for OnRxDone
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnTxTimeout) for OnTxTimeout
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnRxTimeout) for OnRxTimeout
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.OnRxError) for OnRxError
    subghz_phy_app.o(i.SubghzApp_Init) refers to radio.o(.constdata) for Radio
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(.data) for .data
    subghz_phy_app.o(i.SubghzApp_Init) refers to subghz_phy_app.o(i.PingPong_Process) for PingPong_Process
    radio_board_if.o(i.RBI_ConfigRFSwitch) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_ConfigRFSwitch) for BSP_RADIO_ConfigRFSwitch
    radio_board_if.o(i.RBI_DeInit) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_DeInit) for BSP_RADIO_DeInit
    radio_board_if.o(i.RBI_GetRFOMaxPowerConfig) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetRFOMaxPowerConfig) for BSP_RADIO_GetRFOMaxPowerConfig
    radio_board_if.o(i.RBI_GetTxConfig) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetTxConfig) for BSP_RADIO_GetTxConfig
    radio_board_if.o(i.RBI_Init) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init) for BSP_RADIO_Init
    radio_board_if.o(i.RBI_IsDCDC) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsDCDC) for BSP_RADIO_IsDCDC
    radio_board_if.o(i.RBI_IsTCXO) refers to stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsTCXO) for BSP_RADIO_IsTCXO
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_IsReady) for LL_RCC_HSI_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSE_IsReady) for LL_RCC_HSE_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_IsReady) for LL_RCC_PLL_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_IsReady) for LL_RCC_MSI_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource) for LL_RCC_GetSysClkSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to sys_app.o(i.HAL_InitTick) for HAL_InitTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32wlxx_hal.o(.data) for uwTickPrio
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_IsReady) for LL_RCC_MSI_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_SetCalibTrimming) for LL_RCC_MSI_SetCalibTrimming
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_SetCalibTrimming) for LL_RCC_HSI_SetCalibTrimming
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource) for LL_RCC_GetSysClkSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSE_IsReady) for LL_RCC_HSE_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_IsReady) for LL_RCC_PLL_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to sys_app.o(i.HAL_InitTick) for HAL_InitTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32wlxx_hal.o(.data) for uwTickPrio
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetClockConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource) for LL_RCC_GetSysClkSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLK3Freq) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLK3Freq) refers to system_stm32wlxx.o(.constdata) for AHBPrescTable
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) refers to system_stm32wlxx.o(.constdata) for AHBPrescTable
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetOscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_GetMainSource) for LL_RCC_PLL_GetMainSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to system_stm32wlxx.o(.constdata) for APBPrescTable
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to system_stm32wlxx.o(.constdata) for APBPrescTable
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource) for LL_RCC_GetSysClkSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_GetMainSource) for LL_RCC_PLL_GetMainSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) refers to system_stm32wlxx.o(.constdata) for MSIRangeTable
    stm32wlxx_hal_rcc.o(i.HAL_RCC_MCOConfig) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32wlxx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_CSSCallback) for HAL_RCC_CSSCallback
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource) for LL_RCC_GetSysClkSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_GetMainSource) for LL_RCC_PLL_GetMainSource
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_IsReady) for LL_RCC_MSI_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange) for RCC_SetFlashLatencyFromMSIRange
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_SetCalibTrimming) for LL_RCC_MSI_SetCalibTrimming
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to sys_app.o(i.HAL_InitTick) for HAL_InitTick
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSE_IsReady) for LL_RCC_HSE_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_IsReady) for LL_RCC_HSI_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_SetCalibTrimming) for LL_RCC_HSI_SetCalibTrimming
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess) for HAL_PWR_EnableBkUpAccess
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_IsReady) for LL_RCC_PLL_IsReady
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32wlxx_hal.o(.data) for uwTickPrio
    stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatency) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatency) refers to stm32wlxx_hal_rcc.o(.constdata) for .constdata
    stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_GetVoltageRange) for HAL_PWREx_GetVoltageRange
    stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange) refers to stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatency) for RCC_SetFlashLatency
    stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange) refers to system_stm32wlxx.o(.constdata) for MSIRangeTable
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_DisableLSCO) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess) for HAL_PWR_EnableBkUpAccess
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_DisableLSCO) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableBkUpAccess) for HAL_PWR_DisableBkUpAccess
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSCO) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSCO) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess) for HAL_PWR_EnableBkUpAccess
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSCO) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableBkUpAccess) for HAL_PWR_DisableBkUpAccess
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetUSARTClockSource) for LL_RCC_GetUSARTClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetI2CClockSource) for LL_RCC_GetI2CClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetLPTIMClockSource) for LL_RCC_GetLPTIMClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetLPTIMClockSource) for LL_RCC_GetLPTIMClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSE_IsReady) for LL_RCC_LSE_IsReady
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSI_GetPrediv) for LL_RCC_LSI_GetPrediv
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_IsEnabledRangeSelect) for LL_RCC_MSI_IsEnabledRangeSelect
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRangeAfterStandby) for LL_RCC_MSI_GetRangeAfterStandby
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q) for RCC_PLL_GetFreqDomain_Q
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRange) for LL_RCC_MSI_GetRange
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetUSARTClockSource) for LL_RCC_GetUSARTClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetAHBPrescaler) for LL_RCC_GetAHBPrescaler
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P) for RCC_PLL_GetFreqDomain_P
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetI2CClockSource) for LL_RCC_GetI2CClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetAPB1Prescaler) for LL_RCC_GetAPB1Prescaler
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSI_IsReady) for LL_RCC_LSI_IsReady
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_HSI_IsReady) for LL_RCC_HSI_IsReady
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to system_stm32wlxx.o(.constdata) for AHBPrescTable
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to system_stm32wlxx.o(.constdata) for APBPrescTable
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_LSECSS_IRQHandler) refers to stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_LSECSS_Callback) for HAL_RCCEx_LSECSS_Callback
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess) for HAL_PWR_EnableBkUpAccess
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSE_IsReady) for LL_RCC_LSE_IsReady
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetUSARTClockSource) for LL_RCC_SetUSARTClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetLPTIMClockSource) for LL_RCC_SetLPTIMClockSource
    stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetI2CClockSource) for LL_RCC_SetI2CClockSource
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_IsEnabledRangeSelect) for LL_RCC_MSI_IsEnabledRangeSelect
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRangeAfterStandby) for LL_RCC_MSI_GetRangeAfterStandby
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRange) for LL_RCC_MSI_GetRange
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P) refers to system_stm32wlxx.o(.constdata) for MSIRangeTable
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_IsEnabledRangeSelect) for LL_RCC_MSI_IsEnabledRangeSelect
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRangeAfterStandby) for LL_RCC_MSI_GetRangeAfterStandby
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q) refers to stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRange) for LL_RCC_MSI_GetRange
    stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q) refers to system_stm32wlxx.o(.constdata) for MSIRangeTable
    stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32wlxx_hal_flash.o(.bss) for .bss
    stm32wlxx_hal_flash.o(i.HAL_FLASH_GetError) refers to stm32wlxx_hal_flash.o(.bss) for .bss
    stm32wlxx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32wlxx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback) for HAL_FLASH_OperationErrorCallback
    stm32wlxx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32wlxx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32wlxx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback) for HAL_FLASH_EndOfOperationCallback
    stm32wlxx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32wlxx_hal_flash.o(.bss) for .bss
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32wlxx_hal_flash.o(i.FLASH_Program_Fast) for FLASH_Program_Fast
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32wlxx_hal_flash.o(i.FLASH_Program_DoubleWord) for FLASH_Program_DoubleWord
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32wlxx_hal_flash.o(.bss) for .bss
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32wlxx_hal_flash.o(i.FLASH_Program_Fast) for FLASH_Program_Fast
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32wlxx_hal_flash.o(i.FLASH_Program_DoubleWord) for FLASH_Program_DoubleWord
    stm32wlxx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32wlxx_hal_flash.o(.bss) for .bss
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32wlxx_hal_flash.o(.bss) for pFlash
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32wlxx_hal_flash.o(.bss) for pFlash
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetRDP) for FLASH_OB_GetRDP
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetUser) for FLASH_OB_GetUser
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetUser) for FLASH_OB_GetUser
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetRDP) for FLASH_OB_GetRDP
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32wlxx_hal_flash_ex.o(i.FLASH_OB_OptrConfig) for FLASH_OB_OptrConfig
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32wlxx_hal_flash.o(.bss) for pFlash
    stm32wlxx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler) refers to subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback) for HAL_GPIO_EXTI_Callback
    stm32wlxx_hal_dma.o(i.HAL_DMA_DeInit) refers to stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXChannelBaseAndMask) for DMA_CalcDMAMUXChannelBaseAndMask
    stm32wlxx_hal_dma.o(i.HAL_DMA_DeInit) refers to stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXRequestGenBaseAndMask) for DMA_CalcDMAMUXRequestGenBaseAndMask
    stm32wlxx_hal_dma.o(i.HAL_DMA_Init) refers to stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXChannelBaseAndMask) for DMA_CalcDMAMUXChannelBaseAndMask
    stm32wlxx_hal_dma.o(i.HAL_DMA_Init) refers to stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXRequestGenBaseAndMask) for DMA_CalcDMAMUXRequestGenBaseAndMask
    stm32wlxx_hal_dma.o(i.HAL_DMA_PollForTransfer) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_dma.o(i.HAL_DMA_Start) refers to stm32wlxx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32wlxx_hal_dma.o(i.HAL_DMA_Start_IT) refers to stm32wlxx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableLowPowerRunMode) for HAL_PWREx_EnableLowPowerRunMode
    stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableLowPowerRunMode) for HAL_PWREx_DisableLowPowerRunMode
    stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP0Mode) for HAL_PWREx_EnterSTOP0Mode
    stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP1Mode) for HAL_PWREx_EnterSTOP1Mode
    stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_ControlVoltageScaling) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableLowPowerRunMode) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_PVD_PVM_IRQHandler) refers to stm32wlxx_hal_pwr.o(i.HAL_PWR_PVDCallback) for HAL_PWR_PVDCallback
    stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_PVD_PVM_IRQHandler) refers to stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_PVM3Callback) for HAL_PWREx_PVM3Callback
    stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) refers to stm32wlxx_hal_cortex.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_Config) refers to stm32wlxx_hal_cortex.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler) refers to stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_Callback) for HAL_SYSTICK_Callback
    stm32wlxx_hal.o(i.HAL_DeInit) refers to stm32wlxx_hal.o(i.HAL_MspDeInit) for HAL_MspDeInit
    stm32wlxx_hal.o(i.HAL_Delay) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal.o(i.HAL_Delay) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_GetTick) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_GetTickFreq) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_GetTickPrio) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_IncTick) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping) for HAL_NVIC_SetPriorityGrouping
    stm32wlxx_hal.o(i.HAL_Init) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal.o(i.HAL_Init) refers to sys_app.o(i.HAL_InitTick) for HAL_InitTick
    stm32wlxx_hal.o(i.HAL_Init) refers to stm32wlxx_hal_msp.o(i.HAL_MspInit) for HAL_MspInit
    stm32wlxx_hal.o(i.HAL_Init) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal.o(i.HAL_InitTick) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32wlxx_hal.o(i.HAL_InitTick) refers to stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_Config) for HAL_SYSTICK_Config
    stm32wlxx_hal.o(i.HAL_InitTick) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    stm32wlxx_hal.o(i.HAL_InitTick) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal.o(i.HAL_SYSCFG_EnableVREFBUF) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal.o(i.HAL_SetTickFreq) refers to sys_app.o(i.HAL_InitTick) for HAL_InitTick
    stm32wlxx_hal.o(i.HAL_SetTickFreq) refers to stm32wlxx_hal.o(.data) for .data
    stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler) refers to timer_if.o(i.HAL_RTC_AlarmAEventCallback) for HAL_RTC_AlarmAEventCallback
    stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_AlarmBEventCallback) for HAL_RTCEx_AlarmBEventCallback
    stm32wlxx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_DeInit) refers to rtc.o(i.HAL_RTC_MspDeInit) for HAL_RTC_MspDeInit
    stm32wlxx_hal_rtc.o(i.HAL_RTC_GetAlarm) refers to stm32wlxx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32wlxx_hal_rtc.o(i.HAL_RTC_GetDate) refers to stm32wlxx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32wlxx_hal_rtc.o(i.HAL_RTC_GetTime) refers to stm32wlxx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32wlxx_hal_rtc.o(i.HAL_RTC_Init) refers to rtc.o(i.HAL_RTC_MspInit) for HAL_RTC_MspInit
    stm32wlxx_hal_rtc.o(i.HAL_RTC_Init) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_Init) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_PollForAlarmAEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm) refers to stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) refers to stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32wlxx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateRefClock) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateRefClock) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateWakeUpTimer) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_GetTimeStamp) refers to stm32wlxx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForAlarmBEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForInternalTamperEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamperEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTimeStampEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForWakeUpTimerEvent) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SSRUIRQHandler) refers to timer_if.o(i.HAL_RTCEx_SSRUEventCallback) for HAL_RTCEx_SSRUEventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetRefClock) refers to stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetRefClock) refers to stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode) for RTC_ExitInitMode
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSmoothCalib) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift) refers to stm32wlxx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer_IT) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper1EventCallback) for HAL_RTCEx_Tamper1EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper2EventCallback) for HAL_RTCEx_Tamper2EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper3EventCallback) for HAL_RTCEx_Tamper3EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper3EventCallback) for HAL_RTCEx_InternalTamper3EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper5EventCallback) for HAL_RTCEx_InternalTamper5EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper6EventCallback) for HAL_RTCEx_InternalTamper6EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper8EventCallback) for HAL_RTCEx_InternalTamper8EventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampEventCallback) for HAL_RTCEx_TimeStampEventCallback
    stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerIRQHandler) refers to stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerEventCallback) for HAL_RTCEx_WakeUpTimerEventCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_DeInit) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_DeInit) for SUBGHZSPI_DeInit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_DeInit) refers to subghz.o(i.HAL_SUBGHZ_MspDeInit) for HAL_SUBGHZ_MspDeInit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_DeInit) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SetRadioBusyTrigger) for LL_PWR_SetRadioBusyTrigger
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_DeInit) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive) for SUBGHZSPI_Receive
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) for HAL_SUBGHZ_ExecGetCmd
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_TxCpltCallback) for HAL_SUBGHZ_TxCpltCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_RxCpltCallback) for HAL_SUBGHZ_RxCpltCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_PreambleDetectedCallback) for HAL_SUBGHZ_PreambleDetectedCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_SyncWordValidCallback) for HAL_SUBGHZ_SyncWordValidCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_HeaderValidCallback) for HAL_SUBGHZ_HeaderValidCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_HeaderErrorCallback) for HAL_SUBGHZ_HeaderErrorCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_CRCErrorCallback) for HAL_SUBGHZ_CRCErrorCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_CADStatusCallback) for HAL_SUBGHZ_CADStatusCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to radio_driver.o(i.HAL_SUBGHZ_RxTxTimeoutCallback) for HAL_SUBGHZ_RxTxTimeoutCallback
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) for HAL_SUBGHZ_ExecSetCmd
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) refers to subghz.o(i.HAL_SUBGHZ_MspInit) for HAL_SUBGHZ_MspInit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SetRadioBusyTrigger) for LL_PWR_SetRadioBusyTrigger
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Init) for SUBGHZSPI_Init
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive) for SUBGHZSPI_Receive
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegister) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) for HAL_SUBGHZ_ReadRegisters
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive) for SUBGHZSPI_Receive
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegister) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) for HAL_SUBGHZ_WriteRegisters
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) for SUBGHZ_CheckDeviceReady
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) for SUBGHZSPI_Transmit
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS) for LL_PWR_SelectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) refers to stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS) for LL_PWR_UnselectSUBGHZSPI_NSS
    stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) refers to stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) for SUBGHZ_WaitOnBusy
    stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy) refers to system_stm32wlxx.o(.data) for SystemCoreClock
    stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to usart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32wlxx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_LIN_Init) refers to usart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32wlxx_hal_uart.o(i.HAL_LIN_Init) refers to stm32wlxx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32wlxx_hal_uart.o(i.HAL_LIN_Init) refers to stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32wlxx_hal_uart.o(i.HAL_LIN_Init) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_DisableMuteMode) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_EnableMuteMode) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to usart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32wlxx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback) for HAL_UART_AbortReceiveCpltCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32wlxx_hal_uart.o(i.UART_DMARxOnlyAbortCallback) for UART_DMARxOnlyAbortCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback) for HAL_UART_AbortTransmitCpltCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32wlxx_hal_uart.o(i.UART_DMATxOnlyAbortCallback) for UART_DMATxOnlyAbortCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32wlxx_hal_uart.o(i.UART_DMATxAbortCallback) for UART_DMATxAbortCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32wlxx_hal_uart.o(i.UART_DMARxAbortCallback) for UART_DMARxAbortCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32wlxx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32wlxx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32wlxx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32wlxx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32wlxx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32wlxx_hal_uart.o(i.HAL_UART_DeInit) refers to usart.o(i.HAL_UART_MspDeInit) for HAL_UART_MspDeInit
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_WakeupCallback) for HAL_UARTEx_WakeupCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to usart_if.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_TxFifoEmptyCallback) for HAL_UARTEx_TxFifoEmptyCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_RxFifoFullCallback) for HAL_UARTEx_RxFifoFullCallback
    stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32wlxx_hal_uart.o(i.UART_DMAAbortOnError) for UART_DMAAbortOnError
    stm32wlxx_hal_uart.o(i.HAL_UART_Init) refers to usart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32wlxx_hal_uart.o(i.HAL_UART_Init) refers to stm32wlxx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32wlxx_hal_uart.o(i.HAL_UART_Init) refers to stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32wlxx_hal_uart.o(i.HAL_UART_Init) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart.o(i.HAL_UART_Receive) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart.o(i.HAL_UART_Receive) refers to stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32wlxx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) for UART_Start_Receive_DMA
    stm32wlxx_hal_uart.o(i.HAL_UART_Receive_IT) refers to stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) for UART_Start_Receive_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit) refers to stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMATransmitCplt) for UART_DMATransmitCplt
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMATxHalfCplt) for UART_DMATxHalfCplt
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_IT) refers to stm32wlxx_hal_uart.o(i.UART_TxISR_8BIT) for UART_TxISR_8BIT
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_IT) refers to stm32wlxx_hal_uart.o(i.UART_TxISR_8BIT_FIFOEN) for UART_TxISR_8BIT_FIFOEN
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_IT) refers to stm32wlxx_hal_uart.o(i.UART_TxISR_16BIT_FIFOEN) for UART_TxISR_16BIT_FIFOEN
    stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_IT) refers to stm32wlxx_hal_uart.o(i.UART_TxISR_16BIT) for UART_TxISR_16BIT
    stm32wlxx_hal_uart.o(i.UART_CheckIdleState) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart.o(i.UART_CheckIdleState) refers to stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32wlxx_hal_uart.o(i.UART_DMAAbortOnError) refers to stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32wlxx_hal_uart.o(i.UART_DMAError) refers to stm32wlxx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32wlxx_hal_uart.o(i.UART_DMAError) refers to stm32wlxx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32wlxx_hal_uart.o(i.UART_DMAError) refers to stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32wlxx_hal_uart.o(i.UART_DMAReceiveCplt) refers to usart_if.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMAReceiveCplt) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_DMARxAbortCallback) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMARxHalfCplt) refers to stm32wlxx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback) for HAL_UART_RxHalfCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMARxHalfCplt) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_DMARxOnlyAbortCallback) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback) for HAL_UART_AbortReceiveCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMATransmitCplt) refers to usart_if.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMATxAbortCallback) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMATxHalfCplt) refers to stm32wlxx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback) for HAL_UART_TxHalfCpltCallback
    stm32wlxx_hal_uart.o(i.UART_DMATxOnlyAbortCallback) refers to stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback) for HAL_UART_AbortTransmitCpltCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT) refers to usart_if.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN) refers to usart_if.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT) for UART_RxISR_16BIT
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT) refers to usart_if.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN) refers to usart_if.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT) for UART_RxISR_8BIT
    stm32wlxx_hal_uart.o(i.UART_SetConfig) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32wlxx_hal_uart.o(i.UART_SetConfig) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32wlxx_hal_uart.o(i.UART_SetConfig) refers to lludivv7m.o(.text) for __aeabi_uldivmod
    stm32wlxx_hal_uart.o(i.UART_SetConfig) refers to stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32wlxx_hal_uart.o(i.UART_SetConfig) refers to stm32wlxx_hal_uart.o(.constdata) for .constdata
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32wlxx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMAReceiveCplt) for UART_DMAReceiveCplt
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMARxHalfCplt) for UART_DMARxHalfCplt
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32wlxx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN) for UART_RxISR_8BIT_FIFOEN
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN) for UART_RxISR_16BIT_FIFOEN
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT) for UART_RxISR_8BIT
    stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) refers to stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT) for UART_RxISR_16BIT
    stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart_ex.o(i.HAL_MultiProcessorEx_AddressLength_Set) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart_ex.o(i.HAL_RS485Ex_Init) refers to usart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32wlxx_hal_uart_ex.o(i.HAL_RS485Ex_Init) refers to stm32wlxx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32wlxx_hal_uart_ex.o(i.HAL_RS485Ex_Init) refers to stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32wlxx_hal_uart_ex.o(i.HAL_RS485Ex_Init) refers to stm32wlxx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableFifoMode) refers to stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess) for UARTEx_SetNbDataToProcess
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle_DMA) refers to stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA) for UART_Start_Receive_DMA
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle_IT) refers to stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT) for UART_Start_Receive_IT
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetRxFifoThreshold) refers to stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess) for UARTEx_SetNbDataToProcess
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetTxFifoThreshold) refers to stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess) for UARTEx_SetNbDataToProcess
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_StopModeWakeUpSourceConfig) refers to sys_app.o(i.HAL_GetTick) for HAL_GetTick
    stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_StopModeWakeUpSourceConfig) refers to stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess) refers to stm32wlxx_hal_uart_ex.o(.constdata) for .constdata
    system_stm32wlxx.o(i.SystemCoreClockUpdate) refers to system_stm32wlxx.o(.constdata) for .constdata
    system_stm32wlxx.o(i.SystemCoreClockUpdate) refers to system_stm32wlxx.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_CADStatusCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_CRCErrorCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_HeaderErrorCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_HeaderValidCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_PreambleDetectedCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_RxCpltCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_RxTxTimeoutCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_SyncWordValidCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.HAL_SUBGHZ_TxCpltCallback) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.Radio_SMPS_Set) refers to radio_board_if.o(i.RBI_IsDCDC) for RBI_IsDCDC
    radio_driver.o(i.Radio_SMPS_Set) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.Radio_SMPS_Set) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_Calibrate) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_CalibrateImage) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_ClearDeviceErrors) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_ClearIrqStatus) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_GetCFO) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.SUBGRF_GetDeviceErrors) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue) refers to radio_driver.o(.constdata) for .constdata
    radio_driver.o(i.SUBGRF_GetIrqStatus) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_GetOperatingMode) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_GetPacketStatus) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_GetPacketStatus) refers to stm32_mem.o(i.UTIL_MEM_set_8) for UTIL_MEM_set_8
    radio_driver.o(i.SUBGRF_GetPacketStatus) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_GetPacketType) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_GetPayload) refers to radio_driver.o(i.SUBGRF_GetRxBufferStatus) for SUBGRF_GetRxBufferStatus
    radio_driver.o(i.SUBGRF_GetPayload) refers to radio_driver.o(i.SUBGRF_ReadBuffer) for SUBGRF_ReadBuffer
    radio_driver.o(i.SUBGRF_GetRandom) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.SUBGRF_GetRandom) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_GetRandom) refers to radio_driver.o(i.SUBGRF_SetRx) for SUBGRF_SetRx
    radio_driver.o(i.SUBGRF_GetRandom) refers to radio_driver.o(i.SUBGRF_ReadRegisters) for SUBGRF_ReadRegisters
    radio_driver.o(i.SUBGRF_GetRandom) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio_driver.o(i.SUBGRF_GetRssiInst) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_GetRxBufferStatus) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_GetRxBufferStatus) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.SUBGRF_GetRxBufferStatus) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_GetStatus) refers to radio_driver.o(i.SUBGRF_ReadCommand) for SUBGRF_ReadCommand
    radio_driver.o(i.SUBGRF_Init) refers to subghz.o(i.MX_SUBGHZ_Init) for MX_SUBGHZ_Init
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(i.Radio_SMPS_Set) for Radio_SMPS_Set
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio_driver.o(i.SUBGRF_Init) refers to radio_board_if.o(i.RBI_IsTCXO) for RBI_IsTCXO
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_Init) refers to radio_board_if.o(i.RBI_Init) for RBI_Init
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(i.SUBGRF_SetTcxoMode) for SUBGRF_SetTcxoMode
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(i.SUBGRF_Calibrate) for SUBGRF_Calibrate
    radio_driver.o(i.SUBGRF_Init) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_ReadBuffer) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer) for HAL_SUBGHZ_ReadBuffer
    radio_driver.o(i.SUBGRF_ReadBuffer) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_ReadCommand) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd) for HAL_SUBGHZ_ExecGetCmd
    radio_driver.o(i.SUBGRF_ReadCommand) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_ReadRegister) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) for HAL_SUBGHZ_ReadRegisters
    radio_driver.o(i.SUBGRF_ReadRegister) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_ReadRegisters) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters) for HAL_SUBGHZ_ReadRegisters
    radio_driver.o(i.SUBGRF_ReadRegisters) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_SendPayload) refers to radio_driver.o(i.SUBGRF_SetPayload) for SUBGRF_SetPayload
    radio_driver.o(i.SUBGRF_SendPayload) refers to radio_driver.o(i.SUBGRF_SetTx) for SUBGRF_SetTx
    radio_driver.o(i.SUBGRF_SetBufferBaseAddress) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetCad) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetCad) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetCadParams) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetCadParams) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetCrcPolynomial) refers to radio_driver.o(i.SUBGRF_WriteRegisters) for SUBGRF_WriteRegisters
    radio_driver.o(i.SUBGRF_SetCrcPolynomial) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetCrcSeed) refers to radio_driver.o(i.SUBGRF_WriteRegisters) for SUBGRF_WriteRegisters
    radio_driver.o(i.SUBGRF_SetCrcSeed) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetDioIrqParams) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetFs) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetFs) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_SetModulationParams) refers to radio_driver.o(i.SUBGRF_SetPacketType) for SUBGRF_SetPacketType
    radio_driver.o(i.SUBGRF_SetModulationParams) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetModulationParams) refers to lludivv7m.o(.text) for __aeabi_uldivmod
    radio_driver.o(i.SUBGRF_SetModulationParams) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetPaConfig) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetPacketParams) refers to radio_driver.o(i.SUBGRF_SetPacketType) for SUBGRF_SetPacketType
    radio_driver.o(i.SUBGRF_SetPacketParams) refers to radio_driver.o(i.SUBGRF_SetCrcSeed) for SUBGRF_SetCrcSeed
    radio_driver.o(i.SUBGRF_SetPacketParams) refers to radio_driver.o(i.SUBGRF_SetCrcPolynomial) for SUBGRF_SetCrcPolynomial
    radio_driver.o(i.SUBGRF_SetPacketParams) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetPacketParams) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetPacketType) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_SetPacketType) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetPacketType) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetPayload) refers to radio_driver.o(i.SUBGRF_WriteBuffer) for SUBGRF_WriteBuffer
    radio_driver.o(i.SUBGRF_SetRegulatorMode) refers to radio_board_if.o(i.RBI_IsDCDC) for RBI_IsDCDC
    radio_driver.o(i.SUBGRF_SetRegulatorMode) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetRfFrequency) refers to radio_driver.o(i.SUBGRF_CalibrateImage) for SUBGRF_CalibrateImage
    radio_driver.o(i.SUBGRF_SetRfFrequency) refers to lludivv7m.o(.text) for __aeabi_uldivmod
    radio_driver.o(i.SUBGRF_SetRfFrequency) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetRfFrequency) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetRfTxPower) refers to radio_board_if.o(i.RBI_GetTxConfig) for RBI_GetTxConfig
    radio_driver.o(i.SUBGRF_SetRfTxPower) refers to radio_driver.o(i.SUBGRF_SetTxParams) for SUBGRF_SetTxParams
    radio_driver.o(i.SUBGRF_SetRx) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetRx) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetRxBoosted) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_SetRxBoosted) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetRxBoosted) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetRxDutyCycle) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetRxDutyCycle) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetRxTxFallbackMode) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetSleep) refers to radio_board_if.o(i.RBI_ConfigRFSwitch) for RBI_ConfigRFSwitch
    radio_driver.o(i.SUBGRF_SetSleep) refers to radio_driver.o(i.Radio_SMPS_Set) for Radio_SMPS_Set
    radio_driver.o(i.SUBGRF_SetSleep) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetSleep) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetStandby) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetStandby) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetStopRxTimerOnPreambleDetect) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetSwitch) refers to radio_driver.o(i.Radio_SMPS_Set) for Radio_SMPS_Set
    radio_driver.o(i.SUBGRF_SetSwitch) refers to radio_board_if.o(i.RBI_ConfigRFSwitch) for RBI_ConfigRFSwitch
    radio_driver.o(i.SUBGRF_SetSyncWord) refers to radio_driver.o(i.SUBGRF_WriteRegisters) for SUBGRF_WriteRegisters
    radio_driver.o(i.SUBGRF_SetTcxoMode) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetTx) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetTx) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_SetTxContinuousWave) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetTxInfinitePreamble) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetTxParams) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.SUBGRF_SetTxParams) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_SetTxParams) refers to radio_board_if.o(i.RBI_GetRFOMaxPowerConfig) for RBI_GetRFOMaxPowerConfig
    radio_driver.o(i.SUBGRF_SetTxParams) refers to radio_driver.o(i.SUBGRF_SetPaConfig) for SUBGRF_SetPaConfig
    radio_driver.o(i.SUBGRF_SetTxParams) refers to radio_driver.o(i.SUBGRF_WriteCommand) for SUBGRF_WriteCommand
    radio_driver.o(i.SUBGRF_SetWhiteningSeed) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio_driver.o(i.SUBGRF_SetWhiteningSeed) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio_driver.o(i.SUBGRF_SetWhiteningSeed) refers to radio_driver.o(.data) for .data
    radio_driver.o(i.SUBGRF_WriteBuffer) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer) for HAL_SUBGHZ_WriteBuffer
    radio_driver.o(i.SUBGRF_WriteBuffer) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_WriteCommand) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd) for HAL_SUBGHZ_ExecSetCmd
    radio_driver.o(i.SUBGRF_WriteCommand) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_WriteRegister) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) for HAL_SUBGHZ_WriteRegisters
    radio_driver.o(i.SUBGRF_WriteRegister) refers to subghz.o(.bss) for hsubghz
    radio_driver.o(i.SUBGRF_WriteRegisters) refers to stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters) for HAL_SUBGHZ_WriteRegisters
    radio_driver.o(i.SUBGRF_WriteRegisters) refers to subghz.o(.bss) for hsubghz
    radio.o(i.RadioGetStatus) refers to radio_driver.o(i.SUBGRF_GetOperatingMode) for SUBGRF_GetOperatingMode
    radio.o(i.RadioGetWakeupTime) refers to radio_driver.o(i.SUBGRF_GetRadioWakeUpTime) for SUBGRF_GetRadioWakeUpTime
    radio.o(i.RadioInit) refers to radio_driver.o(i.SUBGRF_Init) for SUBGRF_Init
    radio.o(i.RadioInit) refers to radio_driver.o(i.SUBGRF_SetRegulatorMode) for SUBGRF_SetRegulatorMode
    radio.o(i.RadioInit) refers to radio_driver.o(i.SUBGRF_SetBufferBaseAddress) for SUBGRF_SetBufferBaseAddress
    radio.o(i.RadioInit) refers to radio_driver.o(i.SUBGRF_SetTxParams) for SUBGRF_SetTxParams
    radio.o(i.RadioInit) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioInit) refers to radio.o(i.RadioSleep) for RadioSleep
    radio.o(i.RadioInit) refers to stm32_timer.o(i.UTIL_TIMER_Create) for UTIL_TIMER_Create
    radio.o(i.RadioInit) refers to stm32_timer.o(i.UTIL_TIMER_Stop) for UTIL_TIMER_Stop
    radio.o(i.RadioInit) refers to radio.o(.data) for .data
    radio.o(i.RadioInit) refers to radio.o(.bss) for .bss
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnDioIrq) for RadioOnDioIrq
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnTxTimeoutIrq) for RadioOnTxTimeoutIrq
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnRxTimeoutIrq) for RadioOnRxTimeoutIrq
    radio.o(i.RadioIrqProcess) refers to stm32_timer.o(i.UTIL_TIMER_Stop) for UTIL_TIMER_Stop
    radio.o(i.RadioIrqProcess) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_GetOperatingMode) for SUBGRF_GetOperatingMode
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioIrqProcess) refers to radio_fw.o(i.RFW_Is_LongPacketModeEnabled) for RFW_Is_LongPacketModeEnabled
    radio.o(i.RadioIrqProcess) refers to radio_fw.o(i.RFW_DeInit_TxLongPacket) for RFW_DeInit_TxLongPacket
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_GetPayload) for SUBGRF_GetPayload
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_GetPacketStatus) for SUBGRF_GetPacketStatus
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_GetCFO) for SUBGRF_GetCFO
    radio.o(i.RadioIrqProcess) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(i.RadioIrqProcess) refers to radio.o(i.RadioRead) for RadioRead
    radio.o(i.RadioIrqProcess) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioIrqProcess) refers to radio_fw.o(i.RFW_Is_Init) for RFW_Is_Init
    radio.o(i.RadioIrqProcess) refers to radio_fw.o(i.RFW_ReceivePayload) for RFW_ReceivePayload
    radio.o(i.RadioIrqProcess) refers to radio.o(.bss) for .bss
    radio.o(i.RadioIrqProcess) refers to radio.o(.data) for .data
    radio.o(i.RadioIsChannelFree) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioIsChannelFree) refers to radio_driver.o(i.SUBGRF_SetRfFrequency) for SUBGRF_SetRfFrequency
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioSetRxConfig) for RadioSetRxConfig
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioRx) for RadioRx
    radio.o(i.RadioIsChannelFree) refers to radio_driver.o(i.SUBGRF_GetRadioWakeUpTime) for SUBGRF_GetRadioWakeUpTime
    radio.o(i.RadioIsChannelFree) refers to sys_app.o(i.HAL_Delay) for HAL_Delay
    radio.o(i.RadioIsChannelFree) refers to stm32_timer.o(i.UTIL_TIMER_GetCurrentTime) for UTIL_TIMER_GetCurrentTime
    radio.o(i.RadioIsChannelFree) refers to radio_driver.o(i.SUBGRF_GetRssiInst) for SUBGRF_GetRssiInst
    radio.o(i.RadioIsChannelFree) refers to stm32_timer.o(i.UTIL_TIMER_GetElapsedTime) for UTIL_TIMER_GetElapsedTime
    radio.o(i.RadioOnDioIrq) refers to radio.o(i.RadioIrqProcess) for RadioIrqProcess
    radio.o(i.RadioOnDioIrq) refers to radio.o(.bss) for .bss
    radio.o(i.RadioOnRxTimeoutIrq) refers to radio.o(.data) for .data
    radio.o(i.RadioOnTxTimeoutIrq) refers to radio.o(.data) for .data
    radio.o(i.RadioRandom) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioRandom) refers to radio_driver.o(i.SUBGRF_GetRandom) for SUBGRF_GetRandom
    radio.o(i.RadioRead) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioReadRegisters) refers to radio_driver.o(i.SUBGRF_ReadRegisters) for SUBGRF_ReadRegisters
    radio.o(i.RadioRssi) refers to radio_driver.o(i.SUBGRF_GetRssiInst) for SUBGRF_GetRssiInst
    radio.o(i.RadioRx) refers to radio_fw.o(i.RFW_Is_Init) for RFW_Is_Init
    radio.o(i.RadioRx) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioRx) refers to stm32_timer.o(i.UTIL_TIMER_SetPeriod) for UTIL_TIMER_SetPeriod
    radio.o(i.RadioRx) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    radio.o(i.RadioRx) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioRx) refers to radio_driver.o(i.SUBGRF_SetRx) for SUBGRF_SetRx
    radio.o(i.RadioRx) refers to radio_fw.o(i.RFW_ReceiveInit) for RFW_ReceiveInit
    radio.o(i.RadioRx) refers to radio.o(.bss) for .bss
    radio.o(i.RadioRxBoosted) refers to radio_fw.o(i.RFW_Is_Init) for RFW_Is_Init
    radio.o(i.RadioRxBoosted) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioRxBoosted) refers to stm32_timer.o(i.UTIL_TIMER_SetPeriod) for UTIL_TIMER_SetPeriod
    radio.o(i.RadioRxBoosted) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    radio.o(i.RadioRxBoosted) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioRxBoosted) refers to radio_driver.o(i.SUBGRF_SetRxBoosted) for SUBGRF_SetRxBoosted
    radio.o(i.RadioRxBoosted) refers to radio_fw.o(i.RFW_ReceiveInit) for RFW_ReceiveInit
    radio.o(i.RadioRxBoosted) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioSend) refers to radio_fw.o(i.RFW_Is_Init) for RFW_Is_Init
    radio.o(i.RadioSend) refers to radio_fw.o(i.RFW_TransmitInit) for RFW_TransmitInit
    radio.o(i.RadioSend) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) for UTIL_ADV_TRACE_COND_FSend
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSend) refers to radio_driver.o(i.SUBGRF_SendPayload) for SUBGRF_SendPayload
    radio.o(i.RadioSend) refers to stm32_timer.o(i.UTIL_TIMER_SetPeriod) for UTIL_TIMER_SetPeriod
    radio.o(i.RadioSend) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    radio.o(i.RadioSend) refers to radio.o(i.payload_integration) for payload_integration
    radio.o(i.RadioSend) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(i.RadioSend) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetChannel) refers to radio_driver.o(i.SUBGRF_SetRfFrequency) for SUBGRF_SetRfFrequency
    radio.o(i.RadioSetMaxPayloadLength) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSetMaxPayloadLength) refers to radio.o(.data) for .data
    radio.o(i.RadioSetMaxPayloadLength) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetModem) refers to radio_fw.o(i.RFW_SetRadioModem) for RFW_SetRadioModem
    radio.o(i.RadioSetModem) refers to radio_driver.o(i.SUBGRF_SetPacketType) for SUBGRF_SetPacketType
    radio.o(i.RadioSetModem) refers to radio.o(i.RadioSetPublicNetwork) for RadioSetPublicNetwork
    radio.o(i.RadioSetModem) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetPublicNetwork) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetPublicNetwork) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioSetPublicNetwork) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetRxConfig) refers to radio_fw.o(i.RFW_DeInit) for RFW_DeInit
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetStopRxTimerOnPreambleDetect) for SUBGRF_SetStopRxTimerOnPreambleDetect
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue) for SUBGRF_GetFskBandwidthRegValue
    radio.o(i.RadioSetRxConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetModulationParams) for SUBGRF_SetModulationParams
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetSyncWord) for SUBGRF_SetSyncWord
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetWhiteningSeed) for SUBGRF_SetWhiteningSeed
    radio.o(i.RadioSetRxConfig) refers to radio.o(i.RadioRead) for RadioRead
    radio.o(i.RadioSetRxConfig) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout) for SUBGRF_SetLoRaSymbNumTimeout
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioSetRxConfig) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioSetRxConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetRxConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetRxConfig) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioSetRxDutyCycle) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioSetRxDutyCycle) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioSetRxDutyCycle) refers to radio_driver.o(i.SUBGRF_SetRxDutyCycle) for SUBGRF_SetRxDutyCycle
    radio.o(i.RadioSetRxDutyCycle) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetRxGenericConfig) refers to radio_fw.o(i.RFW_DeInit) for RFW_DeInit
    radio.o(i.RadioSetRxGenericConfig) refers to stm32_mem.o(i.UTIL_MEM_cpy_8) for UTIL_MEM_cpy_8
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetStopRxTimerOnPreambleDetect) for SUBGRF_SetStopRxTimerOnPreambleDetect
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue) for SUBGRF_GetFskBandwidthRegValue
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioSetRxGenericConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetModulationParams) for SUBGRF_SetModulationParams
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetSyncWord) for SUBGRF_SetSyncWord
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetWhiteningSeed) for SUBGRF_SetWhiteningSeed
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetCrcPolynomial) for SUBGRF_SetCrcPolynomial
    radio.o(i.RadioSetRxGenericConfig) refers to radio_fw.o(i.RFW_Init) for RFW_Init
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout) for SUBGRF_SetLoRaSymbNumTimeout
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioSetRxGenericConfig) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioSetRxGenericConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetRxGenericConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetTxConfig) refers to radio_fw.o(i.RFW_DeInit) for RFW_DeInit
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue) for SUBGRF_GetFskBandwidthRegValue
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioSetTxConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetModulationParams) for SUBGRF_SetModulationParams
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetSyncWord) for SUBGRF_SetSyncWord
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetWhiteningSeed) for SUBGRF_SetWhiteningSeed
    radio.o(i.RadioSetTxConfig) refers to radio_driver.o(i.SUBGRF_SetRfTxPower) for SUBGRF_SetRfTxPower
    radio.o(i.RadioSetTxConfig) refers to radio_fw.o(i.RFW_SetAntSwitch) for RFW_SetAntSwitch
    radio.o(i.RadioSetTxConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetTxConfig) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioSetTxConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetTxContinuousWave) refers to radio_driver.o(i.SUBGRF_SetRfFrequency) for SUBGRF_SetRfFrequency
    radio.o(i.RadioSetTxContinuousWave) refers to radio_driver.o(i.SUBGRF_SetRfTxPower) for SUBGRF_SetRfTxPower
    radio.o(i.RadioSetTxContinuousWave) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioSetTxContinuousWave) refers to radio_driver.o(i.SUBGRF_SetTxContinuousWave) for SUBGRF_SetTxContinuousWave
    radio.o(i.RadioSetTxContinuousWave) refers to stm32_timer.o(i.UTIL_TIMER_SetPeriod) for UTIL_TIMER_SetPeriod
    radio.o(i.RadioSetTxContinuousWave) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    radio.o(i.RadioSetTxContinuousWave) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetTxGenericConfig) refers to radio_fw.o(i.RFW_DeInit) for RFW_DeInit
    radio.o(i.RadioSetTxGenericConfig) refers to stm32_mem.o(i.UTIL_MEM_cpy_8) for UTIL_MEM_cpy_8
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioSetTxGenericConfig) refers to radio_fw.o(i.RFW_Init) for RFW_Init
    radio.o(i.RadioSetTxGenericConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetModulationParams) for SUBGRF_SetModulationParams
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetPacketParams) for SUBGRF_SetPacketParams
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetSyncWord) for SUBGRF_SetSyncWord
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetWhiteningSeed) for SUBGRF_SetWhiteningSeed
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetCrcPolynomial) for SUBGRF_SetCrcPolynomial
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_ReadRegister) for SUBGRF_ReadRegister
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioSetTxGenericConfig) refers to radio_driver.o(i.SUBGRF_SetRfTxPower) for SUBGRF_SetRfTxPower
    radio.o(i.RadioSetTxGenericConfig) refers to radio_fw.o(i.RFW_SetAntSwitch) for RFW_SetAntSwitch
    radio.o(i.RadioSetTxGenericConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetTxGenericConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSleep) refers to radio_driver.o(i.SUBGRF_SetSleep) for SUBGRF_SetSleep
    radio.o(i.RadioSleep) refers to sys_app.o(i.HAL_Delay) for HAL_Delay
    radio.o(i.RadioStandby) refers to radio_driver.o(i.SUBGRF_SetStandby) for SUBGRF_SetStandby
    radio.o(i.RadioStartCad) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioStartCad) refers to radio_driver.o(i.SUBGRF_SetDioIrqParams) for SUBGRF_SetDioIrqParams
    radio.o(i.RadioStartCad) refers to radio_driver.o(i.SUBGRF_SetCad) for SUBGRF_SetCad
    radio.o(i.RadioStartCad) refers to radio.o(.bss) for .bss
    radio.o(i.RadioTimeOnAir) refers to radio.o(i.RadioGetLoRaTimeOnAirNumerator) for RadioGetLoRaTimeOnAirNumerator
    radio.o(i.RadioTimeOnAir) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioTxCw) refers to radio_driver.o(i.SUBGRF_SetRfTxPower) for SUBGRF_SetRfTxPower
    radio.o(i.RadioTxCw) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioTxCw) refers to radio_driver.o(i.SUBGRF_SetTxContinuousWave) for SUBGRF_SetTxContinuousWave
    radio.o(i.RadioTxPrbs) refers to radio_driver.o(i.SUBGRF_SetSwitch) for SUBGRF_SetSwitch
    radio.o(i.RadioTxPrbs) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(i.RadioTxPrbs) refers to radio_driver.o(i.SUBGRF_SetTxInfinitePreamble) for SUBGRF_SetTxInfinitePreamble
    radio.o(i.RadioTxPrbs) refers to radio_driver.o(i.SUBGRF_SetTx) for SUBGRF_SetTx
    radio.o(i.RadioTxPrbs) refers to radio.o(.bss) for .bss
    radio.o(i.RadioWrite) refers to radio_driver.o(i.SUBGRF_WriteRegister) for SUBGRF_WriteRegister
    radio.o(i.RadioWriteRegisters) refers to radio_driver.o(i.SUBGRF_WriteRegisters) for SUBGRF_WriteRegisters
    radio.o(.constdata) refers to radio.o(i.RadioInit) for RadioInit
    radio.o(.constdata) refers to radio.o(i.RadioGetStatus) for RadioGetStatus
    radio.o(.constdata) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(.constdata) refers to radio.o(i.RadioSetChannel) for RadioSetChannel
    radio.o(.constdata) refers to radio.o(i.RadioIsChannelFree) for RadioIsChannelFree
    radio.o(.constdata) refers to radio.o(i.RadioRandom) for RadioRandom
    radio.o(.constdata) refers to radio.o(i.RadioSetRxConfig) for RadioSetRxConfig
    radio.o(.constdata) refers to radio.o(i.RadioSetTxConfig) for RadioSetTxConfig
    radio.o(.constdata) refers to radio.o(i.RadioCheckRfFrequency) for RadioCheckRfFrequency
    radio.o(.constdata) refers to radio.o(i.RadioTimeOnAir) for RadioTimeOnAir
    radio.o(.constdata) refers to radio.o(i.RadioSend) for RadioSend
    radio.o(.constdata) refers to radio.o(i.RadioSleep) for RadioSleep
    radio.o(.constdata) refers to radio.o(i.RadioStandby) for RadioStandby
    radio.o(.constdata) refers to radio.o(i.RadioRx) for RadioRx
    radio.o(.constdata) refers to radio.o(i.RadioStartCad) for RadioStartCad
    radio.o(.constdata) refers to radio.o(i.RadioSetTxContinuousWave) for RadioSetTxContinuousWave
    radio.o(.constdata) refers to radio.o(i.RadioRssi) for RadioRssi
    radio.o(.constdata) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(.constdata) refers to radio.o(i.RadioRead) for RadioRead
    radio.o(.constdata) refers to radio.o(i.RadioWriteRegisters) for RadioWriteRegisters
    radio.o(.constdata) refers to radio.o(i.RadioReadRegisters) for RadioReadRegisters
    radio.o(.constdata) refers to radio.o(i.RadioSetMaxPayloadLength) for RadioSetMaxPayloadLength
    radio.o(.constdata) refers to radio.o(i.RadioSetPublicNetwork) for RadioSetPublicNetwork
    radio.o(.constdata) refers to radio.o(i.RadioGetWakeupTime) for RadioGetWakeupTime
    radio.o(.constdata) refers to radio.o(i.RadioIrqProcess) for RadioIrqProcess
    radio.o(.constdata) refers to radio.o(i.RadioRxBoosted) for RadioRxBoosted
    radio.o(.constdata) refers to radio.o(i.RadioSetRxDutyCycle) for RadioSetRxDutyCycle
    radio.o(.constdata) refers to radio.o(i.RadioTxPrbs) for RadioTxPrbs
    radio.o(.constdata) refers to radio.o(i.RadioTxCw) for RadioTxCw
    radio.o(.constdata) refers to radio.o(i.RadioSetRxGenericConfig) for RadioSetRxGenericConfig
    radio.o(.constdata) refers to radio.o(i.RadioSetTxGenericConfig) for RadioSetTxGenericConfig
    radio.o(.constdata) refers to radio_fw.o(i.RFW_TransmitLongPacket) for RFW_TransmitLongPacket
    radio.o(.constdata) refers to radio_fw.o(i.RFW_ReceiveLongPacket) for RFW_ReceiveLongPacket
    stm32_adv_trace.o(i.TRACE_AllocateBufer) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.TRACE_Lock) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.TRACE_Send) refers to sys_app.o(i.UTIL_ADV_TRACE_PreSendHook) for UTIL_ADV_TRACE_PreSendHook
    stm32_adv_trace.o(i.TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.TRACE_Send) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.TRACE_Send) refers to usart_if.o(.constdata) for UTIL_TraceDriver
    stm32_adv_trace.o(i.TRACE_TxCpltCallback) refers to sys_app.o(i.UTIL_ADV_TRACE_PostSendHook) for UTIL_ADV_TRACE_PostSendHook
    stm32_adv_trace.o(i.TRACE_TxCpltCallback) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.TRACE_TxCpltCallback) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.TRACE_TxCpltCallback) refers to usart_if.o(.constdata) for UTIL_TraceDriver
    stm32_adv_trace.o(i.TRACE_UnLock) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like) for tiny_vsnprintf_like
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_adv_trace.o(i.TRACE_AllocateBufer) for TRACE_AllocateBufer
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_adv_trace.o(i.TRACE_Send) for TRACE_Send
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send) refers to stm32_adv_trace.o(i.TRACE_AllocateBufer) for TRACE_AllocateBufer
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send) refers to stm32_adv_trace.o(i.TRACE_Send) for TRACE_Send
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_AllocateBufer) for TRACE_AllocateBufer
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Allocation) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Finalize) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Finalize) for UTIL_ADV_TRACE_ZCSend_Finalize
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_DeInit) refers to usart_if.o(.constdata) for UTIL_TraceDriver
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_FSend) refers to stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like) for tiny_vsnprintf_like
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_FSend) refers to stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) for UTIL_ADV_TRACE_Send
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_GetRegion) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_GetVerboseLevel) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init) refers to stm32_mem.o(i.UTIL_MEM_set_8) for UTIL_MEM_set_8
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init) refers to usart_if.o(.constdata) for UTIL_TraceDriver
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init) refers to stm32_adv_trace.o(i.TRACE_TxCpltCallback) for TRACE_TxCpltCallback
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_IsBufferEmpty) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_RegisterTimeStampFunction) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ResetRegion) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_AllocateBufer) for TRACE_AllocateBufer
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) refers to stm32_adv_trace.o(i.TRACE_Send) for TRACE_Send
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetRegion) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetVerboseLevel) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_StartRxProcess) refers to usart_if.o(.constdata) for UTIL_TraceDriver
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_Lock) for TRACE_Lock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_AllocateBufer) for TRACE_AllocateBufer
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Allocation) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Allocation) refers to stm32_adv_trace.o(.bss) for .bss
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Finalize) refers to stm32_adv_trace.o(i.TRACE_UnLock) for TRACE_UnLock
    stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Finalize) refers to stm32_adv_trace.o(i.TRACE_Send) for TRACE_Send
    stm32_systime.o(i.CalendarGetMonth) refers to stm32_systime.o(i.CalendarDiv61) for CalendarDiv61
    stm32_systime.o(i.SysTimeFromMs) refers to stm32_systime.o(i.SysTimeAdd) for SysTimeAdd
    stm32_systime.o(i.SysTimeFromMs) refers to timer_if.o(.constdata) for UTIL_SYSTIMDriver
    stm32_systime.o(i.SysTimeGet) refers to stm32_systime.o(i.SysTimeAdd) for SysTimeAdd
    stm32_systime.o(i.SysTimeGet) refers to timer_if.o(.constdata) for UTIL_SYSTIMDriver
    stm32_systime.o(i.SysTimeGetMcuTime) refers to timer_if.o(.constdata) for UTIL_SYSTIMDriver
    stm32_systime.o(i.SysTimeLocalTime) refers to stm32_systime.o(i.CalendarDiv60) for CalendarDiv60
    stm32_systime.o(i.SysTimeLocalTime) refers to stm32_systime.o(i.CalendarGetMonth) for CalendarGetMonth
    stm32_systime.o(i.SysTimeLocalTime) refers to stm32_systime.o(.constdata) for .constdata
    stm32_systime.o(i.SysTimeMkTime) refers to stm32_systime.o(.constdata) for .constdata
    stm32_systime.o(i.SysTimeSet) refers to stm32_systime.o(i.SysTimeSub) for SysTimeSub
    stm32_systime.o(i.SysTimeSet) refers to timer_if.o(.constdata) for UTIL_SYSTIMDriver
    stm32_systime.o(i.SysTimeToMs) refers to stm32_systime.o(i.SysTimeSub) for SysTimeSub
    stm32_systime.o(i.SysTimeToMs) refers to timer_if.o(.constdata) for UTIL_SYSTIMDriver
    stm32_systime.o(.data) refers to stm32_systime.o(.conststring) for .conststring
    stm32_tiny_sscanf.o(i.tiny_sscanf) refers to stm32_tiny_sscanf.o(i.tiny_vfscanf) for tiny_vfscanf
    stm32_tiny_sscanf.o(i.tiny_vfscanf) refers to strlen.o(.text) for strlen
    stm32_tiny_vsnprintf.o(i.ee_number) refers to stm32_tiny_vsnprintf.o(.data) for .data
    stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like) refers to strlen.o(.text) for strlen
    stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like) refers to stm32_tiny_vsnprintf.o(i.ee_number) for ee_number
    stm32_tiny_vsnprintf.o(.data) refers to stm32_tiny_vsnprintf.o(.conststring) for .conststring
    stm32_seq.o(i.SEQ_BitPosition) refers to stm32_seq.o(.constdata) for .constdata
    stm32_seq.o(i.UTIL_SEQ_ClrEvt) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_EvtIdle) refers to stm32_seq.o(i.UTIL_SEQ_Run) for UTIL_SEQ_Run
    stm32_seq.o(i.UTIL_SEQ_Init) refers to stm32_mem.o(i.UTIL_MEM_set_8) for UTIL_MEM_set_8
    stm32_seq.o(i.UTIL_SEQ_Init) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_IsEvtPend) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_IsPauseTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_IsSchedulableTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_PauseTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_RegTask) refers to stm32_seq.o(i.SEQ_BitPosition) for SEQ_BitPosition
    stm32_seq.o(i.UTIL_SEQ_RegTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_ResumeTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_Run) refers to stm32_seq.o(i.SEQ_BitPosition) for SEQ_BitPosition
    stm32_seq.o(i.UTIL_SEQ_Run) refers to stm32_seq.o(i.UTIL_SEQ_PreIdle) for UTIL_SEQ_PreIdle
    stm32_seq.o(i.UTIL_SEQ_Run) refers to sys_app.o(i.UTIL_SEQ_Idle) for UTIL_SEQ_Idle
    stm32_seq.o(i.UTIL_SEQ_Run) refers to stm32_seq.o(i.UTIL_SEQ_PostIdle) for UTIL_SEQ_PostIdle
    stm32_seq.o(i.UTIL_SEQ_Run) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_SetEvt) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_SetTask) refers to stm32_seq.o(.data) for .data
    stm32_seq.o(i.UTIL_SEQ_WaitEvt) refers to stm32_seq.o(i.UTIL_SEQ_EvtIdle) for UTIL_SEQ_EvtIdle
    stm32_seq.o(i.UTIL_SEQ_WaitEvt) refers to stm32_seq.o(.data) for .data
    stm32_timer.o(i.TimerExists) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.TimerInsertNewHeadTimer) refers to stm32_timer.o(i.TimerSetTimeout) for TimerSetTimeout
    stm32_timer.o(i.TimerInsertNewHeadTimer) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.TimerInsertTimer) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.TimerSetTimeout) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_Create) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_DeInit) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_GetCurrentTime) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_GetElapsedTime) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_GetFirstRemainingTime) refers to stm32_timer.o(i.UTIL_TIMER_GetRemainingTime) for UTIL_TIMER_GetRemainingTime
    stm32_timer.o(i.UTIL_TIMER_GetFirstRemainingTime) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.UTIL_TIMER_GetRemainingTime) refers to stm32_timer.o(i.TimerExists) for TimerExists
    stm32_timer.o(i.UTIL_TIMER_GetRemainingTime) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_IRQ_Handler) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    stm32_timer.o(i.UTIL_TIMER_IRQ_Handler) refers to stm32_timer.o(i.TimerSetTimeout) for TimerSetTimeout
    stm32_timer.o(i.UTIL_TIMER_IRQ_Handler) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_IRQ_Handler) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.UTIL_TIMER_Init) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.UTIL_TIMER_Init) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_SetPeriod) refers to stm32_timer.o(i.TimerExists) for TimerExists
    stm32_timer.o(i.UTIL_TIMER_SetPeriod) refers to stm32_timer.o(i.UTIL_TIMER_Stop) for UTIL_TIMER_Stop
    stm32_timer.o(i.UTIL_TIMER_SetPeriod) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    stm32_timer.o(i.UTIL_TIMER_SetPeriod) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_Start) refers to stm32_timer.o(i.TimerExists) for TimerExists
    stm32_timer.o(i.UTIL_TIMER_Start) refers to stm32_timer.o(i.TimerInsertNewHeadTimer) for TimerInsertNewHeadTimer
    stm32_timer.o(i.UTIL_TIMER_Start) refers to stm32_timer.o(i.TimerInsertTimer) for TimerInsertTimer
    stm32_timer.o(i.UTIL_TIMER_Start) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_Start) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.UTIL_TIMER_StartWithPeriod) refers to stm32_timer.o(i.TimerExists) for TimerExists
    stm32_timer.o(i.UTIL_TIMER_StartWithPeriod) refers to stm32_timer.o(i.UTIL_TIMER_Stop) for UTIL_TIMER_Stop
    stm32_timer.o(i.UTIL_TIMER_StartWithPeriod) refers to stm32_timer.o(i.UTIL_TIMER_Start) for UTIL_TIMER_Start
    stm32_timer.o(i.UTIL_TIMER_StartWithPeriod) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_timer.o(i.UTIL_TIMER_Stop) refers to stm32_timer.o(i.TimerSetTimeout) for TimerSetTimeout
    stm32_timer.o(i.UTIL_TIMER_Stop) refers to stm32_timer.o(.data) for .data
    stm32_timer.o(i.UTIL_TIMER_Stop) refers to timer_if.o(.constdata) for UTIL_TimerDriver
    stm32_lpm.o(i.UTIL_LPM_EnterLowPower) refers to stm32_lpm.o(.data) for .data
    stm32_lpm.o(i.UTIL_LPM_EnterLowPower) refers to stm32_lpm_if.o(.constdata) for UTIL_PowerDriver
    stm32_lpm.o(i.UTIL_LPM_GetMode) refers to stm32_lpm.o(.data) for .data
    stm32_lpm.o(i.UTIL_LPM_Init) refers to stm32_lpm.o(.data) for .data
    stm32_lpm.o(i.UTIL_LPM_SetOffMode) refers to stm32_lpm.o(.data) for .data
    stm32_lpm.o(i.UTIL_LPM_SetStopMode) refers to stm32_lpm.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_DeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x.o(i.BSP_LED_DeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    stm32wlxx_lm40x.o(i.BSP_LED_DeInit) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_DeInit) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_GetState) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_ReadPin) for HAL_GPIO_ReadPin
    stm32wlxx_lm40x.o(i.BSP_LED_GetState) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_GetState) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to stm32wlxx_lm40x.o(i.LL_AHB2_GRP1_EnableClock) for LL_AHB2_GRP1_EnableClock
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_Init) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_Off) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x.o(i.BSP_LED_Off) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_Off) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_On) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x.o(i.BSP_LED_On) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_On) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_LED_Toggle) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_TogglePin) for HAL_GPIO_TogglePin
    stm32wlxx_lm40x.o(i.BSP_LED_Toggle) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_LED_Toggle) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_PB_DeInit) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    stm32wlxx_lm40x.o(i.BSP_PB_DeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    stm32wlxx_lm40x.o(i.BSP_PB_DeInit) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_PB_DeInit) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_PB_GetState) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_ReadPin) for HAL_GPIO_ReadPin
    stm32wlxx_lm40x.o(i.BSP_PB_GetState) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_PB_GetState) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_PB_IRQHandler) refers to stm32wlxx_hal_exti.o(i.HAL_EXTI_IRQHandler) for HAL_EXTI_IRQHandler
    stm32wlxx_lm40x.o(i.BSP_PB_IRQHandler) refers to stm32wlxx_lm40x.o(.bss) for .bss
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_lm40x.o(i.LL_AHB2_GRP1_EnableClock) for LL_AHB2_GRP1_EnableClock
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_hal_exti.o(i.HAL_EXTI_GetHandle) for HAL_EXTI_GetHandle
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_hal_exti.o(i.HAL_EXTI_RegisterCallback) for HAL_EXTI_RegisterCallback
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_lm40x.o(.constdata) for .constdata
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_lm40x.o(.data) for .data
    stm32wlxx_lm40x.o(i.BSP_PB_Init) refers to stm32wlxx_lm40x.o(.bss) for .bss
    stm32wlxx_lm40x.o(i.BUTTON_SW1_EXTI_Callback) refers to stm32wlxx_lm40x.o(i.BSP_PB_Callback) for BSP_PB_Callback
    stm32wlxx_lm40x.o(i.BUTTON_SW2_EXTI_Callback) refers to stm32wlxx_lm40x.o(i.BSP_PB_Callback) for BSP_PB_Callback
    stm32wlxx_lm40x.o(i.BUTTON_SW3_EXTI_Callback) refers to stm32wlxx_lm40x.o(i.BSP_PB_Callback) for BSP_PB_Callback
    stm32wlxx_lm40x.o(.data) refers to stm32wlxx_lm40x.o(i.BUTTON_SW1_EXTI_Callback) for BUTTON_SW1_EXTI_Callback
    stm32wlxx_lm40x.o(.data) refers to stm32wlxx_lm40x.o(i.BUTTON_SW2_EXTI_Callback) for BUTTON_SW2_EXTI_Callback
    stm32wlxx_lm40x.o(.data) refers to stm32wlxx_lm40x.o(i.BUTTON_SW3_EXTI_Callback) for BUTTON_SW3_EXTI_Callback
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_ConfigRFSwitch) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_DeInit) refers to stm32wlxx_lm40x_radio.o(i.LL_AHB2_GRP1_EnableClock) for LL_AHB2_GRP1_EnableClock
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_DeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_DeInit) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init) refers to rt_memclr_w.o(.text) for __aeabi_memclr4
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init) refers to stm32wlxx_lm40x_radio.o(i.LL_AHB2_GRP1_EnableClock) for LL_AHB2_GRP1_EnableClock
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init) refers to stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    rt_memcpy_v6.o(.text) refers to rt_memcpy_w.o(.text) for __aeabi_memcpy4
    rt_memclr.o(.text) refers to rt_memclr_w.o(.text) for _memset_w
    __main.o(!!!main) refers to __rtentry.o(.ARM.Collect$$rtentry$$00000000) for __rt_entry
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) for __rt_entry_li
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) for __rt_entry_main
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000C) for __rt_entry_postli_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$00000009) for __rt_entry_postsh_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$00000002) for __rt_entry_presh_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry4.o(.ARM.Collect$$rtentry$$00000004) for __rt_entry_sh
    aeabi_ldiv0_sigfpe.o(.text) refers to rt_div0.o(.text) for __rt_div0
    __rtentry2.o(.ARM.Collect$$rtentry$$00000008) refers to boardinit2.o(.text) for _platform_post_stackheap_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) refers to libinit.o(.ARM.Collect$$libinit$$00000000) for __rt_lib_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000B) refers to boardinit3.o(.text) for _platform_post_lib_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) refers to main.o(i.main) for main
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) refers to exit.o(.text) for exit
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$00000001) for .ARM.Collect$$rtentry$$00000001
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$00000008) for .ARM.Collect$$rtentry$$00000008
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) for .ARM.Collect$$rtentry$$0000000A
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000B) for .ARM.Collect$$rtentry$$0000000B
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) for .ARM.Collect$$rtentry$$0000000D
    __rtentry4.o(.ARM.Collect$$rtentry$$00000004) refers to sys_stackheap_outer.o(.text) for __user_setup_stackheap
    __rtentry4.o(.ARM.exidx) refers to __rtentry4.o(.ARM.Collect$$rtentry$$00000004) for .ARM.Collect$$rtentry$$00000004
    rt_div0.o(.text) refers to defsig_fpe_outer.o(.text) for __rt_SIGFPE
    sys_stackheap_outer.o(.text) refers to libspace.o(.text) for __user_perproc_libspace
    sys_stackheap_outer.o(.text) refers to startup_stm32wle5xx.o(.text) for __user_initial_stackheap
    exit.o(.text) refers to rtexit.o(.ARM.Collect$$rtexit$$00000000) for __rt_exit
    defsig_fpe_outer.o(.text) refers to defsig_fpe_inner.o(.text) for __rt_SIGFPE_inner
    defsig_fpe_outer.o(.text) refers to defsig_exit.o(.text) for __sig_exit
    defsig_fpe_formal.o(.text) refers to rt_raise.o(.text) for __rt_raise
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000002E) for __rt_lib_init_alloca_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000002C) for __rt_lib_init_argv_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001B) for __rt_lib_init_atexit_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000021) for __rt_lib_init_clock_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000032) for __rt_lib_init_cpp_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000030) for __rt_lib_init_exceptions_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000002) for __rt_lib_init_fp_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001F) for __rt_lib_init_fp_trap_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000023) for __rt_lib_init_getenv_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000A) for __rt_lib_init_heap_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000011) for __rt_lib_init_lc_collate_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000013) for __rt_lib_init_lc_ctype_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000015) for __rt_lib_init_lc_monetary_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000017) for __rt_lib_init_lc_numeric_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000019) for __rt_lib_init_lc_time_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000004) for __rt_lib_init_preinit_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000E) for __rt_lib_init_rand_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000033) for __rt_lib_init_return
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001D) for __rt_lib_init_signal_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000025) for __rt_lib_init_stdio_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000C) for __rt_lib_init_user_alloc_1
    libspace.o(.text) refers to libspace.o(.bss) for __libspace_start
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for __rt_exit_exit
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for __rt_exit_ls
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000002) for __rt_exit_prels_1
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for __rt_exit_exit
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for __rt_exit_ls
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000002) for __rt_exit_prels_1
    rtexit.o(.ARM.exidx) refers to rtexit.o(.ARM.Collect$$rtexit$$00000000) for .ARM.Collect$$rtexit$$00000000
    rt_raise.o(.text) refers to __raise.o(.text) for __raise
    rt_raise.o(.text) refers to sys_exit.o(.text) for _sys_exit
    defsig_exit.o(.text) refers to sys_exit.o(.text) for _sys_exit
    defsig_fpe_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    libinit2.o(.ARM.Collect$$libinit$$00000010) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000012) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000014) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000016) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000018) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000026) refers to argv_veneer.o(.emb_text) for __ARM_argv_veneer
    libinit2.o(.ARM.Collect$$libinit$$00000027) refers to argv_veneer.o(.emb_text) for __ARM_argv_veneer
    sys_exit.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_exit.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    rtexit2.o(.ARM.Collect$$rtexit$$00000003) refers to libshutdown.o(.ARM.Collect$$libshutdown$$00000000) for __rt_lib_shutdown
    rtexit2.o(.ARM.Collect$$rtexit$$00000004) refers to sys_exit.o(.text) for _sys_exit
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000001) for .ARM.Collect$$rtexit$$00000001
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for .ARM.Collect$$rtexit$$00000003
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for .ARM.Collect$$rtexit$$00000004
    __raise.o(.text) refers to defsig.o(CL$$defsig) for __default_signal_handler
    defsig_general.o(.text) refers to sys_wrch.o(.text) for _ttywrch
    argv_veneer.o(.emb_text) refers to no_argv.o(.text) for __ARM_get_argv
    sys_wrch.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_wrch.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    defsig.o(CL$$defsig) refers to defsig_fpe_inner.o(.text) for __rt_SIGFPE_inner
    defsig.o(CL$$defsig) refers to defsig_rtmem_inner.o(.text) for __rt_SIGRTMEM_inner
    _get_argv_nomalloc.o(.text) refers (Special) to hrguard.o(.text) for __heap_region$guard
    _get_argv_nomalloc.o(.text) refers to defsig_rtmem_outer.o(.text) for __rt_SIGRTMEM
    _get_argv_nomalloc.o(.text) refers to sys_command.o(.text) for _sys_command_string
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000006) for __rt_lib_shutdown_fp_trap_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E) for __rt_lib_shutdown_heap_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F) for __rt_lib_shutdown_return
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000009) for __rt_lib_shutdown_signal_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000003) for __rt_lib_shutdown_stdio_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B) for __rt_lib_shutdown_user_alloc_1
    sys_command.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_command.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    defsig_abrt_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtred_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtmem_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtmem_outer.o(.text) refers to defsig_rtmem_inner.o(.text) for __rt_SIGRTMEM_inner
    defsig_rtmem_outer.o(.text) refers to defsig_exit.o(.text) for __sig_exit
    defsig_rtmem_formal.o(.text) refers to rt_raise.o(.text) for __rt_raise
    defsig_stak_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_pvfn_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_cppl_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_segv_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_other.o(.text) refers to defsig_general.o(.text) for __default_signal_display


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing gpio.o(.rev16_text), (4 bytes).
    Removing gpio.o(.revsh_text), (4 bytes).
    Removing gpio.o(.rrx_text), (6 bytes).
    Removing dma.o(.rev16_text), (4 bytes).
    Removing dma.o(.revsh_text), (4 bytes).
    Removing dma.o(.rrx_text), (6 bytes).
    Removing rtc.o(.rev16_text), (4 bytes).
    Removing rtc.o(.revsh_text), (4 bytes).
    Removing rtc.o(.rrx_text), (6 bytes).
    Removing rtc.o(i.HAL_RTC_MspDeInit), (56 bytes).
    Removing subghz.o(.rev16_text), (4 bytes).
    Removing subghz.o(.revsh_text), (4 bytes).
    Removing subghz.o(.rrx_text), (6 bytes).
    Removing subghz.o(i.HAL_SUBGHZ_MspDeInit), (18 bytes).
    Removing stm32_lpm_if.o(.rev16_text), (4 bytes).
    Removing stm32_lpm_if.o(.revsh_text), (4 bytes).
    Removing stm32_lpm_if.o(.rrx_text), (6 bytes).
    Removing stm32_lpm_if.o(i.PWR_EnterOffMode), (2 bytes).
    Removing stm32_lpm_if.o(i.PWR_EnterSleepMode), (18 bytes).
    Removing stm32_lpm_if.o(i.PWR_EnterStopMode), (24 bytes).
    Removing stm32_lpm_if.o(i.PWR_ExitOffMode), (2 bytes).
    Removing stm32_lpm_if.o(i.PWR_ExitSleepMode), (4 bytes).
    Removing stm32_lpm_if.o(i.PWR_ExitStopMode), (14 bytes).
    Removing stm32_lpm_if.o(.constdata), (24 bytes).
    Removing sys_app.o(.rev16_text), (4 bytes).
    Removing sys_app.o(.revsh_text), (4 bytes).
    Removing sys_app.o(.rrx_text), (6 bytes).
    Removing sys_app.o(i.UTIL_SEQ_Idle), (4 bytes).
    Removing sys_debug.o(.rev16_text), (4 bytes).
    Removing sys_debug.o(.revsh_text), (4 bytes).
    Removing sys_debug.o(.rrx_text), (6 bytes).
    Removing sys_debug.o(i.DBG_Init), (18 bytes).
    Removing timer_if.o(.rev16_text), (4 bytes).
    Removing timer_if.o(.revsh_text), (4 bytes).
    Removing timer_if.o(.rrx_text), (6 bytes).
    Removing usart_if.o(.rev16_text), (4 bytes).
    Removing usart_if.o(.revsh_text), (4 bytes).
    Removing usart_if.o(.rrx_text), (6 bytes).
    Removing usart_if.o(i.vcom_Resume), (44 bytes).
    Removing usart_if.o(i.vcom_Trace), (20 bytes).
    Removing usart.o(.rev16_text), (4 bytes).
    Removing usart.o(.revsh_text), (4 bytes).
    Removing usart.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_it.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_it.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_it.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_msp.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_msp.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_msp.o(.rrx_text), (6 bytes).
    Removing app_subghz_phy.o(.rev16_text), (4 bytes).
    Removing app_subghz_phy.o(.revsh_text), (4 bytes).
    Removing app_subghz_phy.o(.rrx_text), (6 bytes).
    Removing app_subghz_phy.o(i.MX_SubGHz_Phy_Process), (8 bytes).
    Removing subghz_phy_app.o(.rev16_text), (4 bytes).
    Removing subghz_phy_app.o(.revsh_text), (4 bytes).
    Removing subghz_phy_app.o(.rrx_text), (6 bytes).
    Removing radio_board_if.o(.rev16_text), (4 bytes).
    Removing radio_board_if.o(.revsh_text), (4 bytes).
    Removing radio_board_if.o(.rrx_text), (6 bytes).
    Removing radio_board_if.o(i.RBI_DeInit), (4 bytes).
    Removing stm32wlxx_hal_rcc.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_rcc.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_rcc.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_CSSCallback), (2 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_DeInit), (236 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_EnableCSS), (14 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_GetClockConfig), (76 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLK3Freq), (36 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_GetOscConfig), (258 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_GetResetSource), (22 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_MCOConfig), (80 bytes).
    Removing stm32wlxx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler), (24 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_DisableLSCO), (52 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_DisableLSECSS), (26 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_DisableMSIPLLMode), (14 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSCO), (104 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSECSS), (16 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableLSECSS_IT), (40 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_EnableMSIPLLMode), (14 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig), (136 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq), (728 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_LSECSS_Callback), (2 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_LSECSS_IRQHandler), (18 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_WakeUpStopCLKConfig), (16 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetAHBPrescaler), (12 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetAPB1Prescaler), (12 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetI2CClockSource), (18 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetLPTIMClockSource), (16 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_GetUSARTClockSource), (16 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_HSI_IsReady), (12 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSI_GetPrediv), (14 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSI_IsReady), (14 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRange), (12 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_GetRangeAfterStandby), (14 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.LL_RCC_MSI_IsEnabledRangeSelect), (12 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_P), (160 bytes).
    Removing stm32wlxx_hal_rcc_ex.o(i.RCC_PLL_GetFreqDomain_Q), (160 bytes).
    Removing stm32wlxx_hal_flash.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_flash.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_flash.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_flash.o(i.FLASH_Program_DoubleWord), (28 bytes).
    Removing stm32wlxx_hal_flash.o(i.FLASH_Program_Fast), (52 bytes).
    Removing stm32wlxx_hal_flash.o(i.FLASH_WaitForLastOperation), (108 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback), (2 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_GetError), (12 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_IRQHandler), (164 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_Lock), (28 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_OB_Launch), (20 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_OB_Lock), (28 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_OB_Unlock), (40 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback), (2 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_Program), (100 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_Program_IT), (116 bytes).
    Removing stm32wlxx_hal_flash.o(i.HAL_FLASH_Unlock), (40 bytes).
    Removing stm32wlxx_hal_flash.o(.bss), (24 bytes).
    Removing stm32wlxx_hal_flash_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_flash_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_flash_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.FLASH_MassErase), (20 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetRDP), (24 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.FLASH_OB_GetUser), (24 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.FLASH_OB_OptrConfig), (24 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.FLASH_PageErase), (28 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_AllowOperation), (16 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase), (148 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT), (100 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_FlashEmptyCheck), (16 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_ForceFlashEmpty), (20 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_IsOperationSuspended), (20 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig), (132 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram), (248 bytes).
    Removing stm32wlxx_hal_flash_ex.o(i.HAL_FLASHEx_SuspendOperation), (16 bytes).
    Removing stm32wlxx_hal_gpio.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_gpio.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_gpio.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback), (2 bytes).
    Removing stm32wlxx_hal_gpio.o(i.HAL_GPIO_LockPin), (34 bytes).
    Removing stm32wlxx_hal_gpio.o(i.HAL_GPIO_ReadPin), (10 bytes).
    Removing stm32wlxx_hal_gpio.o(i.HAL_GPIO_WriteMultipleStatePin), (8 bytes).
    Removing stm32wlxx_hal_dma.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_dma.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_dma.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_GetError), (4 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_GetState), (6 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_PollForTransfer), (270 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_RegisterCallback), (74 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_Start), (84 bytes).
    Removing stm32wlxx_hal_dma.o(i.HAL_DMA_UnRegisterCallback), (82 bytes).
    Removing stm32wlxx_hal_dma_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_dma_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_dma_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_dma_ex.o(i.HAL_DMAEx_ConfigMuxRequestGenerator), (80 bytes).
    Removing stm32wlxx_hal_dma_ex.o(i.HAL_DMAEx_ConfigMuxSync), (88 bytes).
    Removing stm32wlxx_hal_dma_ex.o(i.HAL_DMAEx_DisableMuxRequestGenerator), (26 bytes).
    Removing stm32wlxx_hal_dma_ex.o(i.HAL_DMAEx_EnableMuxRequestGenerator), (26 bytes).
    Removing stm32wlxx_hal_dma_ex.o(i.HAL_DMAEx_MUX_IRQHandler), (100 bytes).
    Removing stm32wlxx_hal_pwr.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_pwr.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_pwr.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_ConfigPVD), (104 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DeInit), (92 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableBkUpAccess), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DisablePVD), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableSEVOnPend), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableSleepOnExit), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_DisableWakeUpPin), (20 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnablePVD), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableSEVOnPend), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableSleepOnExit), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableWakeUpPin), (32 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode), (72 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSTANDBYMode), (36 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode), (16 bytes).
    Removing stm32wlxx_hal_pwr.o(i.HAL_PWR_PVDCallback), (2 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_ConfigPVM), (108 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_ControlVoltageScaling), (104 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableBORPVD_ULP), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableBatteryCharging), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableFlashPowerDown), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableGPIOPullDown), (72 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableGPIOPullUp), (72 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableInternalWakeUpLine), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableLowPowerRunMode), (68 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisablePVM3), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisablePullUpPullDownConfig), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableSRAMRetention), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_DisableWPVD), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableBORPVD_ULP), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableBatteryCharging), (28 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableFlashPowerDown), (24 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableGPIOPullDown), (104 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableGPIOPullUp), (104 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableInternalWakeUpLine), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableLowPowerRunMode), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnablePVM3), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnablePullUpPullDownConfig), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableSRAMRetention), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnableWPVD), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSHUTDOWNMode), (32 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP0Mode), (52 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP1Mode), (56 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_EnterSTOP2Mode), (56 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_PVD_PVM_IRQHandler), (48 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_PVM3Callback), (2 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SMPS_GetEffectiveMode), (16 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SMPS_SetMode), (20 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SetRadioBusyPolarity), (20 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SetRadioBusyTrigger), (20 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SetRadioEOL), (20 bytes).
    Removing stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_SetRadioIRQTrigger), (20 bytes).
    Removing stm32wlxx_hal_cortex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_cortex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_cortex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_MPU_ConfigRegion), (84 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_MPU_Disable), (16 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_MPU_Enable), (24 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_ClearPendingIRQ), (26 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_GetActive), (36 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_GetPendingIRQ), (36 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_GetPriority), (84 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_GetPriorityGrouping), (16 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPendingIRQ), (26 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_NVIC_SystemReset), (36 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig), (24 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_Callback), (2 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_Config), (40 bytes).
    Removing stm32wlxx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler), (8 bytes).
    Removing stm32wlxx_hal.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGSleepMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGStandbyMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_DisableDBGStopMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_EnableDBGSleepMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_EnableDBGStandbyMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DBGMCU_EnableDBGStopMode), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_DeInit), (76 bytes).
    Removing stm32wlxx_hal.o(i.HAL_Delay), (36 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetDEVID), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetHalVersion), (6 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetREVID), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetTick), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetTickFreq), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetTickPrio), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetUIDw0), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetUIDw1), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_GetUIDw2), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_IncTick), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_InitTick), (64 bytes).
    Removing stm32wlxx_hal.o(i.HAL_MspDeInit), (2 bytes).
    Removing stm32wlxx_hal.o(i.HAL_MspInit), (2 bytes).
    Removing stm32wlxx_hal.o(i.HAL_ResumeTick), (14 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_DisableIOAnalogSwitchBooster), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_DisableVREFBUF), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_EnableIOAnalogSwitchBooster), (16 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_EnableVREFBUF), (48 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_SRAM2Erase), (24 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_VREFBUF_HighImpedanceConfig), (20 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_VREFBUF_TrimmingConfig), (12 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SYSCFG_VREFBUF_VoltageScalingConfig), (40 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SetTickFreq), (36 bytes).
    Removing stm32wlxx_hal.o(i.HAL_SuspendTick), (14 bytes).
    Removing stm32wlxx_hal_exti.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_exti.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_exti.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_ClearConfigLine), (128 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_ClearPending), (28 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_GenerateSWI), (28 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_GetConfigLine), (164 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_GetPending), (32 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_IRQHandler), (44 bytes).
    Removing stm32wlxx_hal_exti.o(i.HAL_EXTI_SetConfigLine), (176 bytes).
    Removing stm32wlxx_hal_rtc.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_rtc.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_rtc.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmAEventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DST_Add1Hour), (32 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DST_ClearStoreOperation), (32 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DST_ReadStoreOperation), (16 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DST_SetStoreOperation), (32 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DST_Sub1Hour), (32 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_DeInit), (176 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_GetAlarm), (140 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_GetDate), (72 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_GetState), (6 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_GetTime), (104 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_MspDeInit), (2 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_MspInit), (2 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_PollForAlarmAEvent), (72 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm), (368 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_SetDate), (168 bytes).
    Removing stm32wlxx_hal_rtc.o(i.HAL_RTC_SetTime), (220 bytes).
    Removing stm32wlxx_hal_rtc.o(i.RTC_Bcd2ToByte), (18 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateCalibrationOutPut), (64 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateInternalTamper), (32 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateInternalTimeStamp), (100 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateRefClock), (88 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateSSRU), (72 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateTamper), (48 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateTimeStamp), (92 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateWakeUpTimer), (140 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_DisableBypassShadow), (64 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_GetTimeStamp), (164 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_GetWakeUpTimer), (12 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper3EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper5EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper6EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_InternalTamper8EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_MonotonicCounterGet), (16 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_MonotonicCounterIncrement), (12 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForAlarmBEvent), (72 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForInternalTamperEvent), (56 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamperEvent), (56 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTimeStampEvent), (88 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_PollForWakeUpTimerEvent), (72 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SSRUEventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetCalibrationOutPut), (76 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetInternalTamper), (88 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetInternalTamper_IT), (112 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetInternalTimeStamp), (64 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetLowPowerCalib), (64 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetRefClock), (88 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSmoothCalib), (156 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift), (196 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetTamper), (136 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetTamper_IT), (156 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetTimeStamp), (76 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetTimeStamp_IT), (96 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer), (172 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer_IT), (220 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper1EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper2EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper3EventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TamperIRQHandler), (92 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampEventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampIRQHandler), (40 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerEventCallback), (2 bytes).
    Removing stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerIRQHandler), (40 bytes).
    Removing stm32wlxx_hal_subghz.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_subghz.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_subghz.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_CADStatusCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_CRCErrorCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_DeInit), (136 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_GetError), (4 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_GetState), (4 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_HeaderErrorCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_HeaderValidCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_MspDeInit), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_MspInit), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_PreambleDetectedCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegister), (6 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_RxCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_RxTxTimeoutCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_SyncWordValidCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_TxCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegister), (12 bytes).
    Removing stm32wlxx_hal_subghz.o(i.SUBGHZSPI_DeInit), (16 bytes).
    Removing stm32wlxx_hal_tim.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_tim.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_tim.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_tim_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_tim_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_tim_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_uart.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_uart.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_uart.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_EnableReceiver), (76 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_EnableTransmitter), (76 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_HalfDuplex_Init), (116 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_LIN_Init), (140 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_LIN_SendBreak), (46 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_DisableMuteMode), (52 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_EnableMuteMode), (52 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_EnterMuteMode), (12 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_MultiProcessor_Init), (138 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Abort), (252 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive), (168 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortReceive_IT), (184 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit), (140 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_AbortTransmit_IT), (148 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Abort_IT), (288 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_DMAPause), (142 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_DMAResume), (134 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_DMAStop), (144 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_DeInit), (68 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_DisableReceiverTimeout), (68 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_EnableReceiverTimeout), (68 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_GetError), (6 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_GetState), (10 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_MspDeInit), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_MspInit), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Receive), (244 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Receive_DMA), (84 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_ReceiverTimeout_Config), (24 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_RxCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Transmit), (188 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_IT), (172 bytes).
    Removing stm32wlxx_hal_uart.o(i.HAL_UART_TxCpltCallback), (2 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMAReceiveCplt), (130 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMARxAbortCallback), (66 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMARxHalfCplt), (28 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMARxOnlyAbortCallback), (40 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMATxAbortCallback), (74 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_DMATxOnlyAbortCallback), (40 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_Start_Receive_DMA), (164 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_TxISR_16BIT), (82 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_TxISR_16BIT_FIFOEN), (104 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_TxISR_8BIT), (78 bytes).
    Removing stm32wlxx_hal_uart.o(i.UART_TxISR_8BIT_FIFOEN), (100 bytes).
    Removing stm32wlxx_hal_uart_ex.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_hal_uart_ex.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_hal_uart_ex.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_MultiProcessorEx_AddressLength_Set), (48 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_RS485Ex_Init), (140 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_DisableFifoMode), (62 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_DisableStopMode), (46 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle), (310 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle_DMA), (90 bytes).
    Removing stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_ReceiveToIdle_IT), (90 bytes).
    Removing system_stm32wlxx.o(.rev16_text), (4 bytes).
    Removing system_stm32wlxx.o(.revsh_text), (4 bytes).
    Removing system_stm32wlxx.o(.rrx_text), (6 bytes).
    Removing system_stm32wlxx.o(i.SystemCoreClockUpdate), (172 bytes).
    Removing radio_driver.o(.rev16_text), (4 bytes).
    Removing radio_driver.o(.revsh_text), (4 bytes).
    Removing radio_driver.o(.rrx_text), (6 bytes).
    Removing radio_driver.o(i.SUBGRF_ClearDeviceErrors), (18 bytes).
    Removing radio_driver.o(i.SUBGRF_ClearIrqStatus), (24 bytes).
    Removing radio_driver.o(i.SUBGRF_GetDeviceErrors), (88 bytes).
    Removing radio_driver.o(i.SUBGRF_GetIrqStatus), (20 bytes).
    Removing radio_driver.o(i.SUBGRF_GetPacketType), (12 bytes).
    Removing radio_driver.o(i.SUBGRF_GetStatus), (38 bytes).
    Removing radio_driver.o(i.SUBGRF_SetCadParams), (60 bytes).
    Removing radio_driver.o(i.SUBGRF_SetFs), (24 bytes).
    Removing radio_driver.o(i.SUBGRF_SetRxTxFallbackMode), (14 bytes).
    Removing radio_fw.o(.rev16_text), (4 bytes).
    Removing radio_fw.o(.revsh_text), (4 bytes).
    Removing radio_fw.o(.rrx_text), (6 bytes).
    Removing radio.o(.rev16_text), (4 bytes).
    Removing radio.o(.revsh_text), (4 bytes).
    Removing radio.o(.rrx_text), (6 bytes).
    Removing stm32_adv_trace.o(.rev16_text), (4 bytes).
    Removing stm32_adv_trace.o(.revsh_text), (4 bytes).
    Removing stm32_adv_trace.o(.rrx_text), (6 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_Send), (168 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Allocation), (164 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_ZCSend_Finalize), (4 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_DeInit), (12 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_FSend), (34 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_GetRegion), (12 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_GetVerboseLevel), (12 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_IsBufferEmpty), (24 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_PostSendHook), (2 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_PreSendHook), (2 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_ResetRegion), (16 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_Send), (76 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetRegion), (16 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_StartRxProcess), (12 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Allocation), (68 bytes).
    Removing stm32_adv_trace.o(i.UTIL_ADV_TRACE_ZCSend_Finalize), (14 bytes).
    Removing stm32_mem.o(.rev16_text), (4 bytes).
    Removing stm32_mem.o(.revsh_text), (4 bytes).
    Removing stm32_mem.o(.rrx_text), (6 bytes).
    Removing stm32_mem.o(i.UTIL_MEM_cpyr_8), (22 bytes).
    Removing stm32_systime.o(i.CalendarDiv60), (40 bytes).
    Removing stm32_systime.o(i.CalendarDiv61), (40 bytes).
    Removing stm32_systime.o(i.CalendarGetMonth), (68 bytes).
    Removing stm32_systime.o(i.SysTimeFromMs), (68 bytes).
    Removing stm32_systime.o(i.SysTimeGetMcuTime), (32 bytes).
    Removing stm32_systime.o(i.SysTimeLocalTime), (244 bytes).
    Removing stm32_systime.o(i.SysTimeMkTime), (116 bytes).
    Removing stm32_systime.o(i.SysTimeSet), (64 bytes).
    Removing stm32_systime.o(i.SysTimeSub), (36 bytes).
    Removing stm32_systime.o(i.SysTimeToMs), (60 bytes).
    Removing stm32_systime.o(.constdata), (32 bytes).
    Removing stm32_systime.o(.conststring), (28 bytes).
    Removing stm32_systime.o(.data), (28 bytes).
    Removing stm32_tiny_sscanf.o(i.tiny_sscanf), (18 bytes).
    Removing stm32_tiny_sscanf.o(i.tiny_vfscanf), (506 bytes).
    Removing stm32_seq.o(.rev16_text), (4 bytes).
    Removing stm32_seq.o(.revsh_text), (4 bytes).
    Removing stm32_seq.o(.rrx_text), (6 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_ClrEvt), (24 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_DeInit), (2 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_EvtIdle), (6 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_Idle), (2 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_Init), (56 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_IsEvtPend), (16 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_IsPauseTask), (28 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_IsSchedulableTask), (40 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_PauseTask), (24 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_PostIdle), (2 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_PreIdle), (2 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_ResumeTask), (24 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_Run), (212 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_SetEvt), (24 bytes).
    Removing stm32_seq.o(i.UTIL_SEQ_WaitEvt), (76 bytes).
    Removing stm32_timer.o(.rev16_text), (4 bytes).
    Removing stm32_timer.o(.revsh_text), (4 bytes).
    Removing stm32_timer.o(.rrx_text), (6 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_DeInit), (12 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_GetFirstRemainingTime), (28 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_GetRemainingTime), (48 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_IsRunning), (8 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_SetReloadMode), (16 bytes).
    Removing stm32_timer.o(i.UTIL_TIMER_StartWithPeriod), (48 bytes).
    Removing stm32_lpm.o(.rev16_text), (4 bytes).
    Removing stm32_lpm.o(.revsh_text), (4 bytes).
    Removing stm32_lpm.o(.rrx_text), (6 bytes).
    Removing stm32_lpm.o(i.UTIL_LPM_DeInit), (2 bytes).
    Removing stm32_lpm.o(i.UTIL_LPM_EnterLowPower), (60 bytes).
    Removing stm32_lpm.o(i.UTIL_LPM_GetMode), (36 bytes).
    Removing stm32wlxx_lm40x.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_lm40x.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_lm40x.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_GetVersion), (8 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_LED_DeInit), (48 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_LED_GetState), (24 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_LED_Off), (32 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_LED_On), (32 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_PB_DeInit), (44 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_PB_GetState), (24 bytes).
    Removing stm32wlxx_lm40x.o(i.BSP_PB_IRQHandler), (16 bytes).
    Removing stm32wlxx_lm40x_radio.o(.rev16_text), (4 bytes).
    Removing stm32wlxx_lm40x_radio.o(.revsh_text), (4 bytes).
    Removing stm32wlxx_lm40x_radio.o(.rrx_text), (6 bytes).
    Removing stm32wlxx_lm40x_radio.o(i.BSP_RADIO_DeInit), (56 bytes).

544 unused section(s) (total 22638 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../Core/Src/dma.c                        0x00000000   Number         0  dma.o ABSOLUTE
    ../Core/Src/gpio.c                       0x00000000   Number         0  gpio.o ABSOLUTE
    ../Core/Src/main.c                       0x00000000   Number         0  main.o ABSOLUTE
    ../Core/Src/rtc.c                        0x00000000   Number         0  rtc.o ABSOLUTE
    ../Core/Src/stm32_lpm_if.c               0x00000000   Number         0  stm32_lpm_if.o ABSOLUTE
    ../Core/Src/stm32wlxx_hal_msp.c          0x00000000   Number         0  stm32wlxx_hal_msp.o ABSOLUTE
    ../Core/Src/stm32wlxx_it.c               0x00000000   Number         0  stm32wlxx_it.o ABSOLUTE
    ../Core/Src/subghz.c                     0x00000000   Number         0  subghz.o ABSOLUTE
    ../Core/Src/sys_app.c                    0x00000000   Number         0  sys_app.o ABSOLUTE
    ../Core/Src/sys_debug.c                  0x00000000   Number         0  sys_debug.o ABSOLUTE
    ../Core/Src/system_stm32wlxx.c           0x00000000   Number         0  system_stm32wlxx.o ABSOLUTE
    ../Core/Src/timer_if.c                   0x00000000   Number         0  timer_if.o ABSOLUTE
    ../Core/Src/usart.c                      0x00000000   Number         0  usart.o ABSOLUTE
    ../Core/Src/usart_if.c                   0x00000000   Number         0  usart_if.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal.c 0x00000000   Number         0  stm32wlxx_hal.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_cortex.c 0x00000000   Number         0  stm32wlxx_hal_cortex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_dma.c 0x00000000   Number         0  stm32wlxx_hal_dma.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_dma_ex.c 0x00000000   Number         0  stm32wlxx_hal_dma_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_exti.c 0x00000000   Number         0  stm32wlxx_hal_exti.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_flash.c 0x00000000   Number         0  stm32wlxx_hal_flash.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_flash_ex.c 0x00000000   Number         0  stm32wlxx_hal_flash_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_gpio.c 0x00000000   Number         0  stm32wlxx_hal_gpio.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_pwr.c 0x00000000   Number         0  stm32wlxx_hal_pwr.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_pwr_ex.c 0x00000000   Number         0  stm32wlxx_hal_pwr_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_rcc.c 0x00000000   Number         0  stm32wlxx_hal_rcc.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_rcc_ex.c 0x00000000   Number         0  stm32wlxx_hal_rcc_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_rtc.c 0x00000000   Number         0  stm32wlxx_hal_rtc.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_rtc_ex.c 0x00000000   Number         0  stm32wlxx_hal_rtc_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_subghz.c 0x00000000   Number         0  stm32wlxx_hal_subghz.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_tim.c 0x00000000   Number         0  stm32wlxx_hal_tim.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_tim_ex.c 0x00000000   Number         0  stm32wlxx_hal_tim_ex.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_uart.c 0x00000000   Number         0  stm32wlxx_hal_uart.o ABSOLUTE
    ../Drivers/STM32WLxx_HAL_Driver/Src/stm32wlxx_hal_uart_ex.c 0x00000000   Number         0  stm32wlxx_hal_uart_ex.o ABSOLUTE
    ../Middlewares/Third_Party/SubGHz_Phy/stm32_radio_driver/radio.c 0x00000000   Number         0  radio.o ABSOLUTE
    ../Middlewares/Third_Party/SubGHz_Phy/stm32_radio_driver/radio_driver.c 0x00000000   Number         0  radio_driver.o ABSOLUTE
    ../Middlewares/Third_Party/SubGHz_Phy/stm32_radio_driver/radio_fw.c 0x00000000   Number         0  radio_fw.o ABSOLUTE
    ../SubGHz_Phy/App/app_subghz_phy.c       0x00000000   Number         0  app_subghz_phy.o ABSOLUTE
    ../SubGHz_Phy/App/subghz_phy_app.c       0x00000000   Number         0  subghz_phy_app.o ABSOLUTE
    ../SubGHz_Phy/Target/radio_board_if.c    0x00000000   Number         0  radio_board_if.o ABSOLUTE
    ../Utilities/lpm/tiny_lpm/stm32_lpm.c    0x00000000   Number         0  stm32_lpm.o ABSOLUTE
    ../Utilities/misc/stm32_mem.c            0x00000000   Number         0  stm32_mem.o ABSOLUTE
    ../Utilities/misc/stm32_systime.c        0x00000000   Number         0  stm32_systime.o ABSOLUTE
    ../Utilities/misc/stm32_tiny_sscanf.c    0x00000000   Number         0  stm32_tiny_sscanf.o ABSOLUTE
    ../Utilities/misc/stm32_tiny_vsnprintf.c 0x00000000   Number         0  stm32_tiny_vsnprintf.o ABSOLUTE
    ../Utilities/sequencer/stm32_seq.c       0x00000000   Number         0  stm32_seq.o ABSOLUTE
    ../Utilities/timer/stm32_timer.c         0x00000000   Number         0  stm32_timer.o ABSOLUTE
    ../Utilities/trace/adv_trace/stm32_adv_trace.c 0x00000000   Number         0  stm32_adv_trace.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit2.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit1.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit3.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardshut.o ABSOLUTE
    ../clib/angel/handlers.s                 0x00000000   Number         0  __scatter_copy.o ABSOLUTE
    ../clib/angel/handlers.s                 0x00000000   Number         0  __scatter_zi.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry4.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  rtexit.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry2.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  rtexit2.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  rt_div0.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  rt_raise.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_ldiv0_sigfpe.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_ldiv0.o ABSOLUTE
    ../clib/angel/scatter.s                  0x00000000   Number         0  __scatter.o ABSOLUTE
    ../clib/angel/startup.s                  0x00000000   Number         0  __main.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  sys_stackheap_outer.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  indicate_semi.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  use_no_semi.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  libspace.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_command.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_wrch.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_exit.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  no_argv.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  _get_argv_nomalloc.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  argv_veneer.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  argv_veneer.o ABSOLUTE
    ../clib/heapalloc.c                      0x00000000   Number         0  hrguard.o ABSOLUTE
    ../clib/heapaux.c                        0x00000000   Number         0  heapauxi.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libshutdown2.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libshutdown.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libinit2.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libinit.o ABSOLUTE
    ../clib/longlong.s                       0x00000000   Number         0  lludivv7m.o ABSOLUTE
    ../clib/memcpset.s                       0x00000000   Number         0  rt_memclr.o ABSOLUTE
    ../clib/memcpset.s                       0x00000000   Number         0  rt_memcpy_w.o ABSOLUTE
    ../clib/memcpset.s                       0x00000000   Number         0  rt_memcpy_v6.o ABSOLUTE
    ../clib/memcpset.s                       0x00000000   Number         0  rt_memclr_w.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_other.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtred_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_abrt_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_exit.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_stak_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_pvfn_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_segv_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  __raise.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_cppl_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_general.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_outer.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_formal.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_formal.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_outer.o ABSOLUTE
    ../clib/signal.s                         0x00000000   Number         0  defsig.o ABSOLUTE
    ../clib/stdlib.c                         0x00000000   Number         0  exit.o ABSOLUTE
    ../clib/string.c                         0x00000000   Number         0  strncmp.o ABSOLUTE
    ../clib/string.c                         0x00000000   Number         0  strlen.o ABSOLUTE
    ../fplib/fpinit.s                        0x00000000   Number         0  fpinit.o ABSOLUTE
    ..\BSP\STM32WLxx_LM40x\stm32wlxx_LM40x.c 0x00000000   Number         0  stm32wlxx_lm40x.o ABSOLUTE
    ..\BSP\STM32WLxx_LM40x\stm32wlxx_LM40x_radio.c 0x00000000   Number         0  stm32wlxx_lm40x_radio.o ABSOLUTE
    ..\Core\Src\dma.c                        0x00000000   Number         0  dma.o ABSOLUTE
    ..\Core\Src\gpio.c                       0x00000000   Number         0  gpio.o ABSOLUTE
    ..\Core\Src\main.c                       0x00000000   Number         0  main.o ABSOLUTE
    ..\Core\Src\rtc.c                        0x00000000   Number         0  rtc.o ABSOLUTE
    ..\Core\Src\stm32_lpm_if.c               0x00000000   Number         0  stm32_lpm_if.o ABSOLUTE
    ..\Core\Src\stm32wlxx_hal_msp.c          0x00000000   Number         0  stm32wlxx_hal_msp.o ABSOLUTE
    ..\Core\Src\stm32wlxx_it.c               0x00000000   Number         0  stm32wlxx_it.o ABSOLUTE
    ..\Core\Src\subghz.c                     0x00000000   Number         0  subghz.o ABSOLUTE
    ..\Core\Src\sys_app.c                    0x00000000   Number         0  sys_app.o ABSOLUTE
    ..\Core\Src\sys_debug.c                  0x00000000   Number         0  sys_debug.o ABSOLUTE
    ..\Core\Src\system_stm32wlxx.c           0x00000000   Number         0  system_stm32wlxx.o ABSOLUTE
    ..\Core\Src\timer_if.c                   0x00000000   Number         0  timer_if.o ABSOLUTE
    ..\Core\Src\usart.c                      0x00000000   Number         0  usart.o ABSOLUTE
    ..\Core\Src\usart_if.c                   0x00000000   Number         0  usart_if.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal.c 0x00000000   Number         0  stm32wlxx_hal.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_cortex.c 0x00000000   Number         0  stm32wlxx_hal_cortex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_dma.c 0x00000000   Number         0  stm32wlxx_hal_dma.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_dma_ex.c 0x00000000   Number         0  stm32wlxx_hal_dma_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_exti.c 0x00000000   Number         0  stm32wlxx_hal_exti.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_flash.c 0x00000000   Number         0  stm32wlxx_hal_flash.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_flash_ex.c 0x00000000   Number         0  stm32wlxx_hal_flash_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_gpio.c 0x00000000   Number         0  stm32wlxx_hal_gpio.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_pwr.c 0x00000000   Number         0  stm32wlxx_hal_pwr.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_pwr_ex.c 0x00000000   Number         0  stm32wlxx_hal_pwr_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_rcc.c 0x00000000   Number         0  stm32wlxx_hal_rcc.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_rcc_ex.c 0x00000000   Number         0  stm32wlxx_hal_rcc_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_rtc.c 0x00000000   Number         0  stm32wlxx_hal_rtc.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_rtc_ex.c 0x00000000   Number         0  stm32wlxx_hal_rtc_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_subghz.c 0x00000000   Number         0  stm32wlxx_hal_subghz.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_tim.c 0x00000000   Number         0  stm32wlxx_hal_tim.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_tim_ex.c 0x00000000   Number         0  stm32wlxx_hal_tim_ex.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_uart.c 0x00000000   Number         0  stm32wlxx_hal_uart.o ABSOLUTE
    ..\Drivers\STM32WLxx_HAL_Driver\Src\stm32wlxx_hal_uart_ex.c 0x00000000   Number         0  stm32wlxx_hal_uart_ex.o ABSOLUTE
    ..\Middlewares\Third_Party\SubGHz_Phy\stm32_radio_driver\radio.c 0x00000000   Number         0  radio.o ABSOLUTE
    ..\Middlewares\Third_Party\SubGHz_Phy\stm32_radio_driver\radio_driver.c 0x00000000   Number         0  radio_driver.o ABSOLUTE
    ..\Middlewares\Third_Party\SubGHz_Phy\stm32_radio_driver\radio_fw.c 0x00000000   Number         0  radio_fw.o ABSOLUTE
    ..\SubGHz_Phy\App\app_subghz_phy.c       0x00000000   Number         0  app_subghz_phy.o ABSOLUTE
    ..\SubGHz_Phy\App\subghz_phy_app.c       0x00000000   Number         0  subghz_phy_app.o ABSOLUTE
    ..\SubGHz_Phy\Target\radio_board_if.c    0x00000000   Number         0  radio_board_if.o ABSOLUTE
    ..\Utilities\lpm\tiny_lpm\stm32_lpm.c    0x00000000   Number         0  stm32_lpm.o ABSOLUTE
    ..\Utilities\misc\stm32_mem.c            0x00000000   Number         0  stm32_mem.o ABSOLUTE
    ..\Utilities\sequencer\stm32_seq.c       0x00000000   Number         0  stm32_seq.o ABSOLUTE
    ..\Utilities\timer\stm32_timer.c         0x00000000   Number         0  stm32_timer.o ABSOLUTE
    ..\Utilities\trace\adv_trace\stm32_adv_trace.c 0x00000000   Number         0  stm32_adv_trace.o ABSOLUTE
    ..\\BSP\\STM32WLxx_LM40x\\stm32wlxx_LM40x.c 0x00000000   Number         0  stm32wlxx_lm40x.o ABSOLUTE
    ..\\BSP\\STM32WLxx_LM40x\\stm32wlxx_LM40x_radio.c 0x00000000   Number         0  stm32wlxx_lm40x_radio.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    startup_stm32wle5xx.s                    0x00000000   Number         0  startup_stm32wle5xx.o ABSOLUTE
    RESET                                    0x08000000   Section      312  startup_stm32wle5xx.o(RESET)
    !!!main                                  0x08000138   Section        8  __main.o(!!!main)
    !!!scatter                               0x08000140   Section       52  __scatter.o(!!!scatter)
    !!handler_copy                           0x08000174   Section       26  __scatter_copy.o(!!handler_copy)
    !!handler_zi                             0x08000190   Section       28  __scatter_zi.o(!!handler_zi)
    .ARM.Collect$$libinit$$00000000          0x080001ac   Section        2  libinit.o(.ARM.Collect$$libinit$$00000000)
    .ARM.Collect$$libinit$$00000002          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000002)
    .ARM.Collect$$libinit$$00000004          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000004)
    .ARM.Collect$$libinit$$0000000A          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000A)
    .ARM.Collect$$libinit$$0000000C          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000C)
    .ARM.Collect$$libinit$$0000000E          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000E)
    .ARM.Collect$$libinit$$00000011          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000011)
    .ARM.Collect$$libinit$$00000013          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000013)
    .ARM.Collect$$libinit$$00000015          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000015)
    .ARM.Collect$$libinit$$00000017          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000017)
    .ARM.Collect$$libinit$$00000019          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000019)
    .ARM.Collect$$libinit$$0000001B          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001B)
    .ARM.Collect$$libinit$$0000001D          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001D)
    .ARM.Collect$$libinit$$0000001F          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001F)
    .ARM.Collect$$libinit$$00000021          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000021)
    .ARM.Collect$$libinit$$00000023          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000023)
    .ARM.Collect$$libinit$$00000025          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000025)
    .ARM.Collect$$libinit$$0000002C          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000002C)
    .ARM.Collect$$libinit$$0000002E          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000002E)
    .ARM.Collect$$libinit$$00000030          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000030)
    .ARM.Collect$$libinit$$00000032          0x080001ae   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000032)
    .ARM.Collect$$libinit$$00000033          0x080001ae   Section        2  libinit2.o(.ARM.Collect$$libinit$$00000033)
    .ARM.Collect$$libshutdown$$00000000      0x080001b0   Section        2  libshutdown.o(.ARM.Collect$$libshutdown$$00000000)
    .ARM.Collect$$libshutdown$$00000003      0x080001b2   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000003)
    .ARM.Collect$$libshutdown$$00000006      0x080001b2   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000006)
    .ARM.Collect$$libshutdown$$00000009      0x080001b2   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000009)
    .ARM.Collect$$libshutdown$$0000000B      0x080001b2   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B)
    .ARM.Collect$$libshutdown$$0000000E      0x080001b2   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E)
    .ARM.Collect$$libshutdown$$0000000F      0x080001b2   Section        2  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F)
    .ARM.Collect$$rtentry$$00000000          0x080001b4   Section        0  __rtentry.o(.ARM.Collect$$rtentry$$00000000)
    .ARM.Collect$$rtentry$$00000002          0x080001b4   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$00000002)
    .ARM.Collect$$rtentry$$00000004          0x080001b4   Section        6  __rtentry4.o(.ARM.Collect$$rtentry$$00000004)
    .ARM.Collect$$rtentry$$00000009          0x080001ba   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$00000009)
    .ARM.Collect$$rtentry$$0000000A          0x080001ba   Section        4  __rtentry2.o(.ARM.Collect$$rtentry$$0000000A)
    .ARM.Collect$$rtentry$$0000000C          0x080001be   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000C)
    .ARM.Collect$$rtentry$$0000000D          0x080001be   Section        8  __rtentry2.o(.ARM.Collect$$rtentry$$0000000D)
    .ARM.Collect$$rtexit$$00000000           0x080001c6   Section        2  rtexit.o(.ARM.Collect$$rtexit$$00000000)
    .ARM.Collect$$rtexit$$00000002           0x080001c8   Section        0  rtexit2.o(.ARM.Collect$$rtexit$$00000002)
    .ARM.Collect$$rtexit$$00000003           0x080001c8   Section        4  rtexit2.o(.ARM.Collect$$rtexit$$00000003)
    .ARM.Collect$$rtexit$$00000004           0x080001cc   Section        6  rtexit2.o(.ARM.Collect$$rtexit$$00000004)
    .text                                    0x080001d4   Section       64  startup_stm32wle5xx.o(.text)
    .text                                    0x08000214   Section      238  lludivv7m.o(.text)
    .text                                    0x08000302   Section        0  strlen.o(.text)
    .text                                    0x08000340   Section        0  strncmp.o(.text)
    .text                                    0x080003d6   Section      138  rt_memcpy_v6.o(.text)
    .text                                    0x08000460   Section       68  rt_memclr.o(.text)
    .text                                    0x080004a4   Section       78  rt_memclr_w.o(.text)
    .text                                    0x080004f2   Section        0  heapauxi.o(.text)
    .text                                    0x080004f8   Section      100  rt_memcpy_w.o(.text)
    .text                                    0x0800055c   Section       74  sys_stackheap_outer.o(.text)
    .text                                    0x080005a6   Section        0  exit.o(.text)
    .text                                    0x080005b4   Section        8  libspace.o(.text)
    .text                                    0x080005bc   Section        0  sys_exit.o(.text)
    .text                                    0x080005c8   Section        2  use_no_semi.o(.text)
    .text                                    0x080005ca   Section        0  indicate_semi.o(.text)
    i.BSP_LED_Init                           0x080005cc   Section        0  stm32wlxx_lm40x.o(i.BSP_LED_Init)
    i.BSP_LED_Toggle                         0x0800061c   Section        0  stm32wlxx_lm40x.o(i.BSP_LED_Toggle)
    i.BSP_PB_Callback                        0x0800063c   Section        0  stm32wlxx_lm40x.o(i.BSP_PB_Callback)
    i.BSP_PB_Init                            0x08000640   Section        0  stm32wlxx_lm40x.o(i.BSP_PB_Init)
    i.BSP_RADIO_ConfigRFSwitch               0x080006e4   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_ConfigRFSwitch)
    i.BSP_RADIO_GetRFOMaxPowerConfig         0x08000728   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetRFOMaxPowerConfig)
    i.BSP_RADIO_GetTxConfig                  0x08000732   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetTxConfig)
    i.BSP_RADIO_Init                         0x08000736   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init)
    i.BSP_RADIO_IsDCDC                       0x08000792   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsDCDC)
    i.BSP_RADIO_IsTCXO                       0x08000796   Section        0  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsTCXO)
    i.BUTTON_SW1_EXTI_Callback               0x0800079a   Section        0  stm32wlxx_lm40x.o(i.BUTTON_SW1_EXTI_Callback)
    BUTTON_SW1_EXTI_Callback                 0x0800079b   Thumb Code    10  stm32wlxx_lm40x.o(i.BUTTON_SW1_EXTI_Callback)
    i.BUTTON_SW2_EXTI_Callback               0x080007a4   Section        0  stm32wlxx_lm40x.o(i.BUTTON_SW2_EXTI_Callback)
    BUTTON_SW2_EXTI_Callback                 0x080007a5   Thumb Code    10  stm32wlxx_lm40x.o(i.BUTTON_SW2_EXTI_Callback)
    i.BUTTON_SW3_EXTI_Callback               0x080007ae   Section        0  stm32wlxx_lm40x.o(i.BUTTON_SW3_EXTI_Callback)
    BUTTON_SW3_EXTI_Callback                 0x080007af   Thumb Code    10  stm32wlxx_lm40x.o(i.BUTTON_SW3_EXTI_Callback)
    i.BusFault_Handler                       0x080007b8   Section        0  stm32wlxx_it.o(i.BusFault_Handler)
    i.DMA1_Channel5_IRQHandler               0x080007bc   Section        0  stm32wlxx_it.o(i.DMA1_Channel5_IRQHandler)
    i.DMA_CalcDMAMUXChannelBaseAndMask       0x080007c8   Section        0  stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXChannelBaseAndMask)
    DMA_CalcDMAMUXChannelBaseAndMask         0x080007c9   Thumb Code    66  stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXChannelBaseAndMask)
    i.DMA_CalcDMAMUXRequestGenBaseAndMask    0x08000814   Section        0  stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXRequestGenBaseAndMask)
    DMA_CalcDMAMUXRequestGenBaseAndMask      0x08000815   Thumb Code    34  stm32wlxx_hal_dma.o(i.DMA_CalcDMAMUXRequestGenBaseAndMask)
    i.DMA_SetConfig                          0x0800083c   Section        0  stm32wlxx_hal_dma.o(i.DMA_SetConfig)
    DMA_SetConfig                            0x0800083d   Thumb Code    62  stm32wlxx_hal_dma.o(i.DMA_SetConfig)
    i.DebugMon_Handler                       0x0800087a   Section        0  stm32wlxx_it.o(i.DebugMon_Handler)
    i.EXTI0_IRQHandler                       0x0800087c   Section        0  stm32wlxx_it.o(i.EXTI0_IRQHandler)
    i.Error_Handler                          0x08000882   Section        0  main.o(i.Error_Handler)
    i.GetTimerTicks                          0x08000888   Section        0  timer_if.o(i.GetTimerTicks)
    GetTimerTicks                            0x08000889   Thumb Code    14  timer_if.o(i.GetTimerTicks)
    i.HAL_DMA_Abort                          0x0800089c   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_Abort)
    i.HAL_DMA_Abort_IT                       0x0800090a   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT)
    i.HAL_DMA_DeInit                         0x0800097c   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_DeInit)
    i.HAL_DMA_IRQHandler                     0x08000a24   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_IRQHandler)
    i.HAL_DMA_Init                           0x08000afc   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_Init)
    i.HAL_DMA_Start_IT                       0x08000bc4   Section        0  stm32wlxx_hal_dma.o(i.HAL_DMA_Start_IT)
    i.HAL_Delay                              0x08000c54   Section        0  sys_app.o(i.HAL_Delay)
    i.HAL_EXTI_GetHandle                     0x08000c5e   Section        0  stm32wlxx_hal_exti.o(i.HAL_EXTI_GetHandle)
    i.HAL_EXTI_RegisterCallback              0x08000c6a   Section        0  stm32wlxx_hal_exti.o(i.HAL_EXTI_RegisterCallback)
    i.HAL_GPIO_DeInit                        0x08000c78   Section        0  stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit)
    i.HAL_GPIO_EXTI_Callback                 0x08000d68   Section        0  subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback)
    i.HAL_GPIO_EXTI_IRQHandler               0x08000db4   Section        0  stm32wlxx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler)
    i.HAL_GPIO_Init                          0x08000dcc   Section        0  stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init)
    i.HAL_GPIO_TogglePin                     0x08000f2c   Section        0  stm32wlxx_hal_gpio.o(i.HAL_GPIO_TogglePin)
    i.HAL_GPIO_WritePin                      0x08000f3c   Section        0  stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin)
    i.HAL_GetTick                            0x08000f48   Section        0  sys_app.o(i.HAL_GetTick)
    i.HAL_Init                               0x08000f5c   Section        0  stm32wlxx_hal.o(i.HAL_Init)
    i.HAL_InitTick                           0x08000f88   Section        0  sys_app.o(i.HAL_InitTick)
    i.HAL_MspInit                            0x08000f8c   Section        0  stm32wlxx_hal_msp.o(i.HAL_MspInit)
    i.HAL_NVIC_DisableIRQ                    0x08000f8e   Section        0  stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ)
    i.HAL_NVIC_EnableIRQ                     0x08000fb0   Section        0  stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    i.HAL_NVIC_SetPriority                   0x08000fcc   Section        0  stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    i.HAL_NVIC_SetPriorityGrouping           0x0800100c   Section        0  stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping)
    i.HAL_PWREx_GetVoltageRange              0x08001030   Section        0  stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_GetVoltageRange)
    i.HAL_PWR_EnableBkUpAccess               0x08001040   Section        0  stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess)
    i.HAL_RCCEx_PeriphCLKConfig              0x08001050   Section        0  stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig)
    i.HAL_RCC_ClockConfig                    0x080011f0   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    i.HAL_RCC_GetHCLKFreq                    0x080013b8   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq)
    i.HAL_RCC_GetPCLK1Freq                   0x080013dc   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    i.HAL_RCC_GetPCLK2Freq                   0x080013fc   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    i.HAL_RCC_GetSysClockFreq                0x0800141c   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    i.HAL_RCC_OscConfig                      0x08001500   Section        0  stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig)
    i.HAL_RTCEx_AlarmBEventCallback          0x08001a0e   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_AlarmBEventCallback)
    i.HAL_RTCEx_BKUPRead                     0x08001a10   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead)
    i.HAL_RTCEx_BKUPWrite                    0x08001a1c   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite)
    i.HAL_RTCEx_EnableBypassShadow           0x08001a28   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_EnableBypassShadow)
    i.HAL_RTCEx_SSRUEventCallback            0x08001a68   Section        0  timer_if.o(i.HAL_RTCEx_SSRUEventCallback)
    i.HAL_RTCEx_SSRUIRQHandler               0x08001a78   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SSRUIRQHandler)
    i.HAL_RTCEx_SetSSRU_IT                   0x08001aa0   Section        0  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSSRU_IT)
    i.HAL_RTC_AlarmAEventCallback            0x08001af0   Section        0  timer_if.o(i.HAL_RTC_AlarmAEventCallback)
    i.HAL_RTC_AlarmIRQHandler                0x08001af4   Section        0  stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler)
    i.HAL_RTC_DeactivateAlarm                0x08001b34   Section        0  stm32wlxx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm)
    i.HAL_RTC_Init                           0x08001bb8   Section        0  stm32wlxx_hal_rtc.o(i.HAL_RTC_Init)
    i.HAL_RTC_MspInit                        0x08001c60   Section        0  rtc.o(i.HAL_RTC_MspInit)
    i.HAL_RTC_SetAlarm_IT                    0x08001cd4   Section        0  stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT)
    i.HAL_RTC_WaitForSynchro                 0x08001e50   Section        0  stm32wlxx_hal_rtc.o(i.HAL_RTC_WaitForSynchro)
    i.HAL_SUBGHZ_CADStatusCallback           0x08001e84   Section        0  radio_driver.o(i.HAL_SUBGHZ_CADStatusCallback)
    i.HAL_SUBGHZ_CRCErrorCallback            0x08001e9c   Section        0  radio_driver.o(i.HAL_SUBGHZ_CRCErrorCallback)
    i.HAL_SUBGHZ_ExecGetCmd                  0x08001ea8   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd)
    i.HAL_SUBGHZ_ExecSetCmd                  0x08001f18   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd)
    i.HAL_SUBGHZ_HeaderErrorCallback         0x08001f94   Section        0  radio_driver.o(i.HAL_SUBGHZ_HeaderErrorCallback)
    i.HAL_SUBGHZ_HeaderValidCallback         0x08001fa0   Section        0  radio_driver.o(i.HAL_SUBGHZ_HeaderValidCallback)
    i.HAL_SUBGHZ_IRQHandler                  0x08001fac   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler)
    i.HAL_SUBGHZ_Init                        0x08002040   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init)
    i.HAL_SUBGHZ_MspInit                     0x080020e4   Section        0  subghz.o(i.HAL_SUBGHZ_MspInit)
    i.HAL_SUBGHZ_PreambleDetectedCallback    0x08002110   Section        0  radio_driver.o(i.HAL_SUBGHZ_PreambleDetectedCallback)
    i.HAL_SUBGHZ_ReadBuffer                  0x0800211c   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer)
    i.HAL_SUBGHZ_ReadRegisters               0x08002194   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters)
    i.HAL_SUBGHZ_RxCpltCallback              0x08002214   Section        0  radio_driver.o(i.HAL_SUBGHZ_RxCpltCallback)
    i.HAL_SUBGHZ_RxTxTimeoutCallback         0x08002220   Section        0  radio_driver.o(i.HAL_SUBGHZ_RxTxTimeoutCallback)
    i.HAL_SUBGHZ_SyncWordValidCallback       0x08002230   Section        0  radio_driver.o(i.HAL_SUBGHZ_SyncWordValidCallback)
    i.HAL_SUBGHZ_TxCpltCallback              0x0800223c   Section        0  radio_driver.o(i.HAL_SUBGHZ_TxCpltCallback)
    i.HAL_SUBGHZ_WriteBuffer                 0x08002248   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer)
    i.HAL_SUBGHZ_WriteRegisters              0x080022b6   Section        0  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters)
    i.HAL_UARTEx_EnableFifoMode              0x08002330   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableFifoMode)
    i.HAL_UARTEx_EnableStopMode              0x0800237a   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableStopMode)
    i.HAL_UARTEx_RxEventCallback             0x080023a8   Section        0  stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback)
    i.HAL_UARTEx_RxFifoFullCallback          0x080023aa   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_RxFifoFullCallback)
    i.HAL_UARTEx_SetRxFifoThreshold          0x080023ac   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetRxFifoThreshold)
    i.HAL_UARTEx_SetTxFifoThreshold          0x080023f8   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetTxFifoThreshold)
    i.HAL_UARTEx_StopModeWakeUpSourceConfig  0x08002444   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_StopModeWakeUpSourceConfig)
    i.HAL_UARTEx_TxFifoEmptyCallback         0x080024ce   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_TxFifoEmptyCallback)
    i.HAL_UARTEx_WakeupCallback              0x080024d0   Section        0  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_WakeupCallback)
    i.HAL_UART_ErrorCallback                 0x080024d2   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback)
    i.HAL_UART_IRQHandler                    0x080024d4   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler)
    i.HAL_UART_Init                          0x080027b4   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_Init)
    i.HAL_UART_MspDeInit                     0x08002820   Section        0  usart.o(i.HAL_UART_MspDeInit)
    i.HAL_UART_MspInit                       0x08002858   Section        0  usart.o(i.HAL_UART_MspInit)
    i.HAL_UART_Receive_IT                    0x0800291c   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_Receive_IT)
    i.HAL_UART_RxCpltCallback                0x08002970   Section        0  usart_if.o(i.HAL_UART_RxCpltCallback)
    i.HAL_UART_Transmit_DMA                  0x080029a8   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA)
    i.HAL_UART_TxCpltCallback                0x08002a4c   Section        0  usart_if.o(i.HAL_UART_TxCpltCallback)
    i.HAL_UART_TxHalfCpltCallback            0x08002a68   Section        0  stm32wlxx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback)
    i.HardFault_Handler                      0x08002a6a   Section        0  stm32wlxx_it.o(i.HardFault_Handler)
    i.LL_AHB1_GRP1_EnableClock               0x08002a6c   Section        0  dma.o(i.LL_AHB1_GRP1_EnableClock)
    LL_AHB1_GRP1_EnableClock                 0x08002a6d   Thumb Code    20  dma.o(i.LL_AHB1_GRP1_EnableClock)
    i.LL_AHB2_GRP1_EnableClock               0x08002a80   Section        0  gpio.o(i.LL_AHB2_GRP1_EnableClock)
    LL_AHB2_GRP1_EnableClock                 0x08002a81   Thumb Code    20  gpio.o(i.LL_AHB2_GRP1_EnableClock)
    i.LL_AHB2_GRP1_EnableClock               0x08002a94   Section        0  stm32wlxx_lm40x.o(i.LL_AHB2_GRP1_EnableClock)
    LL_AHB2_GRP1_EnableClock                 0x08002a95   Thumb Code    20  stm32wlxx_lm40x.o(i.LL_AHB2_GRP1_EnableClock)
    i.LL_AHB2_GRP1_EnableClock               0x08002aa8   Section        0  stm32wlxx_lm40x_radio.o(i.LL_AHB2_GRP1_EnableClock)
    LL_AHB2_GRP1_EnableClock                 0x08002aa9   Thumb Code    20  stm32wlxx_lm40x_radio.o(i.LL_AHB2_GRP1_EnableClock)
    i.LL_PWR_SelectSUBGHZSPI_NSS             0x08002abc   Section        0  stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS)
    LL_PWR_SelectSUBGHZSPI_NSS               0x08002abd   Thumb Code    12  stm32wlxx_hal_subghz.o(i.LL_PWR_SelectSUBGHZSPI_NSS)
    i.LL_PWR_SetRadioBusyTrigger             0x08002acc   Section        0  stm32wlxx_hal_subghz.o(i.LL_PWR_SetRadioBusyTrigger)
    LL_PWR_SetRadioBusyTrigger               0x08002acd   Thumb Code    14  stm32wlxx_hal_subghz.o(i.LL_PWR_SetRadioBusyTrigger)
    i.LL_PWR_UnselectSUBGHZSPI_NSS           0x08002ae0   Section        0  stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS)
    LL_PWR_UnselectSUBGHZSPI_NSS             0x08002ae1   Thumb Code    12  stm32wlxx_hal_subghz.o(i.LL_PWR_UnselectSUBGHZSPI_NSS)
    i.LL_RCC_GetSysClkSource                 0x08002af0   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource)
    LL_RCC_GetSysClkSource                   0x08002af1   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_GetSysClkSource)
    i.LL_RCC_HSE_IsReady                     0x08002afc   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_HSE_IsReady)
    LL_RCC_HSE_IsReady                       0x08002afd   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_HSE_IsReady)
    i.LL_RCC_HSI_IsReady                     0x08002b08   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_IsReady)
    LL_RCC_HSI_IsReady                       0x08002b09   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_IsReady)
    i.LL_RCC_HSI_SetCalibTrimming            0x08002b14   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_SetCalibTrimming)
    LL_RCC_HSI_SetCalibTrimming              0x08002b15   Thumb Code    18  stm32wlxx_hal_rcc.o(i.LL_RCC_HSI_SetCalibTrimming)
    i.LL_RCC_LSE_IsReady                     0x08002b26   Section        0  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSE_IsReady)
    LL_RCC_LSE_IsReady                       0x08002b27   Thumb Code    14  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_LSE_IsReady)
    i.LL_RCC_MSI_IsReady                     0x08002b34   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_IsReady)
    LL_RCC_MSI_IsReady                       0x08002b35   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_IsReady)
    i.LL_RCC_MSI_SetCalibTrimming            0x08002b40   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_SetCalibTrimming)
    LL_RCC_MSI_SetCalibTrimming              0x08002b41   Thumb Code    18  stm32wlxx_hal_rcc.o(i.LL_RCC_MSI_SetCalibTrimming)
    i.LL_RCC_PLL_GetMainSource               0x08002b52   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_GetMainSource)
    LL_RCC_PLL_GetMainSource                 0x08002b53   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_GetMainSource)
    i.LL_RCC_PLL_IsReady                     0x08002b5e   Section        0  stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_IsReady)
    LL_RCC_PLL_IsReady                       0x08002b5f   Thumb Code    12  stm32wlxx_hal_rcc.o(i.LL_RCC_PLL_IsReady)
    i.LL_RCC_SetI2CClockSource               0x08002b6a   Section        0  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetI2CClockSource)
    LL_RCC_SetI2CClockSource                 0x08002b6b   Thumb Code    30  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetI2CClockSource)
    i.LL_RCC_SetLPTIMClockSource             0x08002b88   Section        0  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetLPTIMClockSource)
    LL_RCC_SetLPTIMClockSource               0x08002b89   Thumb Code    22  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetLPTIMClockSource)
    i.LL_RCC_SetUSARTClockSource             0x08002b9e   Section        0  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetUSARTClockSource)
    LL_RCC_SetUSARTClockSource               0x08002b9f   Thumb Code    20  stm32wlxx_hal_rcc_ex.o(i.LL_RCC_SetUSARTClockSource)
    i.MX_DMA_Init                            0x08002bb2   Section        0  dma.o(i.MX_DMA_Init)
    i.MX_GPIO_Init                           0x08002bd4   Section        0  gpio.o(i.MX_GPIO_Init)
    i.MX_RTC_Init                            0x08002c40   Section        0  rtc.o(i.MX_RTC_Init)
    i.MX_SUBGHZ_Init                         0x08002cac   Section        0  subghz.o(i.MX_SUBGHZ_Init)
    i.MX_SubGHz_Phy_Init                     0x08002ccc   Section        0  app_subghz_phy.o(i.MX_SubGHz_Phy_Init)
    i.MX_USART2_UART_Init                    0x08002cdc   Section        0  usart.o(i.MX_USART2_UART_Init)
    i.MemManage_Handler                      0x08002d44   Section        0  stm32wlxx_it.o(i.MemManage_Handler)
    i.NMI_Handler                            0x08002d46   Section        0  stm32wlxx_it.o(i.NMI_Handler)
    i.OnRxDone                               0x08002d48   Section        0  subghz_phy_app.o(i.OnRxDone)
    OnRxDone                                 0x08002d49   Thumb Code   162  subghz_phy_app.o(i.OnRxDone)
    i.OnRxError                              0x08002e44   Section        0  subghz_phy_app.o(i.OnRxError)
    OnRxError                                0x08002e45   Thumb Code    32  subghz_phy_app.o(i.OnRxError)
    i.OnRxTimeout                            0x08002e74   Section        0  subghz_phy_app.o(i.OnRxTimeout)
    OnRxTimeout                              0x08002e75   Thumb Code    30  subghz_phy_app.o(i.OnRxTimeout)
    i.OnTxDone                               0x08002ea8   Section        0  subghz_phy_app.o(i.OnTxDone)
    OnTxDone                                 0x08002ea9   Thumb Code    32  subghz_phy_app.o(i.OnTxDone)
    i.OnTxTimeout                            0x08002ed8   Section        0  subghz_phy_app.o(i.OnTxTimeout)
    OnTxTimeout                              0x08002ed9   Thumb Code    32  subghz_phy_app.o(i.OnTxTimeout)
    i.OnledEvent                             0x08002f0c   Section        0  subghz_phy_app.o(i.OnledEvent)
    OnledEvent                               0x08002f0d   Thumb Code    76  subghz_phy_app.o(i.OnledEvent)
    i.PendSV_Handler                         0x08002f90   Section        0  stm32wlxx_it.o(i.PendSV_Handler)
    i.PingPong_Process                       0x08002f94   Section        0  subghz_phy_app.o(i.PingPong_Process)
    PingPong_Process                         0x08002f95   Thumb Code   312  subghz_phy_app.o(i.PingPong_Process)
    i.RBI_ConfigRFSwitch                     0x08003164   Section        0  radio_board_if.o(i.RBI_ConfigRFSwitch)
    i.RBI_GetRFOMaxPowerConfig               0x08003168   Section        0  radio_board_if.o(i.RBI_GetRFOMaxPowerConfig)
    i.RBI_GetTxConfig                        0x0800316c   Section        0  radio_board_if.o(i.RBI_GetTxConfig)
    i.RBI_Init                               0x08003170   Section        0  radio_board_if.o(i.RBI_Init)
    i.RBI_IsDCDC                             0x08003174   Section        0  radio_board_if.o(i.RBI_IsDCDC)
    i.RBI_IsTCXO                             0x08003178   Section        0  radio_board_if.o(i.RBI_IsTCXO)
    i.RCC_SetFlashLatency                    0x0800317c   Section        0  stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatency)
    RCC_SetFlashLatency                      0x0800317d   Thumb Code   130  stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatency)
    i.RCC_SetFlashLatencyFromMSIRange        0x08003208   Section        0  stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange)
    RCC_SetFlashLatencyFromMSIRange          0x08003209   Thumb Code    54  stm32wlxx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange)
    i.RFW_DeInit                             0x0800324c   Section        0  radio_fw.o(i.RFW_DeInit)
    i.RFW_DeInit_TxLongPacket                0x0800324e   Section        0  radio_fw.o(i.RFW_DeInit_TxLongPacket)
    i.RFW_Init                               0x08003250   Section        0  radio_fw.o(i.RFW_Init)
    i.RFW_Is_Init                            0x08003256   Section        0  radio_fw.o(i.RFW_Is_Init)
    i.RFW_Is_LongPacketModeEnabled           0x0800325a   Section        0  radio_fw.o(i.RFW_Is_LongPacketModeEnabled)
    i.RFW_ReceiveInit                        0x0800325e   Section        0  radio_fw.o(i.RFW_ReceiveInit)
    i.RFW_ReceiveLongPacket                  0x08003264   Section        0  radio_fw.o(i.RFW_ReceiveLongPacket)
    i.RFW_ReceivePayload                     0x0800326a   Section        0  radio_fw.o(i.RFW_ReceivePayload)
    i.RFW_SetAntSwitch                       0x0800326c   Section        0  radio_fw.o(i.RFW_SetAntSwitch)
    i.RFW_SetRadioModem                      0x0800326e   Section        0  radio_fw.o(i.RFW_SetRadioModem)
    i.RFW_TransmitInit                       0x08003270   Section        0  radio_fw.o(i.RFW_TransmitInit)
    i.RFW_TransmitLongPacket                 0x08003276   Section        0  radio_fw.o(i.RFW_TransmitLongPacket)
    i.RTC_Alarm_IRQHandler                   0x0800327c   Section        0  stm32wlxx_it.o(i.RTC_Alarm_IRQHandler)
    i.RTC_ByteToBcd2                         0x08003288   Section        0  stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2)
    i.RTC_EnterInitMode                      0x080032a0   Section        0  stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode)
    i.RTC_ExitInitMode                       0x080032ec   Section        0  stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode)
    i.RadioCheckRfFrequency                  0x08003344   Section        0  radio.o(i.RadioCheckRfFrequency)
    RadioCheckRfFrequency                    0x08003345   Thumb Code     4  radio.o(i.RadioCheckRfFrequency)
    i.RadioGetLoRaTimeOnAirNumerator         0x08003348   Section        0  radio.o(i.RadioGetLoRaTimeOnAirNumerator)
    RadioGetLoRaTimeOnAirNumerator           0x08003349   Thumb Code   122  radio.o(i.RadioGetLoRaTimeOnAirNumerator)
    i.RadioGetStatus                         0x080033c2   Section        0  radio.o(i.RadioGetStatus)
    RadioGetStatus                           0x080033c3   Thumb Code    34  radio.o(i.RadioGetStatus)
    i.RadioGetWakeupTime                     0x080033e4   Section        0  radio.o(i.RadioGetWakeupTime)
    RadioGetWakeupTime                       0x080033e5   Thumb Code    10  radio.o(i.RadioGetWakeupTime)
    i.RadioInit                              0x080033f0   Section        0  radio.o(i.RadioInit)
    RadioInit                                0x080033f1   Thumb Code   122  radio.o(i.RadioInit)
    i.RadioIrqProcess                        0x08003480   Section        0  radio.o(i.RadioIrqProcess)
    RadioIrqProcess                          0x08003481   Thumb Code   602  radio.o(i.RadioIrqProcess)
    i.RadioIsChannelFree                     0x0800373c   Section        0  radio.o(i.RadioIsChannelFree)
    RadioIsChannelFree                       0x0800373d   Thumb Code   134  radio.o(i.RadioIsChannelFree)
    i.RadioOnDioIrq                          0x080037c4   Section        0  radio.o(i.RadioOnDioIrq)
    RadioOnDioIrq                            0x080037c5   Thumb Code    10  radio.o(i.RadioOnDioIrq)
    i.RadioOnRxTimeoutIrq                    0x080037d4   Section        0  radio.o(i.RadioOnRxTimeoutIrq)
    RadioOnRxTimeoutIrq                      0x080037d5   Thumb Code    18  radio.o(i.RadioOnRxTimeoutIrq)
    i.RadioOnTxTimeoutIrq                    0x080037ec   Section        0  radio.o(i.RadioOnTxTimeoutIrq)
    RadioOnTxTimeoutIrq                      0x080037ed   Thumb Code    18  radio.o(i.RadioOnTxTimeoutIrq)
    i.RadioRandom                            0x08003804   Section        0  radio.o(i.RadioRandom)
    RadioRandom                              0x08003805   Thumb Code    22  radio.o(i.RadioRandom)
    i.RadioRead                              0x0800381a   Section        0  radio.o(i.RadioRead)
    RadioRead                                0x0800381b   Thumb Code     4  radio.o(i.RadioRead)
    i.RadioReadRegisters                     0x0800381e   Section        0  radio.o(i.RadioReadRegisters)
    RadioReadRegisters                       0x0800381f   Thumb Code     4  radio.o(i.RadioReadRegisters)
    i.RadioRssi                              0x08003822   Section        0  radio.o(i.RadioRssi)
    RadioRssi                                0x08003823   Thumb Code     4  radio.o(i.RadioRssi)
    i.RadioRx                                0x08003828   Section        0  radio.o(i.RadioRx)
    RadioRx                                  0x08003829   Thumb Code    90  radio.o(i.RadioRx)
    i.RadioRxBoosted                         0x08003888   Section        0  radio.o(i.RadioRxBoosted)
    RadioRxBoosted                           0x08003889   Thumb Code    90  radio.o(i.RadioRxBoosted)
    i.RadioSend                              0x080038e8   Section        0  radio.o(i.RadioSend)
    RadioSend                                0x080038e9   Thumb Code   312  radio.o(i.RadioSend)
    i.RadioSetChannel                        0x08003a40   Section        0  radio.o(i.RadioSetChannel)
    RadioSetChannel                          0x08003a41   Thumb Code     4  radio.o(i.RadioSetChannel)
    i.RadioSetMaxPayloadLength               0x08003a44   Section        0  radio.o(i.RadioSetMaxPayloadLength)
    RadioSetMaxPayloadLength                 0x08003a45   Thumb Code    42  radio.o(i.RadioSetMaxPayloadLength)
    i.RadioSetModem                          0x08003a78   Section        0  radio.o(i.RadioSetModem)
    RadioSetModem                            0x08003a79   Thumb Code    70  radio.o(i.RadioSetModem)
    i.RadioSetPublicNetwork                  0x08003ac4   Section        0  radio.o(i.RadioSetPublicNetwork)
    RadioSetPublicNetwork                    0x08003ac5   Thumb Code    52  radio.o(i.RadioSetPublicNetwork)
    i.RadioSetRxConfig                       0x08003afc   Section        0  radio.o(i.RadioSetRxConfig)
    RadioSetRxConfig                         0x08003afd   Thumb Code   660  radio.o(i.RadioSetRxConfig)
    i.RadioSetRxDutyCycle                    0x08003dac   Section        0  radio.o(i.RadioSetRxDutyCycle)
    RadioSetRxDutyCycle                      0x08003dad   Thumb Code    50  radio.o(i.RadioSetRxDutyCycle)
    i.RadioSetRxGenericConfig                0x08003de4   Section        0  radio.o(i.RadioSetRxGenericConfig)
    RadioSetRxGenericConfig                  0x08003de5   Thumb Code   542  radio.o(i.RadioSetRxGenericConfig)
    i.RadioSetTxConfig                       0x0800400c   Section        0  radio.o(i.RadioSetTxConfig)
    RadioSetTxConfig                         0x0800400d   Thumb Code   364  radio.o(i.RadioSetTxConfig)
    i.RadioSetTxContinuousWave               0x0800418c   Section        0  radio.o(i.RadioSetTxContinuousWave)
    RadioSetTxContinuousWave                 0x0800418d   Thumb Code    54  radio.o(i.RadioSetTxContinuousWave)
    i.RadioSetTxGenericConfig                0x080041c8   Section        0  radio.o(i.RadioSetTxGenericConfig)
    RadioSetTxGenericConfig                  0x080041c9   Thumb Code   644  radio.o(i.RadioSetTxGenericConfig)
    i.RadioSleep                             0x08004454   Section        0  radio.o(i.RadioSleep)
    RadioSleep                               0x08004455   Thumb Code    18  radio.o(i.RadioSleep)
    i.RadioStandby                           0x08004466   Section        0  radio.o(i.RadioStandby)
    RadioStandby                             0x08004467   Thumb Code     6  radio.o(i.RadioStandby)
    i.RadioStartCad                          0x0800446c   Section        0  radio.o(i.RadioStartCad)
    RadioStartCad                            0x0800446d   Thumb Code    36  radio.o(i.RadioStartCad)
    i.RadioTimeOnAir                         0x08004494   Section        0  radio.o(i.RadioTimeOnAir)
    RadioTimeOnAir                           0x08004495   Thumb Code   190  radio.o(i.RadioTimeOnAir)
    i.RadioTxCw                              0x08004564   Section        0  radio.o(i.RadioTxCw)
    RadioTxCw                                0x08004565   Thumb Code    20  radio.o(i.RadioTxCw)
    i.RadioTxPrbs                            0x08004578   Section        0  radio.o(i.RadioTxPrbs)
    RadioTxPrbs                              0x08004579   Thumb Code    38  radio.o(i.RadioTxPrbs)
    i.RadioWrite                             0x080045a8   Section        0  radio.o(i.RadioWrite)
    RadioWrite                               0x080045a9   Thumb Code     4  radio.o(i.RadioWrite)
    i.RadioWriteRegisters                    0x080045ac   Section        0  radio.o(i.RadioWriteRegisters)
    RadioWriteRegisters                      0x080045ad   Thumb Code     4  radio.o(i.RadioWriteRegisters)
    i.Radio_SMPS_Set                         0x080045b0   Section        0  radio_driver.o(i.Radio_SMPS_Set)
    Radio_SMPS_Set                           0x080045b1   Thumb Code    40  radio_driver.o(i.Radio_SMPS_Set)
    i.SEQ_BitPosition                        0x080045d8   Section        0  stm32_seq.o(i.SEQ_BitPosition)
    i.SUBGHZSPI_Init                         0x0800460c   Section        0  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Init)
    i.SUBGHZSPI_Receive                      0x08004630   Section        0  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive)
    i.SUBGHZSPI_Transmit                     0x0800468c   Section        0  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit)
    i.SUBGHZ_CheckDeviceReady                0x080046e4   Section        0  stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady)
    i.SUBGHZ_Radio_IRQHandler                0x0800471c   Section        0  stm32wlxx_it.o(i.SUBGHZ_Radio_IRQHandler)
    i.SUBGHZ_WaitOnBusy                      0x08004728   Section        0  stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy)
    i.SUBGRF_Calibrate                       0x08004770   Section        0  radio_driver.o(i.SUBGRF_Calibrate)
    i.SUBGRF_CalibrateImage                  0x080047b8   Section        0  radio_driver.o(i.SUBGRF_CalibrateImage)
    i.SUBGRF_GetCFO                          0x0800482c   Section        0  radio_driver.o(i.SUBGRF_GetCFO)
    i.SUBGRF_GetFskBandwidthRegValue         0x080048a0   Section        0  radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue)
    i.SUBGRF_GetOperatingMode                0x080048c8   Section        0  radio_driver.o(i.SUBGRF_GetOperatingMode)
    i.SUBGRF_GetPacketStatus                 0x080048d4   Section        0  radio_driver.o(i.SUBGRF_GetPacketStatus)
    i.SUBGRF_GetPayload                      0x08004948   Section        0  radio_driver.o(i.SUBGRF_GetPayload)
    i.SUBGRF_GetRadioWakeUpTime              0x08004976   Section        0  radio_driver.o(i.SUBGRF_GetRadioWakeUpTime)
    i.SUBGRF_GetRandom                       0x0800497a   Section        0  radio_driver.o(i.SUBGRF_GetRandom)
    i.SUBGRF_GetRssiInst                     0x080049d8   Section        0  radio_driver.o(i.SUBGRF_GetRssiInst)
    i.SUBGRF_GetRxBufferStatus               0x080049f0   Section        0  radio_driver.o(i.SUBGRF_GetRxBufferStatus)
    i.SUBGRF_Init                            0x08004a2c   Section        0  radio_driver.o(i.SUBGRF_Init)
    i.SUBGRF_ReadBuffer                      0x08004a88   Section        0  radio_driver.o(i.SUBGRF_ReadBuffer)
    i.SUBGRF_ReadCommand                     0x08004aa8   Section        0  radio_driver.o(i.SUBGRF_ReadCommand)
    SUBGRF_ReadCommand                       0x08004aa9   Thumb Code    26  radio_driver.o(i.SUBGRF_ReadCommand)
    i.SUBGRF_ReadRegister                    0x08004ac8   Section        0  radio_driver.o(i.SUBGRF_ReadRegister)
    i.SUBGRF_ReadRegisters                   0x08004ae0   Section        0  radio_driver.o(i.SUBGRF_ReadRegisters)
    i.SUBGRF_SendPayload                     0x08004b00   Section        0  radio_driver.o(i.SUBGRF_SendPayload)
    i.SUBGRF_SetBufferBaseAddress            0x08004b12   Section        0  radio_driver.o(i.SUBGRF_SetBufferBaseAddress)
    i.SUBGRF_SetCad                          0x08004b28   Section        0  radio_driver.o(i.SUBGRF_SetCad)
    i.SUBGRF_SetCrcPolynomial                0x08004b40   Section        0  radio_driver.o(i.SUBGRF_SetCrcPolynomial)
    i.SUBGRF_SetCrcSeed                      0x08004b68   Section        0  radio_driver.o(i.SUBGRF_SetCrcSeed)
    i.SUBGRF_SetDioIrqParams                 0x08004b90   Section        0  radio_driver.o(i.SUBGRF_SetDioIrqParams)
    i.SUBGRF_SetLoRaSymbNumTimeout           0x08004bc6   Section        0  radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout)
    i.SUBGRF_SetModulationParams             0x08004bfc   Section        0  radio_driver.o(i.SUBGRF_SetModulationParams)
    i.SUBGRF_SetPaConfig                     0x08004ce0   Section        0  radio_driver.o(i.SUBGRF_SetPaConfig)
    i.SUBGRF_SetPacketParams                 0x08004d00   Section        0  radio_driver.o(i.SUBGRF_SetPacketParams)
    i.SUBGRF_SetPacketType                   0x08004dd8   Section        0  radio_driver.o(i.SUBGRF_SetPacketType)
    i.SUBGRF_SetPayload                      0x08004e00   Section        0  radio_driver.o(i.SUBGRF_SetPayload)
    i.SUBGRF_SetRegulatorMode                0x08004e0a   Section        0  radio_driver.o(i.SUBGRF_SetRegulatorMode)
    i.SUBGRF_SetRfFrequency                  0x08004e28   Section        0  radio_driver.o(i.SUBGRF_SetRfFrequency)
    i.SUBGRF_SetRfTxPower                    0x08004e74   Section        0  radio_driver.o(i.SUBGRF_SetRfTxPower)
    i.SUBGRF_SetRx                           0x08004ea0   Section        0  radio_driver.o(i.SUBGRF_SetRx)
    i.SUBGRF_SetRxBoosted                    0x08004ec8   Section        0  radio_driver.o(i.SUBGRF_SetRxBoosted)
    i.SUBGRF_SetRxDutyCycle                  0x08004efc   Section        0  radio_driver.o(i.SUBGRF_SetRxDutyCycle)
    i.SUBGRF_SetSleep                        0x08004f34   Section        0  radio_driver.o(i.SUBGRF_SetSleep)
    i.SUBGRF_SetStandby                      0x08004f74   Section        0  radio_driver.o(i.SUBGRF_SetStandby)
    i.SUBGRF_SetStopRxTimerOnPreambleDetect  0x08004f98   Section        0  radio_driver.o(i.SUBGRF_SetStopRxTimerOnPreambleDetect)
    i.SUBGRF_SetSwitch                       0x08004fa6   Section        0  radio_driver.o(i.SUBGRF_SetSwitch)
    i.SUBGRF_SetSyncWord                     0x08004fce   Section        0  radio_driver.o(i.SUBGRF_SetSyncWord)
    i.SUBGRF_SetTcxoMode                     0x08004fe0   Section        0  radio_driver.o(i.SUBGRF_SetTcxoMode)
    i.SUBGRF_SetTx                           0x08005008   Section        0  radio_driver.o(i.SUBGRF_SetTx)
    i.SUBGRF_SetTxContinuousWave             0x08005030   Section        0  radio_driver.o(i.SUBGRF_SetTxContinuousWave)
    i.SUBGRF_SetTxInfinitePreamble           0x0800503a   Section        0  radio_driver.o(i.SUBGRF_SetTxInfinitePreamble)
    i.SUBGRF_SetTxParams                     0x08005044   Section        0  radio_driver.o(i.SUBGRF_SetTxParams)
    i.SUBGRF_SetWhiteningSeed                0x08005154   Section        0  radio_driver.o(i.SUBGRF_SetWhiteningSeed)
    i.SUBGRF_WriteBuffer                     0x0800518c   Section        0  radio_driver.o(i.SUBGRF_WriteBuffer)
    i.SUBGRF_WriteCommand                    0x080051ac   Section        0  radio_driver.o(i.SUBGRF_WriteCommand)
    SUBGRF_WriteCommand                      0x080051ad   Thumb Code    26  radio_driver.o(i.SUBGRF_WriteCommand)
    i.SUBGRF_WriteRegister                   0x080051cc   Section        0  radio_driver.o(i.SUBGRF_WriteRegister)
    i.SUBGRF_WriteRegisters                  0x080051e0   Section        0  radio_driver.o(i.SUBGRF_WriteRegisters)
    i.SVC_Handler                            0x08005200   Section        0  stm32wlxx_it.o(i.SVC_Handler)
    i.SubghzApp_Init                         0x08005204   Section        0  subghz_phy_app.o(i.SubghzApp_Init)
    i.SysTick_Handler                        0x08005448   Section        0  stm32wlxx_it.o(i.SysTick_Handler)
    i.SysTimeAdd                             0x0800544a   Section        0  stm32_systime.o(i.SysTimeAdd)
    i.SysTimeGet                             0x08005470   Section        0  stm32_systime.o(i.SysTimeGet)
    i.SystemApp_Init                         0x080054b4   Section        0  sys_app.o(i.SystemApp_Init)
    i.SystemClock_Config                     0x080054fc   Section        0  main.o(i.SystemClock_Config)
    i.SystemInit                             0x08005580   Section        0  system_stm32wlxx.o(i.SystemInit)
    i.TAMP_STAMP_LSECSS_SSRU_IRQHandler      0x08005584   Section        0  stm32wlxx_it.o(i.TAMP_STAMP_LSECSS_SSRU_IRQHandler)
    i.TIMER_IF_BkUp_Read_MSBticks            0x08005590   Section        0  timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks)
    TIMER_IF_BkUp_Read_MSBticks              0x08005591   Thumb Code     8  timer_if.o(i.TIMER_IF_BkUp_Read_MSBticks)
    i.TIMER_IF_BkUp_Read_Seconds             0x0800559c   Section        0  timer_if.o(i.TIMER_IF_BkUp_Read_Seconds)
    i.TIMER_IF_BkUp_Read_SubSeconds          0x080055a8   Section        0  timer_if.o(i.TIMER_IF_BkUp_Read_SubSeconds)
    i.TIMER_IF_BkUp_Write_MSBticks           0x080055b4   Section        0  timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks)
    TIMER_IF_BkUp_Write_MSBticks             0x080055b5   Thumb Code    10  timer_if.o(i.TIMER_IF_BkUp_Write_MSBticks)
    i.TIMER_IF_BkUp_Write_Seconds            0x080055c4   Section        0  timer_if.o(i.TIMER_IF_BkUp_Write_Seconds)
    i.TIMER_IF_BkUp_Write_SubSeconds         0x080055d4   Section        0  timer_if.o(i.TIMER_IF_BkUp_Write_SubSeconds)
    i.TIMER_IF_Convert_Tick2ms               0x080055e4   Section        0  timer_if.o(i.TIMER_IF_Convert_Tick2ms)
    i.TIMER_IF_Convert_ms2Tick               0x080055f4   Section        0  timer_if.o(i.TIMER_IF_Convert_ms2Tick)
    i.TIMER_IF_DelayMs                       0x08005606   Section        0  timer_if.o(i.TIMER_IF_DelayMs)
    i.TIMER_IF_GetMinimumTimeout             0x08005624   Section        0  timer_if.o(i.TIMER_IF_GetMinimumTimeout)
    i.TIMER_IF_GetTime                       0x08005628   Section        0  timer_if.o(i.TIMER_IF_GetTime)
    i.TIMER_IF_GetTimerContext               0x08005650   Section        0  timer_if.o(i.TIMER_IF_GetTimerContext)
    i.TIMER_IF_GetTimerElapsedTime           0x0800565c   Section        0  timer_if.o(i.TIMER_IF_GetTimerElapsedTime)
    i.TIMER_IF_GetTimerValue                 0x08005670   Section        0  timer_if.o(i.TIMER_IF_GetTimerValue)
    i.TIMER_IF_Init                          0x08005684   Section        0  timer_if.o(i.TIMER_IF_Init)
    i.TIMER_IF_SetTimerContext               0x080056cc   Section        0  timer_if.o(i.TIMER_IF_SetTimerContext)
    i.TIMER_IF_StartTimer                    0x080056dc   Section        0  timer_if.o(i.TIMER_IF_StartTimer)
    i.TIMER_IF_StopTimer                     0x08005728   Section        0  timer_if.o(i.TIMER_IF_StopTimer)
    i.TRACE_AllocateBufer                    0x0800574c   Section        0  stm32_adv_trace.o(i.TRACE_AllocateBufer)
    TRACE_AllocateBufer                      0x0800574d   Thumb Code    90  stm32_adv_trace.o(i.TRACE_AllocateBufer)
    i.TRACE_Lock                             0x080057ac   Section        0  stm32_adv_trace.o(i.TRACE_Lock)
    TRACE_Lock                               0x080057ad   Thumb Code    20  stm32_adv_trace.o(i.TRACE_Lock)
    i.TRACE_Send                             0x080057c4   Section        0  stm32_adv_trace.o(i.TRACE_Send)
    TRACE_Send                               0x080057c5   Thumb Code   126  stm32_adv_trace.o(i.TRACE_Send)
    i.TRACE_TxCpltCallback                   0x0800584c   Section        0  stm32_adv_trace.o(i.TRACE_TxCpltCallback)
    TRACE_TxCpltCallback                     0x0800584d   Thumb Code   140  stm32_adv_trace.o(i.TRACE_TxCpltCallback)
    i.TRACE_UnLock                           0x080058e0   Section        0  stm32_adv_trace.o(i.TRACE_UnLock)
    TRACE_UnLock                             0x080058e1   Thumb Code    20  stm32_adv_trace.o(i.TRACE_UnLock)
    i.TimerExists                            0x080058f8   Section        0  stm32_timer.o(i.TimerExists)
    i.TimerInsertNewHeadTimer                0x08005914   Section        0  stm32_timer.o(i.TimerInsertNewHeadTimer)
    i.TimerInsertTimer                       0x0800592c   Section        0  stm32_timer.o(i.TimerInsertTimer)
    i.TimerSetTimeout                        0x08005954   Section        0  stm32_timer.o(i.TimerSetTimeout)
    i.TimestampNow                           0x08005988   Section        0  sys_app.o(i.TimestampNow)
    TimestampNow                             0x08005989   Thumb Code    40  sys_app.o(i.TimestampNow)
    i.UARTEx_SetNbDataToProcess              0x080059bc   Section        0  stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess)
    UARTEx_SetNbDataToProcess                0x080059bd   Thumb Code    62  stm32wlxx_hal_uart_ex.o(i.UARTEx_SetNbDataToProcess)
    i.UART_AdvFeatureConfig                  0x08005a00   Section        0  stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig)
    i.UART_CheckIdleState                    0x08005ac8   Section        0  stm32wlxx_hal_uart.o(i.UART_CheckIdleState)
    i.UART_DMAAbortOnError                   0x08005b28   Section        0  stm32wlxx_hal_uart.o(i.UART_DMAAbortOnError)
    UART_DMAAbortOnError                     0x08005b29   Thumb Code    20  stm32wlxx_hal_uart.o(i.UART_DMAAbortOnError)
    i.UART_DMAError                          0x08005b3c   Section        0  stm32wlxx_hal_uart.o(i.UART_DMAError)
    UART_DMAError                            0x08005b3d   Thumb Code    80  stm32wlxx_hal_uart.o(i.UART_DMAError)
    i.UART_DMATransmitCplt                   0x08005b8c   Section        0  stm32wlxx_hal_uart.o(i.UART_DMATransmitCplt)
    UART_DMATransmitCplt                     0x08005b8d   Thumb Code    66  stm32wlxx_hal_uart.o(i.UART_DMATransmitCplt)
    i.UART_DMATxHalfCplt                     0x08005bce   Section        0  stm32wlxx_hal_uart.o(i.UART_DMATxHalfCplt)
    UART_DMATxHalfCplt                       0x08005bcf   Thumb Code    10  stm32wlxx_hal_uart.o(i.UART_DMATxHalfCplt)
    i.UART_EndRxTransfer                     0x08005bd8   Section        0  stm32wlxx_hal_uart.o(i.UART_EndRxTransfer)
    UART_EndRxTransfer                       0x08005bd9   Thumb Code    78  stm32wlxx_hal_uart.o(i.UART_EndRxTransfer)
    i.UART_EndTxTransfer                     0x08005c2c   Section        0  stm32wlxx_hal_uart.o(i.UART_EndTxTransfer)
    UART_EndTxTransfer                       0x08005c2d   Thumb Code    46  stm32wlxx_hal_uart.o(i.UART_EndTxTransfer)
    i.UART_RxISR_16BIT                       0x08005c5a   Section        0  stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT)
    UART_RxISR_16BIT                         0x08005c5b   Thumb Code   162  stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT)
    i.UART_RxISR_16BIT_FIFOEN                0x08005cfc   Section        0  stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN)
    UART_RxISR_16BIT_FIFOEN                  0x08005cfd   Thumb Code   360  stm32wlxx_hal_uart.o(i.UART_RxISR_16BIT_FIFOEN)
    i.UART_RxISR_8BIT                        0x08005e6c   Section        0  stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT)
    UART_RxISR_8BIT                          0x08005e6d   Thumb Code   162  stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT)
    i.UART_RxISR_8BIT_FIFOEN                 0x08005f10   Section        0  stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN)
    UART_RxISR_8BIT_FIFOEN                   0x08005f11   Thumb Code   360  stm32wlxx_hal_uart.o(i.UART_RxISR_8BIT_FIFOEN)
    i.UART_SetConfig                         0x08006080   Section        0  stm32wlxx_hal_uart.o(i.UART_SetConfig)
    i.UART_Start_Receive_IT                  0x080062c8   Section        0  stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT)
    i.UART_WaitOnFlagUntilTimeout            0x080063e0   Section        0  stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    i.USART2_IRQHandler                      0x080064a4   Section        0  stm32wlxx_it.o(i.USART2_IRQHandler)
    i.UTIL_ADV_TRACE_COND_FSend              0x080064b0   Section        0  stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend)
    i.UTIL_ADV_TRACE_Init                    0x08006564   Section        0  stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init)
    i.UTIL_ADV_TRACE_PostSendHook            0x08006598   Section        0  sys_app.o(i.UTIL_ADV_TRACE_PostSendHook)
    i.UTIL_ADV_TRACE_PreSendHook             0x080065a0   Section        0  sys_app.o(i.UTIL_ADV_TRACE_PreSendHook)
    i.UTIL_ADV_TRACE_RegisterTimeStampFunction 0x080065a8   Section        0  stm32_adv_trace.o(i.UTIL_ADV_TRACE_RegisterTimeStampFunction)
    i.UTIL_ADV_TRACE_SetVerboseLevel         0x080065b4   Section        0  stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetVerboseLevel)
    i.UTIL_LPM_Init                          0x080065c0   Section        0  stm32_lpm.o(i.UTIL_LPM_Init)
    i.UTIL_LPM_SetOffMode                    0x080065d0   Section        0  stm32_lpm.o(i.UTIL_LPM_SetOffMode)
    i.UTIL_LPM_SetStopMode                   0x080065f4   Section        0  stm32_lpm.o(i.UTIL_LPM_SetStopMode)
    i.UTIL_MEM_cpy_8                         0x08006618   Section        0  stm32_mem.o(i.UTIL_MEM_cpy_8)
    i.UTIL_MEM_set_8                         0x0800662a   Section        0  stm32_mem.o(i.UTIL_MEM_set_8)
    i.UTIL_SEQ_RegTask                       0x08006638   Section        0  stm32_seq.o(i.UTIL_SEQ_RegTask)
    i.UTIL_SEQ_SetTask                       0x08006658   Section        0  stm32_seq.o(i.UTIL_SEQ_SetTask)
    i.UTIL_TIMER_Create                      0x08006680   Section        0  stm32_timer.o(i.UTIL_TIMER_Create)
    i.UTIL_TIMER_GetCurrentTime              0x080066bc   Section        0  stm32_timer.o(i.UTIL_TIMER_GetCurrentTime)
    i.UTIL_TIMER_GetElapsedTime              0x080066d0   Section        0  stm32_timer.o(i.UTIL_TIMER_GetElapsedTime)
    i.UTIL_TIMER_IRQ_Handler                 0x080066f0   Section        0  stm32_timer.o(i.UTIL_TIMER_IRQ_Handler)
    i.UTIL_TIMER_Init                        0x08006778   Section        0  stm32_timer.o(i.UTIL_TIMER_Init)
    i.UTIL_TIMER_SetPeriod                   0x0800678c   Section        0  stm32_timer.o(i.UTIL_TIMER_SetPeriod)
    i.UTIL_TIMER_Start                       0x080067c4   Section        0  stm32_timer.o(i.UTIL_TIMER_Start)
    i.UTIL_TIMER_Stop                        0x08006840   Section        0  stm32_timer.o(i.UTIL_TIMER_Stop)
    i.UsageFault_Handler                     0x080068a8   Section        0  stm32wlxx_it.o(i.UsageFault_Handler)
    i.__NVIC_SetPriority                     0x080068aa   Section        0  stm32wlxx_hal_cortex.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x080068ab   Thumb Code    32  stm32wlxx_hal_cortex.o(i.__NVIC_SetPriority)
    i.ee_number                              0x080068cc   Section        0  stm32_tiny_vsnprintf.o(i.ee_number)
    ee_number                                0x080068cd   Thumb Code   236  stm32_tiny_vsnprintf.o(i.ee_number)
    i.main                                   0x080069bc   Section        0  main.o(i.main)
    i.payload_integration                    0x080069ce   Section        0  radio.o(i.payload_integration)
    payload_integration                      0x080069cf   Thumb Code   124  radio.o(i.payload_integration)
    i.tiny_snprintf_like                     0x08006a4a   Section        0  sys_app.o(i.tiny_snprintf_like)
    tiny_snprintf_like                       0x08006a4b   Thumb Code    18  sys_app.o(i.tiny_snprintf_like)
    i.tiny_vsnprintf_like                    0x08006a5c   Section        0  stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like)
    i.vcom_DeInit                            0x08006bac   Section        0  usart_if.o(i.vcom_DeInit)
    i.vcom_Init                              0x08006bd8   Section        0  usart_if.o(i.vcom_Init)
    i.vcom_ReceiveInit                       0x08006bfc   Section        0  usart_if.o(i.vcom_ReceiveInit)
    i.vcom_Trace_DMA                         0x08006c44   Section        0  usart_if.o(i.vcom_Trace_DMA)
    .constdata                               0x08006c58   Section       44  timer_if.o(.constdata)
    .constdata                               0x08006c84   Section       20  timer_if.o(.constdata)
    .constdata                               0x08006c98   Section       16  usart_if.o(.constdata)
    .constdata                               0x08006ca8   Section       28  stm32wlxx_hal_rcc.o(.constdata)
    .constdata                               0x08006cc4   Section       24  stm32wlxx_hal_uart.o(.constdata)
    .constdata                               0x08006cdc   Section       16  stm32wlxx_hal_uart_ex.o(.constdata)
    numerator                                0x08006cdc   Data           8  stm32wlxx_hal_uart_ex.o(.constdata)
    denominator                              0x08006ce4   Data           8  stm32wlxx_hal_uart_ex.o(.constdata)
    .constdata                               0x08006cec   Section      128  system_stm32wlxx.o(.constdata)
    .constdata                               0x08006d6c   Section       32  system_stm32wlxx.o(.constdata)
    .constdata                               0x08006d8c   Section      176  radio_driver.o(.constdata)
    FskBandwidths                            0x08006d8c   Data         176  radio_driver.o(.constdata)
    .constdata                               0x08006e3c   Section      132  radio.o(.constdata)
    .constdata                               0x08006ec0   Section        3  radio.o(.constdata)
    .constdata                               0x08006ec3   Section       16  stm32_seq.o(.constdata)
    .constdata                               0x08006ed4   Section       28  stm32wlxx_lm40x.o(.constdata)
    BUTTON_IRQn                              0x08006ed4   Data           3  stm32wlxx_lm40x.o(.constdata)
    LED_PIN                                  0x08006ed8   Data           6  stm32wlxx_lm40x.o(.constdata)
    BUTTON_PIN                               0x08006ede   Data           6  stm32wlxx_lm40x.o(.constdata)
    button_exti_line                         0x08006ee4   Data          12  stm32wlxx_lm40x.o(.constdata)
    .conststring                             0x08006ef0   Section       77  stm32_tiny_vsnprintf.o(.conststring)
    .data                                    0x20000000   Section        1  sys_app.o(.data)
    SYS_TimerInitialisedFlag                 0x20000000   Data           1  sys_app.o(.data)
    .data                                    0x20000004   Section        8  timer_if.o(.data)
    RTC_Initialized                          0x20000004   Data           1  timer_if.o(.data)
    RtcTimerContext                          0x20000008   Data           4  timer_if.o(.data)
    .data                                    0x2000000c   Section       12  usart_if.o(.data)
    TxCpltCallback                           0x20000010   Data           4  usart_if.o(.data)
    RxCpltCallback                           0x20000014   Data           4  usart_if.o(.data)
    .data                                    0x20000018   Section       12  subghz_phy_app.o(.data)
    State                                    0x20000018   Data           1  subghz_phy_app.o(.data)
    random_delay                             0x20000020   Data           4  subghz_phy_app.o(.data)
    .data                                    0x20000024   Section       12  stm32wlxx_hal.o(.data)
    .data                                    0x20000030   Section        4  system_stm32wlxx.o(.data)
    .data                                    0x20000034   Section       12  radio_driver.o(.data)
    ImageCalibrated                          0x20000034   Data           1  radio_driver.o(.data)
    OperatingMode                            0x20000035   Data           1  radio_driver.o(.data)
    PacketType                               0x20000036   Data           1  radio_driver.o(.data)
    LoRaHeaderType                           0x20000037   Data           1  radio_driver.o(.data)
    RadioOnDioIrqCb                          0x2000003c   Data           4  radio_driver.o(.data)
    .data                                    0x20000040   Section        8  radio.o(.data)
    MaxPayloadLength                         0x20000040   Data           1  radio.o(.data)
    RadioEvents                              0x20000044   Data           4  radio.o(.data)
    .data                                    0x20000048   Section        8  stm32_tiny_vsnprintf.o(.data)
    lower_digits                             0x20000048   Data           4  stm32_tiny_vsnprintf.o(.data)
    upper_digits                             0x2000004c   Data           4  stm32_tiny_vsnprintf.o(.data)
    .data                                    0x20000050   Section       36  stm32_seq.o(.data)
    TaskMask                                 0x20000050   Data           4  stm32_seq.o(.data)
    SuperMask                                0x20000054   Data           4  stm32_seq.o(.data)
    EvtSet                                   0x20000058   Data           4  stm32_seq.o(.data)
    EvtWaited                                0x2000005c   Data           4  stm32_seq.o(.data)
    CurrentTaskIdx                           0x20000060   Data           4  stm32_seq.o(.data)
    TaskSet                                  0x20000064   Data           4  stm32_seq.o(.data)
    TaskCb                                   0x20000068   Data           4  stm32_seq.o(.data)
    TaskPrio                                 0x2000006c   Data           8  stm32_seq.o(.data)
    .data                                    0x20000074   Section        4  stm32_timer.o(.data)
    TimerListHead                            0x20000074   Data           4  stm32_timer.o(.data)
    .data                                    0x20000078   Section        8  stm32_lpm.o(.data)
    StopModeDisable                          0x20000078   Data           4  stm32_lpm.o(.data)
    OffModeDisable                           0x2000007c   Data           4  stm32_lpm.o(.data)
    .data                                    0x20000080   Section       48  stm32wlxx_lm40x.o(.data)
    LED_PORT                                 0x20000080   Data          12  stm32wlxx_lm40x.o(.data)
    BUTTON_PORT                              0x2000008c   Data          12  stm32wlxx_lm40x.o(.data)
    button_callback                          0x20000098   Data          12  stm32wlxx_lm40x.o(.data)
    button_interrupt_priority                0x200000a4   Data          12  stm32wlxx_lm40x.o(.data)
    .bss                                     0x200000b0   Section       56  rtc.o(.bss)
    .bss                                     0x200000e8   Section       12  subghz.o(.bss)
    .bss                                     0x200000f4   Section      240  usart.o(.bss)
    .bss                                     0x200001e4   Section      564  subghz_phy_app.o(.bss)
    RadioEvents                              0x200001e4   Data          28  subghz_phy_app.o(.bss)
    BufferRx                                 0x20000200   Data         255  subghz_phy_app.o(.bss)
    BufferTx                                 0x200002ff   Data         255  subghz_phy_app.o(.bss)
    timerLed                                 0x20000400   Data          24  subghz_phy_app.o(.bss)
    .bss                                     0x20000418   Section      396  radio.o(.bss)
    RadioBuffer                              0x20000418   Data         255  radio.o(.bss)
    .bss                                     0x200005a4   Section      792  stm32_adv_trace.o(.bss)
    ADV_TRACE_Ctx                            0x200005a4   Data          24  stm32_adv_trace.o(.bss)
    ADV_TRACE_Buffer                         0x200005bc   Data         512  stm32_adv_trace.o(.bss)
    sztmp                                    0x200007bc   Data         256  stm32_adv_trace.o(.bss)
    .bss                                     0x200008bc   Section       24  stm32wlxx_lm40x.o(.bss)
    .bss                                     0x200008d4   Section       96  libspace.o(.bss)
    HEAP                                     0x20000938   Section      512  startup_stm32wle5xx.o(HEAP)
    Heap_Mem                                 0x20000938   Data         512  startup_stm32wle5xx.o(HEAP)
    STACK                                    0x20000b38   Section     2048  startup_stm32wle5xx.o(STACK)
    Stack_Mem                                0x20000b38   Data        2048  startup_stm32wle5xx.o(STACK)
    __initial_sp                             0x20001338   Data           0  startup_stm32wle5xx.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$UX$STANDARDLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    __ARM_exceptions_init                     - Undefined Weak Reference
    __alloca_initialize                       - Undefined Weak Reference
    __arm_preinit_                            - Undefined Weak Reference
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    __rt_locale                               - Undefined Weak Reference
    __sigvec_lookup                           - Undefined Weak Reference
    _atexit_init                              - Undefined Weak Reference
    _call_atexit_fns                          - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _fp_trap_init                             - Undefined Weak Reference
    _fp_trap_shutdown                         - Undefined Weak Reference
    _get_lc_collate                           - Undefined Weak Reference
    _get_lc_ctype                             - Undefined Weak Reference
    _get_lc_monetary                          - Undefined Weak Reference
    _get_lc_numeric                           - Undefined Weak Reference
    _get_lc_time                              - Undefined Weak Reference
    _getenv_init                              - Undefined Weak Reference
    _handle_redirection                       - Undefined Weak Reference
    _init_alloc                               - Undefined Weak Reference
    _init_user_alloc                          - Undefined Weak Reference
    _initio                                   - Undefined Weak Reference
    _rand_init                                - Undefined Weak Reference
    _signal_finish                            - Undefined Weak Reference
    _signal_init                              - Undefined Weak Reference
    _terminate_alloc                          - Undefined Weak Reference
    _terminate_user_alloc                     - Undefined Weak Reference
    _terminateio                              - Undefined Weak Reference
    __Vectors_Size                           0x00000138   Number         0  startup_stm32wle5xx.o ABSOLUTE
    __Vectors                                0x08000000   Data           4  startup_stm32wle5xx.o(RESET)
    __Vectors_End                            0x08000138   Data           0  startup_stm32wle5xx.o(RESET)
    __main                                   0x08000139   Thumb Code     8  __main.o(!!!main)
    __scatterload                            0x08000141   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_rt2                        0x08000141   Thumb Code    44  __scatter.o(!!!scatter)
    __scatterload_rt2_thumb_only             0x08000141   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_null                       0x0800014f   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_copy                       0x08000175   Thumb Code    26  __scatter_copy.o(!!handler_copy)
    __scatterload_zeroinit                   0x08000191   Thumb Code    28  __scatter_zi.o(!!handler_zi)
    __rt_lib_init                            0x080001ad   Thumb Code     0  libinit.o(.ARM.Collect$$libinit$$00000000)
    __rt_lib_init_alloca_1                   0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000002E)
    __rt_lib_init_argv_1                     0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000002C)
    __rt_lib_init_atexit_1                   0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001B)
    __rt_lib_init_clock_1                    0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000021)
    __rt_lib_init_cpp_1                      0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000032)
    __rt_lib_init_exceptions_1               0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000030)
    __rt_lib_init_fp_1                       0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000002)
    __rt_lib_init_fp_trap_1                  0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001F)
    __rt_lib_init_getenv_1                   0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000023)
    __rt_lib_init_heap_1                     0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000A)
    __rt_lib_init_lc_collate_1               0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000011)
    __rt_lib_init_lc_ctype_1                 0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000013)
    __rt_lib_init_lc_monetary_1              0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000015)
    __rt_lib_init_lc_numeric_1               0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000017)
    __rt_lib_init_lc_time_1                  0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000019)
    __rt_lib_init_preinit_1                  0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000004)
    __rt_lib_init_rand_1                     0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000E)
    __rt_lib_init_return                     0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000033)
    __rt_lib_init_signal_1                   0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001D)
    __rt_lib_init_stdio_1                    0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000025)
    __rt_lib_init_user_alloc_1               0x080001af   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000C)
    __rt_lib_shutdown                        0x080001b1   Thumb Code     0  libshutdown.o(.ARM.Collect$$libshutdown$$00000000)
    __rt_lib_shutdown_fp_trap_1              0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000006)
    __rt_lib_shutdown_heap_1                 0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E)
    __rt_lib_shutdown_return                 0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F)
    __rt_lib_shutdown_signal_1               0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000009)
    __rt_lib_shutdown_stdio_1                0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000003)
    __rt_lib_shutdown_user_alloc_1           0x080001b3   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B)
    __rt_entry                               0x080001b5   Thumb Code     0  __rtentry.o(.ARM.Collect$$rtentry$$00000000)
    __rt_entry_presh_1                       0x080001b5   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$00000002)
    __rt_entry_sh                            0x080001b5   Thumb Code     0  __rtentry4.o(.ARM.Collect$$rtentry$$00000004)
    __rt_entry_li                            0x080001bb   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000A)
    __rt_entry_postsh_1                      0x080001bb   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$00000009)
    __rt_entry_main                          0x080001bf   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000D)
    __rt_entry_postli_1                      0x080001bf   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000C)
    __rt_exit                                0x080001c7   Thumb Code     0  rtexit.o(.ARM.Collect$$rtexit$$00000000)
    __rt_exit_ls                             0x080001c9   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000003)
    __rt_exit_prels_1                        0x080001c9   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000002)
    __rt_exit_exit                           0x080001cd   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000004)
    Reset_Handler                            0x080001d5   Thumb Code     8  startup_stm32wle5xx.o(.text)
    ADC_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    AES_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    COMP_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DAC_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel1_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel2_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel3_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel4_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel6_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA1_Channel7_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel1_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel2_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel3_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel4_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel5_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel6_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMA2_Channel7_IRQHandler                 0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    DMAMUX1_OVR_IRQHandler                   0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI15_10_IRQHandler                     0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI1_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI2_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI3_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI4_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    EXTI9_5_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    FLASH_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    HSEM_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C1_ER_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C1_EV_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C2_ER_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C2_EV_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C3_ER_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    I2C3_EV_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    LPTIM1_IRQHandler                        0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    LPTIM2_IRQHandler                        0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    LPTIM3_IRQHandler                        0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    LPUART1_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    PKA_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    PVD_PVM_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    RCC_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    RNG_IRQHandler                           0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    RTC_WKUP_IRQHandler                      0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    SPI1_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    SPI2_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    SUBGHZSPI_IRQHandler                     0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM16_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM17_IRQHandler                         0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM1_BRK_IRQHandler                      0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM1_CC_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM1_TRG_COM_IRQHandler                  0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM1_UP_IRQHandler                       0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    TIM2_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    USART1_IRQHandler                        0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    WWDG_IRQHandler                          0x080001ef   Thumb Code     0  startup_stm32wle5xx.o(.text)
    __user_initial_stackheap                 0x080001f1   Thumb Code     0  startup_stm32wle5xx.o(.text)
    __aeabi_uldivmod                         0x08000215   Thumb Code     0  lludivv7m.o(.text)
    _ll_udiv                                 0x08000215   Thumb Code   238  lludivv7m.o(.text)
    strlen                                   0x08000303   Thumb Code    62  strlen.o(.text)
    strncmp                                  0x08000341   Thumb Code   150  strncmp.o(.text)
    __aeabi_memcpy                           0x080003d7   Thumb Code     0  rt_memcpy_v6.o(.text)
    __rt_memcpy                              0x080003d7   Thumb Code   138  rt_memcpy_v6.o(.text)
    _memcpy_lastbytes                        0x0800043d   Thumb Code     0  rt_memcpy_v6.o(.text)
    __aeabi_memclr                           0x08000461   Thumb Code     0  rt_memclr.o(.text)
    __rt_memclr                              0x08000461   Thumb Code    68  rt_memclr.o(.text)
    _memset                                  0x08000465   Thumb Code     0  rt_memclr.o(.text)
    __aeabi_memclr4                          0x080004a5   Thumb Code     0  rt_memclr_w.o(.text)
    __aeabi_memclr8                          0x080004a5   Thumb Code     0  rt_memclr_w.o(.text)
    __rt_memclr_w                            0x080004a5   Thumb Code    78  rt_memclr_w.o(.text)
    _memset_w                                0x080004a9   Thumb Code     0  rt_memclr_w.o(.text)
    __use_two_region_memory                  0x080004f3   Thumb Code     2  heapauxi.o(.text)
    __rt_heap_escrow$2region                 0x080004f5   Thumb Code     2  heapauxi.o(.text)
    __rt_heap_expand$2region                 0x080004f7   Thumb Code     2  heapauxi.o(.text)
    __aeabi_memcpy4                          0x080004f9   Thumb Code     0  rt_memcpy_w.o(.text)
    __aeabi_memcpy8                          0x080004f9   Thumb Code     0  rt_memcpy_w.o(.text)
    __rt_memcpy_w                            0x080004f9   Thumb Code   100  rt_memcpy_w.o(.text)
    _memcpy_lastbytes_aligned                0x08000541   Thumb Code     0  rt_memcpy_w.o(.text)
    __user_setup_stackheap                   0x0800055d   Thumb Code    74  sys_stackheap_outer.o(.text)
    exit                                     0x080005a7   Thumb Code    12  exit.o(.text)
    __user_libspace                          0x080005b5   Thumb Code     8  libspace.o(.text)
    __user_perproc_libspace                  0x080005b5   Thumb Code     0  libspace.o(.text)
    __user_perthread_libspace                0x080005b5   Thumb Code     0  libspace.o(.text)
    _sys_exit                                0x080005bd   Thumb Code     8  sys_exit.o(.text)
    __I$use$semihosting                      0x080005c9   Thumb Code     0  use_no_semi.o(.text)
    __use_no_semihosting_swi                 0x080005c9   Thumb Code     2  use_no_semi.o(.text)
    __semihosting_library_function           0x080005cb   Thumb Code     0  indicate_semi.o(.text)
    BSP_LED_Init                             0x080005cd   Thumb Code    72  stm32wlxx_lm40x.o(i.BSP_LED_Init)
    BSP_LED_Toggle                           0x0800061d   Thumb Code    22  stm32wlxx_lm40x.o(i.BSP_LED_Toggle)
    BSP_PB_Callback                          0x0800063d   Thumb Code     2  stm32wlxx_lm40x.o(i.BSP_PB_Callback)
    BSP_PB_Init                              0x08000641   Thumb Code   152  stm32wlxx_lm40x.o(i.BSP_PB_Init)
    BSP_RADIO_ConfigRFSwitch                 0x080006e5   Thumb Code    68  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_ConfigRFSwitch)
    BSP_RADIO_GetRFOMaxPowerConfig           0x08000729   Thumb Code    10  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetRFOMaxPowerConfig)
    BSP_RADIO_GetTxConfig                    0x08000733   Thumb Code     4  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_GetTxConfig)
    BSP_RADIO_Init                           0x08000737   Thumb Code    92  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_Init)
    BSP_RADIO_IsDCDC                         0x08000793   Thumb Code     4  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsDCDC)
    BSP_RADIO_IsTCXO                         0x08000797   Thumb Code     4  stm32wlxx_lm40x_radio.o(i.BSP_RADIO_IsTCXO)
    BusFault_Handler                         0x080007b9   Thumb Code     2  stm32wlxx_it.o(i.BusFault_Handler)
    DMA1_Channel5_IRQHandler                 0x080007bd   Thumb Code     6  stm32wlxx_it.o(i.DMA1_Channel5_IRQHandler)
    DebugMon_Handler                         0x0800087b   Thumb Code     2  stm32wlxx_it.o(i.DebugMon_Handler)
    EXTI0_IRQHandler                         0x0800087d   Thumb Code     6  stm32wlxx_it.o(i.EXTI0_IRQHandler)
    Error_Handler                            0x08000883   Thumb Code     4  main.o(i.Error_Handler)
    HAL_DMA_Abort                            0x0800089d   Thumb Code   110  stm32wlxx_hal_dma.o(i.HAL_DMA_Abort)
    HAL_DMA_Abort_IT                         0x0800090b   Thumb Code   112  stm32wlxx_hal_dma.o(i.HAL_DMA_Abort_IT)
    HAL_DMA_DeInit                           0x0800097d   Thumb Code   154  stm32wlxx_hal_dma.o(i.HAL_DMA_DeInit)
    HAL_DMA_IRQHandler                       0x08000a25   Thumb Code   206  stm32wlxx_hal_dma.o(i.HAL_DMA_IRQHandler)
    HAL_DMA_Init                             0x08000afd   Thumb Code   188  stm32wlxx_hal_dma.o(i.HAL_DMA_Init)
    HAL_DMA_Start_IT                         0x08000bc5   Thumb Code   144  stm32wlxx_hal_dma.o(i.HAL_DMA_Start_IT)
    HAL_Delay                                0x08000c55   Thumb Code    10  sys_app.o(i.HAL_Delay)
    HAL_EXTI_GetHandle                       0x08000c5f   Thumb Code    12  stm32wlxx_hal_exti.o(i.HAL_EXTI_GetHandle)
    HAL_EXTI_RegisterCallback                0x08000c6b   Thumb Code    14  stm32wlxx_hal_exti.o(i.HAL_EXTI_RegisterCallback)
    HAL_GPIO_DeInit                          0x08000c79   Thumb Code   224  stm32wlxx_hal_gpio.o(i.HAL_GPIO_DeInit)
    HAL_GPIO_EXTI_Callback                   0x08000d69   Thumb Code    44  subghz_phy_app.o(i.HAL_GPIO_EXTI_Callback)
    HAL_GPIO_EXTI_IRQHandler                 0x08000db5   Thumb Code    18  stm32wlxx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler)
    HAL_GPIO_Init                            0x08000dcd   Thumb Code   334  stm32wlxx_hal_gpio.o(i.HAL_GPIO_Init)
    HAL_GPIO_TogglePin                       0x08000f2d   Thumb Code    16  stm32wlxx_hal_gpio.o(i.HAL_GPIO_TogglePin)
    HAL_GPIO_WritePin                        0x08000f3d   Thumb Code    10  stm32wlxx_hal_gpio.o(i.HAL_GPIO_WritePin)
    HAL_GetTick                              0x08000f49   Thumb Code    16  sys_app.o(i.HAL_GetTick)
    HAL_Init                                 0x08000f5d   Thumb Code    38  stm32wlxx_hal.o(i.HAL_Init)
    HAL_InitTick                             0x08000f89   Thumb Code     4  sys_app.o(i.HAL_InitTick)
    HAL_MspInit                              0x08000f8d   Thumb Code     2  stm32wlxx_hal_msp.o(i.HAL_MspInit)
    HAL_NVIC_DisableIRQ                      0x08000f8f   Thumb Code    34  stm32wlxx_hal_cortex.o(i.HAL_NVIC_DisableIRQ)
    HAL_NVIC_EnableIRQ                       0x08000fb1   Thumb Code    26  stm32wlxx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    HAL_NVIC_SetPriority                     0x08000fcd   Thumb Code    60  stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    HAL_NVIC_SetPriorityGrouping             0x0800100d   Thumb Code    26  stm32wlxx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping)
    HAL_PWREx_GetVoltageRange                0x08001031   Thumb Code    10  stm32wlxx_hal_pwr_ex.o(i.HAL_PWREx_GetVoltageRange)
    HAL_PWR_EnableBkUpAccess                 0x08001041   Thumb Code    12  stm32wlxx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess)
    HAL_RCCEx_PeriphCLKConfig                0x08001051   Thumb Code   410  stm32wlxx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig)
    HAL_RCC_ClockConfig                      0x080011f1   Thumb Code   442  stm32wlxx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    HAL_RCC_GetHCLKFreq                      0x080013b9   Thumb Code    30  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq)
    HAL_RCC_GetPCLK1Freq                     0x080013dd   Thumb Code    28  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    HAL_RCC_GetPCLK2Freq                     0x080013fd   Thumb Code    28  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    HAL_RCC_GetSysClockFreq                  0x0800141d   Thumb Code   218  stm32wlxx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    HAL_RCC_OscConfig                        0x08001501   Thumb Code  1294  stm32wlxx_hal_rcc.o(i.HAL_RCC_OscConfig)
    HAL_RTCEx_AlarmBEventCallback            0x08001a0f   Thumb Code     2  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_AlarmBEventCallback)
    HAL_RTCEx_BKUPRead                       0x08001a11   Thumb Code     8  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead)
    HAL_RTCEx_BKUPWrite                      0x08001a1d   Thumb Code     8  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite)
    HAL_RTCEx_EnableBypassShadow             0x08001a29   Thumb Code    60  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_EnableBypassShadow)
    HAL_RTCEx_SSRUEventCallback              0x08001a69   Thumb Code    16  timer_if.o(i.HAL_RTCEx_SSRUEventCallback)
    HAL_RTCEx_SSRUIRQHandler                 0x08001a79   Thumb Code    34  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SSRUIRQHandler)
    HAL_RTCEx_SetSSRU_IT                     0x08001aa1   Thumb Code    70  stm32wlxx_hal_rtc_ex.o(i.HAL_RTCEx_SetSSRU_IT)
    HAL_RTC_AlarmAEventCallback              0x08001af1   Thumb Code     4  timer_if.o(i.HAL_RTC_AlarmAEventCallback)
    HAL_RTC_AlarmIRQHandler                  0x08001af5   Thumb Code    54  stm32wlxx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler)
    HAL_RTC_DeactivateAlarm                  0x08001b35   Thumb Code   128  stm32wlxx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm)
    HAL_RTC_Init                             0x08001bb9   Thumb Code   158  stm32wlxx_hal_rtc.o(i.HAL_RTC_Init)
    HAL_RTC_MspInit                          0x08001c61   Thumb Code   110  rtc.o(i.HAL_RTC_MspInit)
    HAL_RTC_SetAlarm_IT                      0x08001cd5   Thumb Code   370  stm32wlxx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT)
    HAL_RTC_WaitForSynchro                   0x08001e51   Thumb Code    48  stm32wlxx_hal_rtc.o(i.HAL_RTC_WaitForSynchro)
    HAL_SUBGHZ_CADStatusCallback             0x08001e85   Thumb Code    20  radio_driver.o(i.HAL_SUBGHZ_CADStatusCallback)
    HAL_SUBGHZ_CRCErrorCallback              0x08001e9d   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_CRCErrorCallback)
    HAL_SUBGHZ_ExecGetCmd                    0x08001ea9   Thumb Code   112  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecGetCmd)
    HAL_SUBGHZ_ExecSetCmd                    0x08001f19   Thumb Code   122  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ExecSetCmd)
    HAL_SUBGHZ_HeaderErrorCallback           0x08001f95   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_HeaderErrorCallback)
    HAL_SUBGHZ_HeaderValidCallback           0x08001fa1   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_HeaderValidCallback)
    HAL_SUBGHZ_IRQHandler                    0x08001fad   Thumb Code   148  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_IRQHandler)
    HAL_SUBGHZ_Init                          0x08002041   Thumb Code   150  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_Init)
    HAL_SUBGHZ_MspInit                       0x080020e5   Thumb Code    42  subghz.o(i.HAL_SUBGHZ_MspInit)
    HAL_SUBGHZ_PreambleDetectedCallback      0x08002111   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_PreambleDetectedCallback)
    HAL_SUBGHZ_ReadBuffer                    0x0800211d   Thumb Code   120  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadBuffer)
    HAL_SUBGHZ_ReadRegisters                 0x08002195   Thumb Code   128  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_ReadRegisters)
    HAL_SUBGHZ_RxCpltCallback                0x08002215   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_RxCpltCallback)
    HAL_SUBGHZ_RxTxTimeoutCallback           0x08002221   Thumb Code    10  radio_driver.o(i.HAL_SUBGHZ_RxTxTimeoutCallback)
    HAL_SUBGHZ_SyncWordValidCallback         0x08002231   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_SyncWordValidCallback)
    HAL_SUBGHZ_TxCpltCallback                0x0800223d   Thumb Code     8  radio_driver.o(i.HAL_SUBGHZ_TxCpltCallback)
    HAL_SUBGHZ_WriteBuffer                   0x08002249   Thumb Code   110  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteBuffer)
    HAL_SUBGHZ_WriteRegisters                0x080022b7   Thumb Code   122  stm32wlxx_hal_subghz.o(i.HAL_SUBGHZ_WriteRegisters)
    HAL_UARTEx_EnableFifoMode                0x08002331   Thumb Code    74  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableFifoMode)
    HAL_UARTEx_EnableStopMode                0x0800237b   Thumb Code    46  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_EnableStopMode)
    HAL_UARTEx_RxEventCallback               0x080023a9   Thumb Code     2  stm32wlxx_hal_uart.o(i.HAL_UARTEx_RxEventCallback)
    HAL_UARTEx_RxFifoFullCallback            0x080023ab   Thumb Code     2  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_RxFifoFullCallback)
    HAL_UARTEx_SetRxFifoThreshold            0x080023ad   Thumb Code    76  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetRxFifoThreshold)
    HAL_UARTEx_SetTxFifoThreshold            0x080023f9   Thumb Code    76  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_SetTxFifoThreshold)
    HAL_UARTEx_StopModeWakeUpSourceConfig    0x08002445   Thumb Code   138  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_StopModeWakeUpSourceConfig)
    HAL_UARTEx_TxFifoEmptyCallback           0x080024cf   Thumb Code     2  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_TxFifoEmptyCallback)
    HAL_UARTEx_WakeupCallback                0x080024d1   Thumb Code     2  stm32wlxx_hal_uart_ex.o(i.HAL_UARTEx_WakeupCallback)
    HAL_UART_ErrorCallback                   0x080024d3   Thumb Code     2  stm32wlxx_hal_uart.o(i.HAL_UART_ErrorCallback)
    HAL_UART_IRQHandler                      0x080024d5   Thumb Code   722  stm32wlxx_hal_uart.o(i.HAL_UART_IRQHandler)
    HAL_UART_Init                            0x080027b5   Thumb Code   106  stm32wlxx_hal_uart.o(i.HAL_UART_Init)
    HAL_UART_MspDeInit                       0x08002821   Thumb Code    52  usart.o(i.HAL_UART_MspDeInit)
    HAL_UART_MspInit                         0x08002859   Thumb Code   180  usart.o(i.HAL_UART_MspInit)
    HAL_UART_Receive_IT                      0x0800291d   Thumb Code    80  stm32wlxx_hal_uart.o(i.HAL_UART_Receive_IT)
    HAL_UART_RxCpltCallback                  0x08002971   Thumb Code    48  usart_if.o(i.HAL_UART_RxCpltCallback)
    HAL_UART_Transmit_DMA                    0x080029a9   Thumb Code   150  stm32wlxx_hal_uart.o(i.HAL_UART_Transmit_DMA)
    HAL_UART_TxCpltCallback                  0x08002a4d   Thumb Code    18  usart_if.o(i.HAL_UART_TxCpltCallback)
    HAL_UART_TxHalfCpltCallback              0x08002a69   Thumb Code     2  stm32wlxx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback)
    HardFault_Handler                        0x08002a6b   Thumb Code     2  stm32wlxx_it.o(i.HardFault_Handler)
    MX_DMA_Init                              0x08002bb3   Thumb Code    34  dma.o(i.MX_DMA_Init)
    MX_GPIO_Init                             0x08002bd5   Thumb Code   104  gpio.o(i.MX_GPIO_Init)
    MX_RTC_Init                              0x08002c41   Thumb Code   100  rtc.o(i.MX_RTC_Init)
    MX_SUBGHZ_Init                           0x08002cad   Thumb Code    28  subghz.o(i.MX_SUBGHZ_Init)
    MX_SubGHz_Phy_Init                       0x08002ccd   Thumb Code    14  app_subghz_phy.o(i.MX_SubGHz_Phy_Init)
    MX_USART2_UART_Init                      0x08002cdd   Thumb Code    94  usart.o(i.MX_USART2_UART_Init)
    MemManage_Handler                        0x08002d45   Thumb Code     2  stm32wlxx_it.o(i.MemManage_Handler)
    NMI_Handler                              0x08002d47   Thumb Code     2  stm32wlxx_it.o(i.NMI_Handler)
    PendSV_Handler                           0x08002f91   Thumb Code     2  stm32wlxx_it.o(i.PendSV_Handler)
    RBI_ConfigRFSwitch                       0x08003165   Thumb Code     4  radio_board_if.o(i.RBI_ConfigRFSwitch)
    RBI_GetRFOMaxPowerConfig                 0x08003169   Thumb Code     4  radio_board_if.o(i.RBI_GetRFOMaxPowerConfig)
    RBI_GetTxConfig                          0x0800316d   Thumb Code     4  radio_board_if.o(i.RBI_GetTxConfig)
    RBI_Init                                 0x08003171   Thumb Code     4  radio_board_if.o(i.RBI_Init)
    RBI_IsDCDC                               0x08003175   Thumb Code     4  radio_board_if.o(i.RBI_IsDCDC)
    RBI_IsTCXO                               0x08003179   Thumb Code     4  radio_board_if.o(i.RBI_IsTCXO)
    RFW_DeInit                               0x0800324d   Thumb Code     2  radio_fw.o(i.RFW_DeInit)
    RFW_DeInit_TxLongPacket                  0x0800324f   Thumb Code     2  radio_fw.o(i.RFW_DeInit_TxLongPacket)
    RFW_Init                                 0x08003251   Thumb Code     6  radio_fw.o(i.RFW_Init)
    RFW_Is_Init                              0x08003257   Thumb Code     4  radio_fw.o(i.RFW_Is_Init)
    RFW_Is_LongPacketModeEnabled             0x0800325b   Thumb Code     4  radio_fw.o(i.RFW_Is_LongPacketModeEnabled)
    RFW_ReceiveInit                          0x0800325f   Thumb Code     6  radio_fw.o(i.RFW_ReceiveInit)
    RFW_ReceiveLongPacket                    0x08003265   Thumb Code     6  radio_fw.o(i.RFW_ReceiveLongPacket)
    RFW_ReceivePayload                       0x0800326b   Thumb Code     2  radio_fw.o(i.RFW_ReceivePayload)
    RFW_SetAntSwitch                         0x0800326d   Thumb Code     2  radio_fw.o(i.RFW_SetAntSwitch)
    RFW_SetRadioModem                        0x0800326f   Thumb Code     2  radio_fw.o(i.RFW_SetRadioModem)
    RFW_TransmitInit                         0x08003271   Thumb Code     6  radio_fw.o(i.RFW_TransmitInit)
    RFW_TransmitLongPacket                   0x08003277   Thumb Code     6  radio_fw.o(i.RFW_TransmitLongPacket)
    RTC_Alarm_IRQHandler                     0x0800327d   Thumb Code     6  stm32wlxx_it.o(i.RTC_Alarm_IRQHandler)
    RTC_ByteToBcd2                           0x08003289   Thumb Code    22  stm32wlxx_hal_rtc.o(i.RTC_ByteToBcd2)
    RTC_EnterInitMode                        0x080032a1   Thumb Code    72  stm32wlxx_hal_rtc.o(i.RTC_EnterInitMode)
    RTC_ExitInitMode                         0x080032ed   Thumb Code    84  stm32wlxx_hal_rtc.o(i.RTC_ExitInitMode)
    SEQ_BitPosition                          0x080045d9   Thumb Code    46  stm32_seq.o(i.SEQ_BitPosition)
    SUBGHZSPI_Init                           0x0800460d   Thumb Code    32  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Init)
    SUBGHZSPI_Receive                        0x08004631   Thumb Code    82  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Receive)
    SUBGHZSPI_Transmit                       0x0800468d   Thumb Code    78  stm32wlxx_hal_subghz.o(i.SUBGHZSPI_Transmit)
    SUBGHZ_CheckDeviceReady                  0x080046e5   Thumb Code    50  stm32wlxx_hal_subghz.o(i.SUBGHZ_CheckDeviceReady)
    SUBGHZ_Radio_IRQHandler                  0x0800471d   Thumb Code     6  stm32wlxx_it.o(i.SUBGHZ_Radio_IRQHandler)
    SUBGHZ_WaitOnBusy                        0x08004729   Thumb Code    62  stm32wlxx_hal_subghz.o(i.SUBGHZ_WaitOnBusy)
    SUBGRF_Calibrate                         0x08004771   Thumb Code    70  radio_driver.o(i.SUBGRF_Calibrate)
    SUBGRF_CalibrateImage                    0x080047b9   Thumb Code    96  radio_driver.o(i.SUBGRF_CalibrateImage)
    SUBGRF_GetCFO                            0x0800482d   Thumb Code   104  radio_driver.o(i.SUBGRF_GetCFO)
    SUBGRF_GetFskBandwidthRegValue           0x080048a1   Thumb Code    36  radio_driver.o(i.SUBGRF_GetFskBandwidthRegValue)
    SUBGRF_GetOperatingMode                  0x080048c9   Thumb Code     6  radio_driver.o(i.SUBGRF_GetOperatingMode)
    SUBGRF_GetPacketStatus                   0x080048d5   Thumb Code   110  radio_driver.o(i.SUBGRF_GetPacketStatus)
    SUBGRF_GetPayload                        0x08004949   Thumb Code    46  radio_driver.o(i.SUBGRF_GetPayload)
    SUBGRF_GetRadioWakeUpTime                0x08004977   Thumb Code     4  radio_driver.o(i.SUBGRF_GetRadioWakeUpTime)
    SUBGRF_GetRandom                         0x0800497b   Thumb Code    94  radio_driver.o(i.SUBGRF_GetRandom)
    SUBGRF_GetRssiInst                       0x080049d9   Thumb Code    24  radio_driver.o(i.SUBGRF_GetRssiInst)
    SUBGRF_GetRxBufferStatus                 0x080049f1   Thumb Code    54  radio_driver.o(i.SUBGRF_GetRxBufferStatus)
    SUBGRF_Init                              0x08004a2d   Thumb Code    88  radio_driver.o(i.SUBGRF_Init)
    SUBGRF_ReadBuffer                        0x08004a89   Thumb Code    26  radio_driver.o(i.SUBGRF_ReadBuffer)
    SUBGRF_ReadRegister                      0x08004ac9   Thumb Code    20  radio_driver.o(i.SUBGRF_ReadRegister)
    SUBGRF_ReadRegisters                     0x08004ae1   Thumb Code    26  radio_driver.o(i.SUBGRF_ReadRegisters)
    SUBGRF_SendPayload                       0x08004b01   Thumb Code    18  radio_driver.o(i.SUBGRF_SendPayload)
    SUBGRF_SetBufferBaseAddress              0x08004b13   Thumb Code    22  radio_driver.o(i.SUBGRF_SetBufferBaseAddress)
    SUBGRF_SetCad                            0x08004b29   Thumb Code    20  radio_driver.o(i.SUBGRF_SetCad)
    SUBGRF_SetCrcPolynomial                  0x08004b41   Thumb Code    34  radio_driver.o(i.SUBGRF_SetCrcPolynomial)
    SUBGRF_SetCrcSeed                        0x08004b69   Thumb Code    34  radio_driver.o(i.SUBGRF_SetCrcSeed)
    SUBGRF_SetDioIrqParams                   0x08004b91   Thumb Code    54  radio_driver.o(i.SUBGRF_SetDioIrqParams)
    SUBGRF_SetLoRaSymbNumTimeout             0x08004bc7   Thumb Code    52  radio_driver.o(i.SUBGRF_SetLoRaSymbNumTimeout)
    SUBGRF_SetModulationParams               0x08004bfd   Thumb Code   214  radio_driver.o(i.SUBGRF_SetModulationParams)
    SUBGRF_SetPaConfig                       0x08004ce1   Thumb Code    30  radio_driver.o(i.SUBGRF_SetPaConfig)
    SUBGRF_SetPacketParams                   0x08004d01   Thumb Code   210  radio_driver.o(i.SUBGRF_SetPacketParams)
    SUBGRF_SetPacketType                     0x08004dd9   Thumb Code    34  radio_driver.o(i.SUBGRF_SetPacketType)
    SUBGRF_SetPayload                        0x08004e01   Thumb Code    10  radio_driver.o(i.SUBGRF_SetPayload)
    SUBGRF_SetRegulatorMode                  0x08004e0b   Thumb Code    28  radio_driver.o(i.SUBGRF_SetRegulatorMode)
    SUBGRF_SetRfFrequency                    0x08004e29   Thumb Code    66  radio_driver.o(i.SUBGRF_SetRfFrequency)
    SUBGRF_SetRfTxPower                      0x08004e75   Thumb Code    42  radio_driver.o(i.SUBGRF_SetRfTxPower)
    SUBGRF_SetRx                             0x08004ea1   Thumb Code    36  radio_driver.o(i.SUBGRF_SetRx)
    SUBGRF_SetRxBoosted                      0x08004ec9   Thumb Code    48  radio_driver.o(i.SUBGRF_SetRxBoosted)
    SUBGRF_SetRxDutyCycle                    0x08004efd   Thumb Code    52  radio_driver.o(i.SUBGRF_SetRxDutyCycle)
    SUBGRF_SetSleep                          0x08004f35   Thumb Code    58  radio_driver.o(i.SUBGRF_SetSleep)
    SUBGRF_SetStandby                        0x08004f75   Thumb Code    30  radio_driver.o(i.SUBGRF_SetStandby)
    SUBGRF_SetStopRxTimerOnPreambleDetect    0x08004f99   Thumb Code    14  radio_driver.o(i.SUBGRF_SetStopRxTimerOnPreambleDetect)
    SUBGRF_SetSwitch                         0x08004fa7   Thumb Code    40  radio_driver.o(i.SUBGRF_SetSwitch)
    SUBGRF_SetSyncWord                       0x08004fcf   Thumb Code    18  radio_driver.o(i.SUBGRF_SetSyncWord)
    SUBGRF_SetTcxoMode                       0x08004fe1   Thumb Code    38  radio_driver.o(i.SUBGRF_SetTcxoMode)
    SUBGRF_SetTx                             0x08005009   Thumb Code    36  radio_driver.o(i.SUBGRF_SetTx)
    SUBGRF_SetTxContinuousWave               0x08005031   Thumb Code    10  radio_driver.o(i.SUBGRF_SetTxContinuousWave)
    SUBGRF_SetTxInfinitePreamble             0x0800503b   Thumb Code    10  radio_driver.o(i.SUBGRF_SetTxInfinitePreamble)
    SUBGRF_SetTxParams                       0x08005045   Thumb Code   270  radio_driver.o(i.SUBGRF_SetTxParams)
    SUBGRF_SetWhiteningSeed                  0x08005155   Thumb Code    52  radio_driver.o(i.SUBGRF_SetWhiteningSeed)
    SUBGRF_WriteBuffer                       0x0800518d   Thumb Code    26  radio_driver.o(i.SUBGRF_WriteBuffer)
    SUBGRF_WriteRegister                     0x080051cd   Thumb Code    16  radio_driver.o(i.SUBGRF_WriteRegister)
    SUBGRF_WriteRegisters                    0x080051e1   Thumb Code    26  radio_driver.o(i.SUBGRF_WriteRegisters)
    SVC_Handler                              0x08005201   Thumb Code     2  stm32wlxx_it.o(i.SVC_Handler)
    SubghzApp_Init                           0x08005205   Thumb Code   350  subghz_phy_app.o(i.SubghzApp_Init)
    SysTick_Handler                          0x08005449   Thumb Code     2  stm32wlxx_it.o(i.SysTick_Handler)
    SysTimeAdd                               0x0800544b   Thumb Code    38  stm32_systime.o(i.SysTimeAdd)
    SysTimeGet                               0x08005471   Thumb Code    62  stm32_systime.o(i.SysTimeGet)
    SystemApp_Init                           0x080054b5   Thumb Code    64  sys_app.o(i.SystemApp_Init)
    SystemClock_Config                       0x080054fd   Thumb Code   128  main.o(i.SystemClock_Config)
    SystemInit                               0x08005581   Thumb Code     2  system_stm32wlxx.o(i.SystemInit)
    TAMP_STAMP_LSECSS_SSRU_IRQHandler        0x08005585   Thumb Code     6  stm32wlxx_it.o(i.TAMP_STAMP_LSECSS_SSRU_IRQHandler)
    TIMER_IF_BkUp_Read_Seconds               0x0800559d   Thumb Code     8  timer_if.o(i.TIMER_IF_BkUp_Read_Seconds)
    TIMER_IF_BkUp_Read_SubSeconds            0x080055a9   Thumb Code     8  timer_if.o(i.TIMER_IF_BkUp_Read_SubSeconds)
    TIMER_IF_BkUp_Write_Seconds              0x080055c5   Thumb Code    10  timer_if.o(i.TIMER_IF_BkUp_Write_Seconds)
    TIMER_IF_BkUp_Write_SubSeconds           0x080055d5   Thumb Code    10  timer_if.o(i.TIMER_IF_BkUp_Write_SubSeconds)
    TIMER_IF_Convert_Tick2ms                 0x080055e5   Thumb Code    16  timer_if.o(i.TIMER_IF_Convert_Tick2ms)
    TIMER_IF_Convert_ms2Tick                 0x080055f5   Thumb Code    18  timer_if.o(i.TIMER_IF_Convert_ms2Tick)
    TIMER_IF_DelayMs                         0x08005607   Thumb Code    30  timer_if.o(i.TIMER_IF_DelayMs)
    TIMER_IF_GetMinimumTimeout               0x08005625   Thumb Code     4  timer_if.o(i.TIMER_IF_GetMinimumTimeout)
    TIMER_IF_GetTime                         0x08005629   Thumb Code    40  timer_if.o(i.TIMER_IF_GetTime)
    TIMER_IF_GetTimerContext                 0x08005651   Thumb Code     6  timer_if.o(i.TIMER_IF_GetTimerContext)
    TIMER_IF_GetTimerElapsedTime             0x0800565d   Thumb Code    14  timer_if.o(i.TIMER_IF_GetTimerElapsedTime)
    TIMER_IF_GetTimerValue                   0x08005671   Thumb Code    16  timer_if.o(i.TIMER_IF_GetTimerValue)
    TIMER_IF_Init                            0x08005685   Thumb Code    64  timer_if.o(i.TIMER_IF_Init)
    TIMER_IF_SetTimerContext                 0x080056cd   Thumb Code    12  timer_if.o(i.TIMER_IF_SetTimerContext)
    TIMER_IF_StartTimer                      0x080056dd   Thumb Code    68  timer_if.o(i.TIMER_IF_StartTimer)
    TIMER_IF_StopTimer                       0x08005729   Thumb Code    28  timer_if.o(i.TIMER_IF_StopTimer)
    TimerExists                              0x080058f9   Thumb Code    24  stm32_timer.o(i.TimerExists)
    TimerInsertNewHeadTimer                  0x08005915   Thumb Code    18  stm32_timer.o(i.TimerInsertNewHeadTimer)
    TimerInsertTimer                         0x0800592d   Thumb Code    34  stm32_timer.o(i.TimerInsertTimer)
    TimerSetTimeout                          0x08005955   Thumb Code    48  stm32_timer.o(i.TimerSetTimeout)
    UART_AdvFeatureConfig                    0x08005a01   Thumb Code   200  stm32wlxx_hal_uart.o(i.UART_AdvFeatureConfig)
    UART_CheckIdleState                      0x08005ac9   Thumb Code    96  stm32wlxx_hal_uart.o(i.UART_CheckIdleState)
    UART_SetConfig                           0x08006081   Thumb Code   552  stm32wlxx_hal_uart.o(i.UART_SetConfig)
    UART_Start_Receive_IT                    0x080062c9   Thumb Code   262  stm32wlxx_hal_uart.o(i.UART_Start_Receive_IT)
    UART_WaitOnFlagUntilTimeout              0x080063e1   Thumb Code   196  stm32wlxx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    USART2_IRQHandler                        0x080064a5   Thumb Code     6  stm32wlxx_it.o(i.USART2_IRQHandler)
    UTIL_ADV_TRACE_COND_FSend                0x080064b1   Thumb Code   170  stm32_adv_trace.o(i.UTIL_ADV_TRACE_COND_FSend)
    UTIL_ADV_TRACE_Init                      0x08006565   Thumb Code    38  stm32_adv_trace.o(i.UTIL_ADV_TRACE_Init)
    UTIL_ADV_TRACE_PostSendHook              0x08006599   Thumb Code     8  sys_app.o(i.UTIL_ADV_TRACE_PostSendHook)
    UTIL_ADV_TRACE_PreSendHook               0x080065a1   Thumb Code     8  sys_app.o(i.UTIL_ADV_TRACE_PreSendHook)
    UTIL_ADV_TRACE_RegisterTimeStampFunction 0x080065a9   Thumb Code     6  stm32_adv_trace.o(i.UTIL_ADV_TRACE_RegisterTimeStampFunction)
    UTIL_ADV_TRACE_SetVerboseLevel           0x080065b5   Thumb Code     6  stm32_adv_trace.o(i.UTIL_ADV_TRACE_SetVerboseLevel)
    UTIL_LPM_Init                            0x080065c1   Thumb Code    10  stm32_lpm.o(i.UTIL_LPM_Init)
    UTIL_LPM_SetOffMode                      0x080065d1   Thumb Code    32  stm32_lpm.o(i.UTIL_LPM_SetOffMode)
    UTIL_LPM_SetStopMode                     0x080065f5   Thumb Code    32  stm32_lpm.o(i.UTIL_LPM_SetStopMode)
    UTIL_MEM_cpy_8                           0x08006619   Thumb Code    18  stm32_mem.o(i.UTIL_MEM_cpy_8)
    UTIL_MEM_set_8                           0x0800662b   Thumb Code    14  stm32_mem.o(i.UTIL_MEM_set_8)
    UTIL_SEQ_RegTask                         0x08006639   Thumb Code    26  stm32_seq.o(i.UTIL_SEQ_RegTask)
    UTIL_SEQ_SetTask                         0x08006659   Thumb Code    34  stm32_seq.o(i.UTIL_SEQ_SetTask)
    UTIL_TIMER_Create                        0x08006681   Thumb Code    56  stm32_timer.o(i.UTIL_TIMER_Create)
    UTIL_TIMER_GetCurrentTime                0x080066bd   Thumb Code    16  stm32_timer.o(i.UTIL_TIMER_GetCurrentTime)
    UTIL_TIMER_GetElapsedTime                0x080066d1   Thumb Code    28  stm32_timer.o(i.UTIL_TIMER_GetElapsedTime)
    UTIL_TIMER_IRQ_Handler                   0x080066f1   Thumb Code   128  stm32_timer.o(i.UTIL_TIMER_IRQ_Handler)
    UTIL_TIMER_Init                          0x08006779   Thumb Code    12  stm32_timer.o(i.UTIL_TIMER_Init)
    UTIL_TIMER_SetPeriod                     0x0800678d   Thumb Code    50  stm32_timer.o(i.UTIL_TIMER_SetPeriod)
    UTIL_TIMER_Start                         0x080067c5   Thumb Code   116  stm32_timer.o(i.UTIL_TIMER_Start)
    UTIL_TIMER_Stop                          0x08006841   Thumb Code    94  stm32_timer.o(i.UTIL_TIMER_Stop)
    UsageFault_Handler                       0x080068a9   Thumb Code     2  stm32wlxx_it.o(i.UsageFault_Handler)
    main                                     0x080069bd   Thumb Code    18  main.o(i.main)
    tiny_vsnprintf_like                      0x08006a5d   Thumb Code   328  stm32_tiny_vsnprintf.o(i.tiny_vsnprintf_like)
    vcom_DeInit                              0x08006bad   Thumb Code    38  usart_if.o(i.vcom_DeInit)
    vcom_Init                                0x08006bd9   Thumb Code    28  usart_if.o(i.vcom_Init)
    vcom_ReceiveInit                         0x08006bfd   Thumb Code    64  usart_if.o(i.vcom_ReceiveInit)
    vcom_Trace_DMA                           0x08006c45   Thumb Code    16  usart_if.o(i.vcom_Trace_DMA)
    UTIL_TimerDriver                         0x08006c58   Data          44  timer_if.o(.constdata)
    UTIL_SYSTIMDriver                        0x08006c84   Data          20  timer_if.o(.constdata)
    UTIL_TraceDriver                         0x08006c98   Data          16  usart_if.o(.constdata)
    UARTPrescTable                           0x08006cc4   Data          24  stm32wlxx_hal_uart.o(.constdata)
    AHBPrescTable                            0x08006cec   Data          64  system_stm32wlxx.o(.constdata)
    MSIRangeTable                            0x08006d2c   Data          64  system_stm32wlxx.o(.constdata)
    APBPrescTable                            0x08006d6c   Data          32  system_stm32wlxx.o(.constdata)
    Radio                                    0x08006e3c   Data         132  radio.o(.constdata)
    Bandwidths                               0x08006ec0   Data           3  radio.o(.constdata)
    SEQ_clz_table_4bit                       0x08006ec3   Data          16  stm32_seq.o(.constdata)
    Region$$Table$$Base                      0x08006f40   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x08006f60   Number         0  anon$$obj.o(Region$$Table)
    charRx                                   0x2000000c   Data           1  usart_if.o(.data)
    RssiValue                                0x20000019   Data           1  subghz_phy_app.o(.data)
    SnrValue                                 0x2000001a   Data           1  subghz_phy_app.o(.data)
    isMaster                                 0x2000001b   Data           1  subghz_phy_app.o(.data)
    RxBufferSize                             0x2000001c   Data           2  subghz_phy_app.o(.data)
    uwTickFreq                               0x20000024   Data           1  stm32wlxx_hal.o(.data)
    uwTickPrio                               0x20000028   Data           4  stm32wlxx_hal.o(.data)
    uwTick                                   0x2000002c   Data           4  stm32wlxx_hal.o(.data)
    SystemCoreClock                          0x20000030   Data           4  system_stm32wlxx.o(.data)
    FrequencyError                           0x20000038   Data           4  radio_driver.o(.data)
    hrtc                                     0x200000b0   Data          56  rtc.o(.bss)
    hsubghz                                  0x200000e8   Data          12  subghz.o(.bss)
    huart2                                   0x200000f4   Data         144  usart.o(.bss)
    hdma_usart2_tx                           0x20000184   Data          96  usart.o(.bss)
    SubgRf                                   0x20000518   Data          92  radio.o(.bss)
    TxTimeoutTimer                           0x20000574   Data          24  radio.o(.bss)
    RxTimeoutTimer                           0x2000058c   Data          24  radio.o(.bss)
    hpb_exti                                 0x200008bc   Data          24  stm32wlxx_lm40x.o(.bss)
    __libspace_start                         0x200008d4   Data          96  libspace.o(.bss)
    __temporary_stack_top$libspace           0x20000934   Data           0  libspace.o(.bss)



==============================================================================

Memory Map of the image

  Image Entry point : 0x08000139

  Load Region LR_IROM1 (Base: 0x08000000, Size: 0x00007010, Max: 0x00040000, ABSOLUTE)

    Execution Region ER_IROM1 (Base: 0x08000000, Size: 0x00006f60, Max: 0x00040000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x08000000   0x00000138   Data   RO            4    RESET               startup_stm32wle5xx.o
    0x08000138   0x00000008   Code   RO         5690  * !!!main             c_w.l(__main.o)
    0x08000140   0x00000034   Code   RO         5858    !!!scatter          c_w.l(__scatter.o)
    0x08000174   0x0000001a   Code   RO         5860    !!handler_copy      c_w.l(__scatter_copy.o)
    0x0800018e   0x00000002   PAD
    0x08000190   0x0000001c   Code   RO         5862    !!handler_zi        c_w.l(__scatter_zi.o)
    0x080001ac   0x00000002   Code   RO         5729    .ARM.Collect$$libinit$$00000000  c_w.l(libinit.o)
    0x080001ae   0x00000000   Code   RO         5742    .ARM.Collect$$libinit$$00000002  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5744    .ARM.Collect$$libinit$$00000004  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5747    .ARM.Collect$$libinit$$0000000A  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5749    .ARM.Collect$$libinit$$0000000C  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5751    .ARM.Collect$$libinit$$0000000E  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5754    .ARM.Collect$$libinit$$00000011  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5756    .ARM.Collect$$libinit$$00000013  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5758    .ARM.Collect$$libinit$$00000015  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5760    .ARM.Collect$$libinit$$00000017  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5762    .ARM.Collect$$libinit$$00000019  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5764    .ARM.Collect$$libinit$$0000001B  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5766    .ARM.Collect$$libinit$$0000001D  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5768    .ARM.Collect$$libinit$$0000001F  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5770    .ARM.Collect$$libinit$$00000021  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5772    .ARM.Collect$$libinit$$00000023  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5774    .ARM.Collect$$libinit$$00000025  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5778    .ARM.Collect$$libinit$$0000002C  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5780    .ARM.Collect$$libinit$$0000002E  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5782    .ARM.Collect$$libinit$$00000030  c_w.l(libinit2.o)
    0x080001ae   0x00000000   Code   RO         5784    .ARM.Collect$$libinit$$00000032  c_w.l(libinit2.o)
    0x080001ae   0x00000002   Code   RO         5785    .ARM.Collect$$libinit$$00000033  c_w.l(libinit2.o)
    0x080001b0   0x00000002   Code   RO         5816    .ARM.Collect$$libshutdown$$00000000  c_w.l(libshutdown.o)
    0x080001b2   0x00000000   Code   RO         5843    .ARM.Collect$$libshutdown$$00000003  c_w.l(libshutdown2.o)
    0x080001b2   0x00000000   Code   RO         5846    .ARM.Collect$$libshutdown$$00000006  c_w.l(libshutdown2.o)
    0x080001b2   0x00000000   Code   RO         5849    .ARM.Collect$$libshutdown$$00000009  c_w.l(libshutdown2.o)
    0x080001b2   0x00000000   Code   RO         5851    .ARM.Collect$$libshutdown$$0000000B  c_w.l(libshutdown2.o)
    0x080001b2   0x00000000   Code   RO         5854    .ARM.Collect$$libshutdown$$0000000E  c_w.l(libshutdown2.o)
    0x080001b2   0x00000002   Code   RO         5855    .ARM.Collect$$libshutdown$$0000000F  c_w.l(libshutdown2.o)
    0x080001b4   0x00000000   Code   RO         5692    .ARM.Collect$$rtentry$$00000000  c_w.l(__rtentry.o)
    0x080001b4   0x00000000   Code   RO         5700    .ARM.Collect$$rtentry$$00000002  c_w.l(__rtentry2.o)
    0x080001b4   0x00000006   Code   RO         5712    .ARM.Collect$$rtentry$$00000004  c_w.l(__rtentry4.o)
    0x080001ba   0x00000000   Code   RO         5702    .ARM.Collect$$rtentry$$00000009  c_w.l(__rtentry2.o)
    0x080001ba   0x00000004   Code   RO         5703    .ARM.Collect$$rtentry$$0000000A  c_w.l(__rtentry2.o)
    0x080001be   0x00000000   Code   RO         5705    .ARM.Collect$$rtentry$$0000000C  c_w.l(__rtentry2.o)
    0x080001be   0x00000008   Code   RO         5706    .ARM.Collect$$rtentry$$0000000D  c_w.l(__rtentry2.o)
    0x080001c6   0x00000002   Code   RO         5733    .ARM.Collect$$rtexit$$00000000  c_w.l(rtexit.o)
    0x080001c8   0x00000000   Code   RO         5789    .ARM.Collect$$rtexit$$00000002  c_w.l(rtexit2.o)
    0x080001c8   0x00000004   Code   RO         5790    .ARM.Collect$$rtexit$$00000003  c_w.l(rtexit2.o)
    0x080001cc   0x00000006   Code   RO         5791    .ARM.Collect$$rtexit$$00000004  c_w.l(rtexit2.o)
    0x080001d2   0x00000002   PAD
    0x080001d4   0x00000040   Code   RO            5    .text               startup_stm32wle5xx.o
    0x08000214   0x000000ee   Code   RO         5676    .text               c_w.l(lludivv7m.o)
    0x08000302   0x0000003e   Code   RO         5678    .text               c_w.l(strlen.o)
    0x08000340   0x00000096   Code   RO         5680    .text               c_w.l(strncmp.o)
    0x080003d6   0x0000008a   Code   RO         5682    .text               c_w.l(rt_memcpy_v6.o)
    0x08000460   0x00000044   Code   RO         5684    .text               c_w.l(rt_memclr.o)
    0x080004a4   0x0000004e   Code   RO         5686    .text               c_w.l(rt_memclr_w.o)
    0x080004f2   0x00000006   Code   RO         5688    .text               c_w.l(heapauxi.o)
    0x080004f8   0x00000064   Code   RO         5697    .text               c_w.l(rt_memcpy_w.o)
    0x0800055c   0x0000004a   Code   RO         5716    .text               c_w.l(sys_stackheap_outer.o)
    0x080005a6   0x0000000c   Code   RO         5718    .text               c_w.l(exit.o)
    0x080005b2   0x00000002   PAD
    0x080005b4   0x00000008   Code   RO         5730    .text               c_w.l(libspace.o)
    0x080005bc   0x0000000c   Code   RO         5786    .text               c_w.l(sys_exit.o)
    0x080005c8   0x00000002   Code   RO         5805    .text               c_w.l(use_no_semi.o)
    0x080005ca   0x00000000   Code   RO         5807    .text               c_w.l(indicate_semi.o)
    0x080005ca   0x00000002   PAD
    0x080005cc   0x00000050   Code   RO         5497    i.BSP_LED_Init      stm32wlxx_lm40x.o
    0x0800061c   0x00000020   Code   RO         5500    i.BSP_LED_Toggle    stm32wlxx_lm40x.o
    0x0800063c   0x00000002   Code   RO         5501    i.BSP_PB_Callback   stm32wlxx_lm40x.o
    0x0800063e   0x00000002   PAD
    0x08000640   0x000000a4   Code   RO         5505    i.BSP_PB_Init       stm32wlxx_lm40x.o
    0x080006e4   0x00000044   Code   RO         5612    i.BSP_RADIO_ConfigRFSwitch  stm32wlxx_lm40x_radio.o
    0x08000728   0x0000000a   Code   RO         5614    i.BSP_RADIO_GetRFOMaxPowerConfig  stm32wlxx_lm40x_radio.o
    0x08000732   0x00000004   Code   RO         5615    i.BSP_RADIO_GetTxConfig  stm32wlxx_lm40x_radio.o
    0x08000736   0x0000005c   Code   RO         5616    i.BSP_RADIO_Init    stm32wlxx_lm40x_radio.o
    0x08000792   0x00000004   Code   RO         5617    i.BSP_RADIO_IsDCDC  stm32wlxx_lm40x_radio.o
    0x08000796   0x00000004   Code   RO         5618    i.BSP_RADIO_IsTCXO  stm32wlxx_lm40x_radio.o
    0x0800079a   0x0000000a   Code   RO         5506    i.BUTTON_SW1_EXTI_Callback  stm32wlxx_lm40x.o
    0x080007a4   0x0000000a   Code   RO         5507    i.BUTTON_SW2_EXTI_Callback  stm32wlxx_lm40x.o
    0x080007ae   0x0000000a   Code   RO         5508    i.BUTTON_SW3_EXTI_Callback  stm32wlxx_lm40x.o
    0x080007b8   0x00000002   Code   RO          895    i.BusFault_Handler  stm32wlxx_it.o
    0x080007ba   0x00000002   PAD
    0x080007bc   0x0000000c   Code   RO          896    i.DMA1_Channel5_IRQHandler  stm32wlxx_it.o
    0x080007c8   0x0000004c   Code   RO         1837    i.DMA_CalcDMAMUXChannelBaseAndMask  stm32wlxx_hal_dma.o
    0x08000814   0x00000028   Code   RO         1838    i.DMA_CalcDMAMUXRequestGenBaseAndMask  stm32wlxx_hal_dma.o
    0x0800083c   0x0000003e   Code   RO         1839    i.DMA_SetConfig     stm32wlxx_hal_dma.o
    0x0800087a   0x00000002   Code   RO          897    i.DebugMon_Handler  stm32wlxx_it.o
    0x0800087c   0x00000006   Code   RO          898    i.EXTI0_IRQHandler  stm32wlxx_it.o
    0x08000882   0x00000004   Code   RO           14    i.Error_Handler     main.o
    0x08000886   0x00000002   PAD
    0x08000888   0x00000014   Code   RO          601    i.GetTimerTicks     timer_if.o
    0x0800089c   0x0000006e   Code   RO         1840    i.HAL_DMA_Abort     stm32wlxx_hal_dma.o
    0x0800090a   0x00000070   Code   RO         1841    i.HAL_DMA_Abort_IT  stm32wlxx_hal_dma.o
    0x0800097a   0x00000002   PAD
    0x0800097c   0x000000a8   Code   RO         1842    i.HAL_DMA_DeInit    stm32wlxx_hal_dma.o
    0x08000a24   0x000000d8   Code   RO         1845    i.HAL_DMA_IRQHandler  stm32wlxx_hal_dma.o
    0x08000afc   0x000000c8   Code   RO         1846    i.HAL_DMA_Init      stm32wlxx_hal_dma.o
    0x08000bc4   0x00000090   Code   RO         1850    i.HAL_DMA_Start_IT  stm32wlxx_hal_dma.o
    0x08000c54   0x0000000a   Code   RO          462    i.HAL_Delay         sys_app.o
    0x08000c5e   0x0000000c   Code   RO         2720    i.HAL_EXTI_GetHandle  stm32wlxx_hal_exti.o
    0x08000c6a   0x0000000e   Code   RO         2723    i.HAL_EXTI_RegisterCallback  stm32wlxx_hal_exti.o
    0x08000c78   0x000000f0   Code   RO         1765    i.HAL_GPIO_DeInit   stm32wlxx_hal_gpio.o
    0x08000d68   0x0000004c   Code   RO         1064    i.HAL_GPIO_EXTI_Callback  subghz_phy_app.o
    0x08000db4   0x00000018   Code   RO         1767    i.HAL_GPIO_EXTI_IRQHandler  stm32wlxx_hal_gpio.o
    0x08000dcc   0x00000160   Code   RO         1768    i.HAL_GPIO_Init     stm32wlxx_hal_gpio.o
    0x08000f2c   0x00000010   Code   RO         1771    i.HAL_GPIO_TogglePin  stm32wlxx_hal_gpio.o
    0x08000f3c   0x0000000a   Code   RO         1773    i.HAL_GPIO_WritePin  stm32wlxx_hal_gpio.o
    0x08000f46   0x00000002   PAD
    0x08000f48   0x00000014   Code   RO          463    i.HAL_GetTick       sys_app.o
    0x08000f5c   0x0000002c   Code   RO         2506    i.HAL_Init          stm32wlxx_hal.o
    0x08000f88   0x00000004   Code   RO          464    i.HAL_InitTick      sys_app.o
    0x08000f8c   0x00000002   Code   RO         1007    i.HAL_MspInit       stm32wlxx_hal_msp.o
    0x08000f8e   0x00000022   Code   RO         2357    i.HAL_NVIC_DisableIRQ  stm32wlxx_hal_cortex.o
    0x08000fb0   0x0000001a   Code   RO         2358    i.HAL_NVIC_EnableIRQ  stm32wlxx_hal_cortex.o
    0x08000fca   0x00000002   PAD
    0x08000fcc   0x00000040   Code   RO         2364    i.HAL_NVIC_SetPriority  stm32wlxx_hal_cortex.o
    0x0800100c   0x00000024   Code   RO         2365    i.HAL_NVIC_SetPriorityGrouping  stm32wlxx_hal_cortex.o
    0x08001030   0x00000010   Code   RO         2135    i.HAL_PWREx_GetVoltageRange  stm32wlxx_hal_pwr_ex.o
    0x08001040   0x00000010   Code   RO         1997    i.HAL_PWR_EnableBkUpAccess  stm32wlxx_hal_pwr.o
    0x08001050   0x000001a0   Code   RO         1385    i.HAL_RCCEx_PeriphCLKConfig  stm32wlxx_hal_rcc_ex.o
    0x080011f0   0x000001c8   Code   RO         1210    i.HAL_RCC_ClockConfig  stm32wlxx_hal_rcc.o
    0x080013b8   0x00000024   Code   RO         1215    i.HAL_RCC_GetHCLKFreq  stm32wlxx_hal_rcc.o
    0x080013dc   0x00000020   Code   RO         1217    i.HAL_RCC_GetPCLK1Freq  stm32wlxx_hal_rcc.o
    0x080013fc   0x00000020   Code   RO         1218    i.HAL_RCC_GetPCLK2Freq  stm32wlxx_hal_rcc.o
    0x0800141c   0x000000e4   Code   RO         1220    i.HAL_RCC_GetSysClockFreq  stm32wlxx_hal_rcc.o
    0x08001500   0x0000050e   Code   RO         1223    i.HAL_RCC_OscConfig  stm32wlxx_hal_rcc.o
    0x08001a0e   0x00000002   Code   RO         2961    i.HAL_RTCEx_AlarmBEventCallback  stm32wlxx_hal_rtc_ex.o
    0x08001a10   0x0000000c   Code   RO         2962    i.HAL_RTCEx_BKUPRead  stm32wlxx_hal_rtc_ex.o
    0x08001a1c   0x0000000c   Code   RO         2963    i.HAL_RTCEx_BKUPWrite  stm32wlxx_hal_rtc_ex.o
    0x08001a28   0x00000040   Code   RO         2973    i.HAL_RTCEx_EnableBypassShadow  stm32wlxx_hal_rtc_ex.o
    0x08001a68   0x00000010   Code   RO          602    i.HAL_RTCEx_SSRUEventCallback  timer_if.o
    0x08001a78   0x00000028   Code   RO         2988    i.HAL_RTCEx_SSRUIRQHandler  stm32wlxx_hal_rtc_ex.o
    0x08001aa0   0x00000050   Code   RO         2995    i.HAL_RTCEx_SetSSRU_IT  stm32wlxx_hal_rtc_ex.o
    0x08001af0   0x00000004   Code   RO          603    i.HAL_RTC_AlarmAEventCallback  timer_if.o
    0x08001af4   0x00000040   Code   RO         2789    i.HAL_RTC_AlarmIRQHandler  stm32wlxx_hal_rtc.o
    0x08001b34   0x00000084   Code   RO         2796    i.HAL_RTC_DeactivateAlarm  stm32wlxx_hal_rtc.o
    0x08001bb8   0x000000a8   Code   RO         2801    i.HAL_RTC_Init      stm32wlxx_hal_rtc.o
    0x08001c60   0x00000074   Code   RO          253    i.HAL_RTC_MspInit   rtc.o
    0x08001cd4   0x0000017c   Code   RO         2806    i.HAL_RTC_SetAlarm_IT  stm32wlxx_hal_rtc.o
    0x08001e50   0x00000034   Code   RO         2809    i.HAL_RTC_WaitForSynchro  stm32wlxx_hal_rtc.o
    0x08001e84   0x00000018   Code   RO         4115    i.HAL_SUBGHZ_CADStatusCallback  radio_driver.o
    0x08001e9c   0x0000000c   Code   RO         4116    i.HAL_SUBGHZ_CRCErrorCallback  radio_driver.o
    0x08001ea8   0x00000070   Code   RO         3288    i.HAL_SUBGHZ_ExecGetCmd  stm32wlxx_hal_subghz.o
    0x08001f18   0x0000007a   Code   RO         3289    i.HAL_SUBGHZ_ExecSetCmd  stm32wlxx_hal_subghz.o
    0x08001f92   0x00000002   PAD
    0x08001f94   0x0000000c   Code   RO         4117    i.HAL_SUBGHZ_HeaderErrorCallback  radio_driver.o
    0x08001fa0   0x0000000c   Code   RO         4118    i.HAL_SUBGHZ_HeaderValidCallback  radio_driver.o
    0x08001fac   0x00000094   Code   RO         3294    i.HAL_SUBGHZ_IRQHandler  stm32wlxx_hal_subghz.o
    0x08002040   0x000000a4   Code   RO         3295    i.HAL_SUBGHZ_Init   stm32wlxx_hal_subghz.o
    0x080020e4   0x0000002a   Code   RO          301    i.HAL_SUBGHZ_MspInit  subghz.o
    0x0800210e   0x00000002   PAD
    0x08002110   0x0000000c   Code   RO         4119    i.HAL_SUBGHZ_PreambleDetectedCallback  radio_driver.o
    0x0800211c   0x00000078   Code   RO         3299    i.HAL_SUBGHZ_ReadBuffer  stm32wlxx_hal_subghz.o
    0x08002194   0x00000080   Code   RO         3301    i.HAL_SUBGHZ_ReadRegisters  stm32wlxx_hal_subghz.o
    0x08002214   0x0000000c   Code   RO         4120    i.HAL_SUBGHZ_RxCpltCallback  radio_driver.o
    0x08002220   0x00000010   Code   RO         4121    i.HAL_SUBGHZ_RxTxTimeoutCallback  radio_driver.o
    0x08002230   0x0000000c   Code   RO         4122    i.HAL_SUBGHZ_SyncWordValidCallback  radio_driver.o
    0x0800223c   0x0000000c   Code   RO         4123    i.HAL_SUBGHZ_TxCpltCallback  radio_driver.o
    0x08002248   0x0000006e   Code   RO         3306    i.HAL_SUBGHZ_WriteBuffer  stm32wlxx_hal_subghz.o
    0x080022b6   0x0000007a   Code   RO         3308    i.HAL_SUBGHZ_WriteRegisters  stm32wlxx_hal_subghz.o
    0x08002330   0x0000004a   Code   RO         3967    i.HAL_UARTEx_EnableFifoMode  stm32wlxx_hal_uart_ex.o
    0x0800237a   0x0000002e   Code   RO         3968    i.HAL_UARTEx_EnableStopMode  stm32wlxx_hal_uart_ex.o
    0x080023a8   0x00000002   Code   RO         3551    i.HAL_UARTEx_RxEventCallback  stm32wlxx_hal_uart.o
    0x080023aa   0x00000002   Code   RO         3972    i.HAL_UARTEx_RxFifoFullCallback  stm32wlxx_hal_uart_ex.o
    0x080023ac   0x0000004c   Code   RO         3973    i.HAL_UARTEx_SetRxFifoThreshold  stm32wlxx_hal_uart_ex.o
    0x080023f8   0x0000004c   Code   RO         3974    i.HAL_UARTEx_SetTxFifoThreshold  stm32wlxx_hal_uart_ex.o
    0x08002444   0x0000008a   Code   RO         3975    i.HAL_UARTEx_StopModeWakeUpSourceConfig  stm32wlxx_hal_uart_ex.o
    0x080024ce   0x00000002   Code   RO         3976    i.HAL_UARTEx_TxFifoEmptyCallback  stm32wlxx_hal_uart_ex.o
    0x080024d0   0x00000002   Code   RO         3977    i.HAL_UARTEx_WakeupCallback  stm32wlxx_hal_uart_ex.o
    0x080024d2   0x00000002   Code   RO         3567    i.HAL_UART_ErrorCallback  stm32wlxx_hal_uart.o
    0x080024d4   0x000002e0   Code   RO         3570    i.HAL_UART_IRQHandler  stm32wlxx_hal_uart.o
    0x080027b4   0x0000006a   Code   RO         3571    i.HAL_UART_Init     stm32wlxx_hal_uart.o
    0x0800281e   0x00000002   PAD
    0x08002820   0x00000038   Code   RO          850    i.HAL_UART_MspDeInit  usart.o
    0x08002858   0x000000c4   Code   RO          851    i.HAL_UART_MspInit  usart.o
    0x0800291c   0x00000054   Code   RO         3576    i.HAL_UART_Receive_IT  stm32wlxx_hal_uart.o
    0x08002970   0x00000038   Code   RO          764    i.HAL_UART_RxCpltCallback  usart_if.o
    0x080029a8   0x000000a4   Code   RO         3581    i.HAL_UART_Transmit_DMA  stm32wlxx_hal_uart.o
    0x08002a4c   0x0000001c   Code   RO          765    i.HAL_UART_TxCpltCallback  usart_if.o
    0x08002a68   0x00000002   Code   RO         3584    i.HAL_UART_TxHalfCpltCallback  stm32wlxx_hal_uart.o
    0x08002a6a   0x00000002   Code   RO          899    i.HardFault_Handler  stm32wlxx_it.o
    0x08002a6c   0x00000014   Code   RO          217    i.LL_AHB1_GRP1_EnableClock  dma.o
    0x08002a80   0x00000014   Code   RO          182    i.LL_AHB2_GRP1_EnableClock  gpio.o
    0x08002a94   0x00000014   Code   RO         5509    i.LL_AHB2_GRP1_EnableClock  stm32wlxx_lm40x.o
    0x08002aa8   0x00000014   Code   RO         5619    i.LL_AHB2_GRP1_EnableClock  stm32wlxx_lm40x_radio.o
    0x08002abc   0x00000010   Code   RO         3309    i.LL_PWR_SelectSUBGHZSPI_NSS  stm32wlxx_hal_subghz.o
    0x08002acc   0x00000014   Code   RO         3310    i.LL_PWR_SetRadioBusyTrigger  stm32wlxx_hal_subghz.o
    0x08002ae0   0x00000010   Code   RO         3311    i.LL_PWR_UnselectSUBGHZSPI_NSS  stm32wlxx_hal_subghz.o
    0x08002af0   0x0000000c   Code   RO         1224    i.LL_RCC_GetSysClkSource  stm32wlxx_hal_rcc.o
    0x08002afc   0x0000000c   Code   RO         1225    i.LL_RCC_HSE_IsReady  stm32wlxx_hal_rcc.o
    0x08002b08   0x0000000c   Code   RO         1226    i.LL_RCC_HSI_IsReady  stm32wlxx_hal_rcc.o
    0x08002b14   0x00000012   Code   RO         1227    i.LL_RCC_HSI_SetCalibTrimming  stm32wlxx_hal_rcc.o
    0x08002b26   0x0000000e   Code   RO         1393    i.LL_RCC_LSE_IsReady  stm32wlxx_hal_rcc_ex.o
    0x08002b34   0x0000000c   Code   RO         1228    i.LL_RCC_MSI_IsReady  stm32wlxx_hal_rcc.o
    0x08002b40   0x00000012   Code   RO         1229    i.LL_RCC_MSI_SetCalibTrimming  stm32wlxx_hal_rcc.o
    0x08002b52   0x0000000c   Code   RO         1230    i.LL_RCC_PLL_GetMainSource  stm32wlxx_hal_rcc.o
    0x08002b5e   0x0000000c   Code   RO         1231    i.LL_RCC_PLL_IsReady  stm32wlxx_hal_rcc.o
    0x08002b6a   0x0000001e   Code   RO         1399    i.LL_RCC_SetI2CClockSource  stm32wlxx_hal_rcc_ex.o
    0x08002b88   0x00000016   Code   RO         1400    i.LL_RCC_SetLPTIMClockSource  stm32wlxx_hal_rcc_ex.o
    0x08002b9e   0x00000014   Code   RO         1401    i.LL_RCC_SetUSARTClockSource  stm32wlxx_hal_rcc_ex.o
    0x08002bb2   0x00000022   Code   RO          218    i.MX_DMA_Init       dma.o
    0x08002bd4   0x0000006c   Code   RO          183    i.MX_GPIO_Init      gpio.o
    0x08002c40   0x0000006c   Code   RO          254    i.MX_RTC_Init       rtc.o
    0x08002cac   0x00000020   Code   RO          302    i.MX_SUBGHZ_Init    subghz.o
    0x08002ccc   0x0000000e   Code   RO         1031    i.MX_SubGHz_Phy_Init  app_subghz_phy.o
    0x08002cda   0x00000002   PAD
    0x08002cdc   0x00000068   Code   RO          852    i.MX_USART2_UART_Init  usart.o
    0x08002d44   0x00000002   Code   RO          900    i.MemManage_Handler  stm32wlxx_it.o
    0x08002d46   0x00000002   Code   RO          901    i.NMI_Handler       stm32wlxx_it.o
    0x08002d48   0x000000fc   Code   RO         1065    i.OnRxDone          subghz_phy_app.o
    0x08002e44   0x00000030   Code   RO         1066    i.OnRxError         subghz_phy_app.o
    0x08002e74   0x00000034   Code   RO         1067    i.OnRxTimeout       subghz_phy_app.o
    0x08002ea8   0x00000030   Code   RO         1068    i.OnTxDone          subghz_phy_app.o
    0x08002ed8   0x00000034   Code   RO         1069    i.OnTxTimeout       subghz_phy_app.o
    0x08002f0c   0x00000084   Code   RO         1070    i.OnledEvent        subghz_phy_app.o
    0x08002f90   0x00000002   Code   RO          902    i.PendSV_Handler    stm32wlxx_it.o
    0x08002f92   0x00000002   PAD
    0x08002f94   0x000001d0   Code   RO         1071    i.PingPong_Process  subghz_phy_app.o
    0x08003164   0x00000004   Code   RO         1146    i.RBI_ConfigRFSwitch  radio_board_if.o
    0x08003168   0x00000004   Code   RO         1148    i.RBI_GetRFOMaxPowerConfig  radio_board_if.o
    0x0800316c   0x00000004   Code   RO         1149    i.RBI_GetTxConfig   radio_board_if.o
    0x08003170   0x00000004   Code   RO         1150    i.RBI_Init          radio_board_if.o
    0x08003174   0x00000004   Code   RO         1151    i.RBI_IsDCDC        radio_board_if.o
    0x08003178   0x00000004   Code   RO         1152    i.RBI_IsTCXO        radio_board_if.o
    0x0800317c   0x0000008c   Code   RO         1232    i.RCC_SetFlashLatency  stm32wlxx_hal_rcc.o
    0x08003208   0x00000044   Code   RO         1233    i.RCC_SetFlashLatencyFromMSIRange  stm32wlxx_hal_rcc.o
    0x0800324c   0x00000002   Code   RO         4540    i.RFW_DeInit        radio_fw.o
    0x0800324e   0x00000002   Code   RO         4541    i.RFW_DeInit_TxLongPacket  radio_fw.o
    0x08003250   0x00000006   Code   RO         4542    i.RFW_Init          radio_fw.o
    0x08003256   0x00000004   Code   RO         4543    i.RFW_Is_Init       radio_fw.o
    0x0800325a   0x00000004   Code   RO         4544    i.RFW_Is_LongPacketModeEnabled  radio_fw.o
    0x0800325e   0x00000006   Code   RO         4545    i.RFW_ReceiveInit   radio_fw.o
    0x08003264   0x00000006   Code   RO         4546    i.RFW_ReceiveLongPacket  radio_fw.o
    0x0800326a   0x00000002   Code   RO         4547    i.RFW_ReceivePayload  radio_fw.o
    0x0800326c   0x00000002   Code   RO         4548    i.RFW_SetAntSwitch  radio_fw.o
    0x0800326e   0x00000002   Code   RO         4549    i.RFW_SetRadioModem  radio_fw.o
    0x08003270   0x00000006   Code   RO         4550    i.RFW_TransmitInit  radio_fw.o
    0x08003276   0x00000006   Code   RO         4551    i.RFW_TransmitLongPacket  radio_fw.o
    0x0800327c   0x0000000c   Code   RO          903    i.RTC_Alarm_IRQHandler  stm32wlxx_it.o
    0x08003288   0x00000016   Code   RO         2811    i.RTC_ByteToBcd2    stm32wlxx_hal_rtc.o
    0x0800329e   0x00000002   PAD
    0x080032a0   0x0000004c   Code   RO         2812    i.RTC_EnterInitMode  stm32wlxx_hal_rtc.o
    0x080032ec   0x00000058   Code   RO         2813    i.RTC_ExitInitMode  stm32wlxx_hal_rtc.o
    0x08003344   0x00000004   Code   RO         4636    i.RadioCheckRfFrequency  radio.o
    0x08003348   0x0000007a   Code   RO         4637    i.RadioGetLoRaTimeOnAirNumerator  radio.o
    0x080033c2   0x00000022   Code   RO         4638    i.RadioGetStatus    radio.o
    0x080033e4   0x0000000a   Code   RO         4639    i.RadioGetWakeupTime  radio.o
    0x080033ee   0x00000002   PAD
    0x080033f0   0x00000090   Code   RO         4640    i.RadioInit         radio.o
    0x08003480   0x000002bc   Code   RO         4641    i.RadioIrqProcess   radio.o
    0x0800373c   0x00000086   Code   RO         4642    i.RadioIsChannelFree  radio.o
    0x080037c2   0x00000002   PAD
    0x080037c4   0x00000010   Code   RO         4643    i.RadioOnDioIrq     radio.o
    0x080037d4   0x00000018   Code   RO         4644    i.RadioOnRxTimeoutIrq  radio.o
    0x080037ec   0x00000018   Code   RO         4645    i.RadioOnTxTimeoutIrq  radio.o
    0x08003804   0x00000016   Code   RO         4646    i.RadioRandom       radio.o
    0x0800381a   0x00000004   Code   RO         4647    i.RadioRead         radio.o
    0x0800381e   0x00000004   Code   RO         4648    i.RadioReadRegisters  radio.o
    0x08003822   0x00000004   Code   RO         4649    i.RadioRssi         radio.o
    0x08003826   0x00000002   PAD
    0x08003828   0x00000060   Code   RO         4650    i.RadioRx           radio.o
    0x08003888   0x00000060   Code   RO         4651    i.RadioRxBoosted    radio.o
    0x080038e8   0x00000158   Code   RO         4652    i.RadioSend         radio.o
    0x08003a40   0x00000004   Code   RO         4653    i.RadioSetChannel   radio.o
    0x08003a44   0x00000034   Code   RO         4654    i.RadioSetMaxPayloadLength  radio.o
    0x08003a78   0x0000004c   Code   RO         4655    i.RadioSetModem     radio.o
    0x08003ac4   0x00000038   Code   RO         4656    i.RadioSetPublicNetwork  radio.o
    0x08003afc   0x000002b0   Code   RO         4657    i.RadioSetRxConfig  radio.o
    0x08003dac   0x00000038   Code   RO         4658    i.RadioSetRxDutyCycle  radio.o
    0x08003de4   0x00000228   Code   RO         4659    i.RadioSetRxGenericConfig  radio.o
    0x0800400c   0x00000180   Code   RO         4660    i.RadioSetTxConfig  radio.o
    0x0800418c   0x0000003c   Code   RO         4661    i.RadioSetTxContinuousWave  radio.o
    0x080041c8   0x0000028c   Code   RO         4662    i.RadioSetTxGenericConfig  radio.o
    0x08004454   0x00000012   Code   RO         4663    i.RadioSleep        radio.o
    0x08004466   0x00000006   Code   RO         4664    i.RadioStandby      radio.o
    0x0800446c   0x00000028   Code   RO         4665    i.RadioStartCad     radio.o
    0x08004494   0x000000d0   Code   RO         4666    i.RadioTimeOnAir    radio.o
    0x08004564   0x00000014   Code   RO         4667    i.RadioTxCw         radio.o
    0x08004578   0x00000030   Code   RO         4668    i.RadioTxPrbs       radio.o
    0x080045a8   0x00000004   Code   RO         4669    i.RadioWrite        radio.o
    0x080045ac   0x00000004   Code   RO         4670    i.RadioWriteRegisters  radio.o
    0x080045b0   0x00000028   Code   RO         4124    i.Radio_SMPS_Set    radio_driver.o
    0x080045d8   0x00000034   Code   RO         5181    i.SEQ_BitPosition   stm32_seq.o
    0x0800460c   0x00000024   Code   RO         3313    i.SUBGHZSPI_Init    stm32wlxx_hal_subghz.o
    0x08004630   0x0000005c   Code   RO         3314    i.SUBGHZSPI_Receive  stm32wlxx_hal_subghz.o
    0x0800468c   0x00000058   Code   RO         3315    i.SUBGHZSPI_Transmit  stm32wlxx_hal_subghz.o
    0x080046e4   0x00000038   Code   RO         3316    i.SUBGHZ_CheckDeviceReady  stm32wlxx_hal_subghz.o
    0x0800471c   0x0000000c   Code   RO          904    i.SUBGHZ_Radio_IRQHandler  stm32wlxx_it.o
    0x08004728   0x00000048   Code   RO         3317    i.SUBGHZ_WaitOnBusy  stm32wlxx_hal_subghz.o
    0x08004770   0x00000046   Code   RO         4125    i.SUBGRF_Calibrate  radio_driver.o
    0x080047b6   0x00000002   PAD
    0x080047b8   0x00000074   Code   RO         4126    i.SUBGRF_CalibrateImage  radio_driver.o
    0x0800482c   0x00000074   Code   RO         4129    i.SUBGRF_GetCFO     radio_driver.o
    0x080048a0   0x00000028   Code   RO         4131    i.SUBGRF_GetFskBandwidthRegValue  radio_driver.o
    0x080048c8   0x0000000c   Code   RO         4133    i.SUBGRF_GetOperatingMode  radio_driver.o
    0x080048d4   0x00000074   Code   RO         4134    i.SUBGRF_GetPacketStatus  radio_driver.o
    0x08004948   0x0000002e   Code   RO         4136    i.SUBGRF_GetPayload  radio_driver.o
    0x08004976   0x00000004   Code   RO         4137    i.SUBGRF_GetRadioWakeUpTime  radio_driver.o
    0x0800497a   0x0000005e   Code   RO         4138    i.SUBGRF_GetRandom  radio_driver.o
    0x080049d8   0x00000018   Code   RO         4139    i.SUBGRF_GetRssiInst  radio_driver.o
    0x080049f0   0x0000003c   Code   RO         4140    i.SUBGRF_GetRxBufferStatus  radio_driver.o
    0x08004a2c   0x0000005c   Code   RO         4142    i.SUBGRF_Init       radio_driver.o
    0x08004a88   0x00000020   Code   RO         4143    i.SUBGRF_ReadBuffer  radio_driver.o
    0x08004aa8   0x00000020   Code   RO         4144    i.SUBGRF_ReadCommand  radio_driver.o
    0x08004ac8   0x00000018   Code   RO         4145    i.SUBGRF_ReadRegister  radio_driver.o
    0x08004ae0   0x00000020   Code   RO         4146    i.SUBGRF_ReadRegisters  radio_driver.o
    0x08004b00   0x00000012   Code   RO         4147    i.SUBGRF_SendPayload  radio_driver.o
    0x08004b12   0x00000016   Code   RO         4148    i.SUBGRF_SetBufferBaseAddress  radio_driver.o
    0x08004b28   0x00000018   Code   RO         4149    i.SUBGRF_SetCad     radio_driver.o
    0x08004b40   0x00000028   Code   RO         4151    i.SUBGRF_SetCrcPolynomial  radio_driver.o
    0x08004b68   0x00000028   Code   RO         4152    i.SUBGRF_SetCrcSeed  radio_driver.o
    0x08004b90   0x00000036   Code   RO         4153    i.SUBGRF_SetDioIrqParams  radio_driver.o
    0x08004bc6   0x00000034   Code   RO         4155    i.SUBGRF_SetLoRaSymbNumTimeout  radio_driver.o
    0x08004bfa   0x00000002   PAD
    0x08004bfc   0x000000e4   Code   RO         4156    i.SUBGRF_SetModulationParams  radio_driver.o
    0x08004ce0   0x0000001e   Code   RO         4157    i.SUBGRF_SetPaConfig  radio_driver.o
    0x08004cfe   0x00000002   PAD
    0x08004d00   0x000000d8   Code   RO         4158    i.SUBGRF_SetPacketParams  radio_driver.o
    0x08004dd8   0x00000028   Code   RO         4159    i.SUBGRF_SetPacketType  radio_driver.o
    0x08004e00   0x0000000a   Code   RO         4160    i.SUBGRF_SetPayload  radio_driver.o
    0x08004e0a   0x0000001c   Code   RO         4161    i.SUBGRF_SetRegulatorMode  radio_driver.o
    0x08004e26   0x00000002   PAD
    0x08004e28   0x0000004c   Code   RO         4162    i.SUBGRF_SetRfFrequency  radio_driver.o
    0x08004e74   0x0000002a   Code   RO         4163    i.SUBGRF_SetRfTxPower  radio_driver.o
    0x08004e9e   0x00000002   PAD
    0x08004ea0   0x00000028   Code   RO         4164    i.SUBGRF_SetRx      radio_driver.o
    0x08004ec8   0x00000034   Code   RO         4165    i.SUBGRF_SetRxBoosted  radio_driver.o
    0x08004efc   0x00000038   Code   RO         4166    i.SUBGRF_SetRxDutyCycle  radio_driver.o
    0x08004f34   0x00000040   Code   RO         4168    i.SUBGRF_SetSleep   radio_driver.o
    0x08004f74   0x00000024   Code   RO         4169    i.SUBGRF_SetStandby  radio_driver.o
    0x08004f98   0x0000000e   Code   RO         4170    i.SUBGRF_SetStopRxTimerOnPreambleDetect  radio_driver.o
    0x08004fa6   0x00000028   Code   RO         4171    i.SUBGRF_SetSwitch  radio_driver.o
    0x08004fce   0x00000012   Code   RO         4172    i.SUBGRF_SetSyncWord  radio_driver.o
    0x08004fe0   0x00000026   Code   RO         4173    i.SUBGRF_SetTcxoMode  radio_driver.o
    0x08005006   0x00000002   PAD
    0x08005008   0x00000028   Code   RO         4174    i.SUBGRF_SetTx      radio_driver.o
    0x08005030   0x0000000a   Code   RO         4175    i.SUBGRF_SetTxContinuousWave  radio_driver.o
    0x0800503a   0x0000000a   Code   RO         4176    i.SUBGRF_SetTxInfinitePreamble  radio_driver.o
    0x08005044   0x0000010e   Code   RO         4177    i.SUBGRF_SetTxParams  radio_driver.o
    0x08005152   0x00000002   PAD
    0x08005154   0x00000038   Code   RO         4178    i.SUBGRF_SetWhiteningSeed  radio_driver.o
    0x0800518c   0x00000020   Code   RO         4179    i.SUBGRF_WriteBuffer  radio_driver.o
    0x080051ac   0x00000020   Code   RO         4180    i.SUBGRF_WriteCommand  radio_driver.o
    0x080051cc   0x00000014   Code   RO         4181    i.SUBGRF_WriteRegister  radio_driver.o
    0x080051e0   0x00000020   Code   RO         4182    i.SUBGRF_WriteRegisters  radio_driver.o
    0x08005200   0x00000002   Code   RO          905    i.SVC_Handler       stm32wlxx_it.o
    0x08005202   0x00000002   PAD
    0x08005204   0x00000244   Code   RO         1072    i.SubghzApp_Init    subghz_phy_app.o
    0x08005448   0x00000002   Code   RO          906    i.SysTick_Handler   stm32wlxx_it.o
    0x0800544a   0x00000026   Code   RO         5048    i.SysTimeAdd        stm32_systime.o
    0x08005470   0x00000044   Code   RO         5050    i.SysTimeGet        stm32_systime.o
    0x080054b4   0x00000048   Code   RO          465    i.SystemApp_Init    sys_app.o
    0x080054fc   0x00000084   Code   RO           15    i.SystemClock_Config  main.o
    0x08005580   0x00000002   Code   RO         4078    i.SystemInit        system_stm32wlxx.o
    0x08005582   0x00000002   PAD
    0x08005584   0x0000000c   Code   RO          907    i.TAMP_STAMP_LSECSS_SSRU_IRQHandler  stm32wlxx_it.o
    0x08005590   0x0000000c   Code   RO          604    i.TIMER_IF_BkUp_Read_MSBticks  timer_if.o
    0x0800559c   0x0000000c   Code   RO          605    i.TIMER_IF_BkUp_Read_Seconds  timer_if.o
    0x080055a8   0x0000000c   Code   RO          606    i.TIMER_IF_BkUp_Read_SubSeconds  timer_if.o
    0x080055b4   0x00000010   Code   RO          607    i.TIMER_IF_BkUp_Write_MSBticks  timer_if.o
    0x080055c4   0x00000010   Code   RO          608    i.TIMER_IF_BkUp_Write_Seconds  timer_if.o
    0x080055d4   0x00000010   Code   RO          609    i.TIMER_IF_BkUp_Write_SubSeconds  timer_if.o
    0x080055e4   0x00000010   Code   RO          610    i.TIMER_IF_Convert_Tick2ms  timer_if.o
    0x080055f4   0x00000012   Code   RO          611    i.TIMER_IF_Convert_ms2Tick  timer_if.o
    0x08005606   0x0000001e   Code   RO          612    i.TIMER_IF_DelayMs  timer_if.o
    0x08005624   0x00000004   Code   RO          613    i.TIMER_IF_GetMinimumTimeout  timer_if.o
    0x08005628   0x00000028   Code   RO          614    i.TIMER_IF_GetTime  timer_if.o
    0x08005650   0x0000000c   Code   RO          615    i.TIMER_IF_GetTimerContext  timer_if.o
    0x0800565c   0x00000014   Code   RO          616    i.TIMER_IF_GetTimerElapsedTime  timer_if.o
    0x08005670   0x00000014   Code   RO          617    i.TIMER_IF_GetTimerValue  timer_if.o
    0x08005684   0x00000048   Code   RO          618    i.TIMER_IF_Init     timer_if.o
    0x080056cc   0x00000010   Code   RO          619    i.TIMER_IF_SetTimerContext  timer_if.o
    0x080056dc   0x0000004c   Code   RO          620    i.TIMER_IF_StartTimer  timer_if.o
    0x08005728   0x00000024   Code   RO          621    i.TIMER_IF_StopTimer  timer_if.o
    0x0800574c   0x00000060   Code   RO         4843    i.TRACE_AllocateBufer  stm32_adv_trace.o
    0x080057ac   0x00000018   Code   RO         4844    i.TRACE_Lock        stm32_adv_trace.o
    0x080057c4   0x00000088   Code   RO         4845    i.TRACE_Send        stm32_adv_trace.o
    0x0800584c   0x00000094   Code   RO         4846    i.TRACE_TxCpltCallback  stm32_adv_trace.o
    0x080058e0   0x00000018   Code   RO         4847    i.TRACE_UnLock      stm32_adv_trace.o
    0x080058f8   0x0000001c   Code   RO         5311    i.TimerExists       stm32_timer.o
    0x08005914   0x00000018   Code   RO         5312    i.TimerInsertNewHeadTimer  stm32_timer.o
    0x0800592c   0x00000028   Code   RO         5313    i.TimerInsertTimer  stm32_timer.o
    0x08005954   0x00000034   Code   RO         5314    i.TimerSetTimeout   stm32_timer.o
    0x08005988   0x00000034   Code   RO          466    i.TimestampNow      sys_app.o
    0x080059bc   0x00000044   Code   RO         3978    i.UARTEx_SetNbDataToProcess  stm32wlxx_hal_uart_ex.o
    0x08005a00   0x000000c8   Code   RO         3585    i.UART_AdvFeatureConfig  stm32wlxx_hal_uart.o
    0x08005ac8   0x00000060   Code   RO         3586    i.UART_CheckIdleState  stm32wlxx_hal_uart.o
    0x08005b28   0x00000014   Code   RO         3587    i.UART_DMAAbortOnError  stm32wlxx_hal_uart.o
    0x08005b3c   0x00000050   Code   RO         3588    i.UART_DMAError     stm32wlxx_hal_uart.o
    0x08005b8c   0x00000042   Code   RO         3593    i.UART_DMATransmitCplt  stm32wlxx_hal_uart.o
    0x08005bce   0x0000000a   Code   RO         3595    i.UART_DMATxHalfCplt  stm32wlxx_hal_uart.o
    0x08005bd8   0x00000054   Code   RO         3597    i.UART_EndRxTransfer  stm32wlxx_hal_uart.o
    0x08005c2c   0x0000002e   Code   RO         3598    i.UART_EndTxTransfer  stm32wlxx_hal_uart.o
    0x08005c5a   0x000000a2   Code   RO         3599    i.UART_RxISR_16BIT  stm32wlxx_hal_uart.o
    0x08005cfc   0x00000170   Code   RO         3600    i.UART_RxISR_16BIT_FIFOEN  stm32wlxx_hal_uart.o
    0x08005e6c   0x000000a2   Code   RO         3601    i.UART_RxISR_8BIT   stm32wlxx_hal_uart.o
    0x08005f0e   0x00000002   PAD
    0x08005f10   0x00000170   Code   RO         3602    i.UART_RxISR_8BIT_FIFOEN  stm32wlxx_hal_uart.o
    0x08006080   0x00000248   Code   RO         3603    i.UART_SetConfig    stm32wlxx_hal_uart.o
    0x080062c8   0x00000118   Code   RO         3605    i.UART_Start_Receive_IT  stm32wlxx_hal_uart.o
    0x080063e0   0x000000c4   Code   RO         3610    i.UART_WaitOnFlagUntilTimeout  stm32wlxx_hal_uart.o
    0x080064a4   0x0000000c   Code   RO          908    i.USART2_IRQHandler  stm32wlxx_it.o
    0x080064b0   0x000000b4   Code   RO         4848    i.UTIL_ADV_TRACE_COND_FSend  stm32_adv_trace.o
    0x08006564   0x00000034   Code   RO         4856    i.UTIL_ADV_TRACE_Init  stm32_adv_trace.o
    0x08006598   0x00000008   Code   RO          467    i.UTIL_ADV_TRACE_PostSendHook  sys_app.o
    0x080065a0   0x00000008   Code   RO          468    i.UTIL_ADV_TRACE_PreSendHook  sys_app.o
    0x080065a8   0x0000000c   Code   RO         4860    i.UTIL_ADV_TRACE_RegisterTimeStampFunction  stm32_adv_trace.o
    0x080065b4   0x0000000c   Code   RO         4864    i.UTIL_ADV_TRACE_SetVerboseLevel  stm32_adv_trace.o
    0x080065c0   0x00000010   Code   RO         5441    i.UTIL_LPM_Init     stm32_lpm.o
    0x080065d0   0x00000024   Code   RO         5442    i.UTIL_LPM_SetOffMode  stm32_lpm.o
    0x080065f4   0x00000024   Code   RO         5443    i.UTIL_LPM_SetStopMode  stm32_lpm.o
    0x08006618   0x00000012   Code   RO         5012    i.UTIL_MEM_cpy_8    stm32_mem.o
    0x0800662a   0x0000000e   Code   RO         5014    i.UTIL_MEM_set_8    stm32_mem.o
    0x08006638   0x00000020   Code   RO         5193    i.UTIL_SEQ_RegTask  stm32_seq.o
    0x08006658   0x00000028   Code   RO         5197    i.UTIL_SEQ_SetTask  stm32_seq.o
    0x08006680   0x0000003c   Code   RO         5315    i.UTIL_TIMER_Create  stm32_timer.o
    0x080066bc   0x00000014   Code   RO         5317    i.UTIL_TIMER_GetCurrentTime  stm32_timer.o
    0x080066d0   0x00000020   Code   RO         5318    i.UTIL_TIMER_GetElapsedTime  stm32_timer.o
    0x080066f0   0x00000088   Code   RO         5321    i.UTIL_TIMER_IRQ_Handler  stm32_timer.o
    0x08006778   0x00000014   Code   RO         5322    i.UTIL_TIMER_Init   stm32_timer.o
    0x0800678c   0x00000038   Code   RO         5324    i.UTIL_TIMER_SetPeriod  stm32_timer.o
    0x080067c4   0x0000007c   Code   RO         5326    i.UTIL_TIMER_Start  stm32_timer.o
    0x08006840   0x00000068   Code   RO         5328    i.UTIL_TIMER_Stop   stm32_timer.o
    0x080068a8   0x00000002   Code   RO          909    i.UsageFault_Handler  stm32wlxx_it.o
    0x080068aa   0x00000020   Code   RO         2371    i.__NVIC_SetPriority  stm32wlxx_hal_cortex.o
    0x080068ca   0x00000002   PAD
    0x080068cc   0x000000f0   Code   RO         5158    i.ee_number         stm32_tiny_vsnprintf.o
    0x080069bc   0x00000012   Code   RO           16    i.main              main.o
    0x080069ce   0x0000007c   Code   RO         4671    i.payload_integration  radio.o
    0x08006a4a   0x00000012   Code   RO          470    i.tiny_snprintf_like  sys_app.o
    0x08006a5c   0x00000150   Code   RO         5159    i.tiny_vsnprintf_like  stm32_tiny_vsnprintf.o
    0x08006bac   0x0000002c   Code   RO          766    i.vcom_DeInit       usart_if.o
    0x08006bd8   0x00000024   Code   RO          767    i.vcom_Init         usart_if.o
    0x08006bfc   0x00000048   Code   RO          768    i.vcom_ReceiveInit  usart_if.o
    0x08006c44   0x00000014   Code   RO          771    i.vcom_Trace_DMA    usart_if.o
    0x08006c58   0x0000002c   Data   RO          622    .constdata          timer_if.o
    0x08006c84   0x00000014   Data   RO          623    .constdata          timer_if.o
    0x08006c98   0x00000010   Data   RO          772    .constdata          usart_if.o
    0x08006ca8   0x0000001c   Data   RO         1234    .constdata          stm32wlxx_hal_rcc.o
    0x08006cc4   0x00000018   Data   RO         3611    .constdata          stm32wlxx_hal_uart.o
    0x08006cdc   0x00000010   Data   RO         3979    .constdata          stm32wlxx_hal_uart_ex.o
    0x08006cec   0x00000080   Data   RO         4079    .constdata          system_stm32wlxx.o
    0x08006d6c   0x00000020   Data   RO         4080    .constdata          system_stm32wlxx.o
    0x08006d8c   0x000000b0   Data   RO         4183    .constdata          radio_driver.o
    0x08006e3c   0x00000084   Data   RO         4673    .constdata          radio.o
    0x08006ec0   0x00000003   Data   RO         4674    .constdata          radio.o
    0x08006ec3   0x00000010   Data   RO         5199    .constdata          stm32_seq.o
    0x08006ed3   0x00000001   PAD
    0x08006ed4   0x0000001c   Data   RO         5511    .constdata          stm32wlxx_lm40x.o
    0x08006ef0   0x0000004d   Data   RO         5160    .conststring        stm32_tiny_vsnprintf.o
    0x08006f3d   0x00000003   PAD
    0x08006f40   0x00000020   Data   RO         5856    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Base: 0x20000000, Size: 0x00001338, Max: 0x00008000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20000000   0x00000001   Data   RW          471    .data               sys_app.o
    0x20000001   0x00000003   PAD
    0x20000004   0x00000008   Data   RW          624    .data               timer_if.o
    0x2000000c   0x0000000c   Data   RW          773    .data               usart_if.o
    0x20000018   0x0000000c   Data   RW         1074    .data               subghz_phy_app.o
    0x20000024   0x0000000c   Data   RW         2521    .data               stm32wlxx_hal.o
    0x20000030   0x00000004   Data   RW         4081    .data               system_stm32wlxx.o
    0x20000034   0x0000000c   Data   RW         4184    .data               radio_driver.o
    0x20000040   0x00000008   Data   RW         4675    .data               radio.o
    0x20000048   0x00000008   Data   RW         5161    .data               stm32_tiny_vsnprintf.o
    0x20000050   0x00000024   Data   RW         5200    .data               stm32_seq.o
    0x20000074   0x00000004   Data   RW         5329    .data               stm32_timer.o
    0x20000078   0x00000008   Data   RW         5444    .data               stm32_lpm.o
    0x20000080   0x00000030   Data   RW         5512    .data               stm32wlxx_lm40x.o
    0x200000b0   0x00000038   Zero   RW          255    .bss                rtc.o
    0x200000e8   0x0000000c   Zero   RW          303    .bss                subghz.o
    0x200000f4   0x000000f0   Zero   RW          853    .bss                usart.o
    0x200001e4   0x00000234   Zero   RW         1073    .bss                subghz_phy_app.o
    0x20000418   0x0000018c   Zero   RW         4672    .bss                radio.o
    0x200005a4   0x00000318   Zero   RW         4868    .bss                stm32_adv_trace.o
    0x200008bc   0x00000018   Zero   RW         5510    .bss                stm32wlxx_lm40x.o
    0x200008d4   0x00000060   Zero   RW         5731    .bss                c_w.l(libspace.o)
    0x20000934   0x00000004   PAD
    0x20000938   0x00000200   Zero   RW            3    HEAP                startup_stm32wle5xx.o
    0x20000b38   0x00000800   Zero   RW            2    STACK               startup_stm32wle5xx.o


    Execution Region RW_IRAM2 (Base: 0x20008000, Size: 0x00008000, Max: 0x00008000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20008000   0x00008000   Zero   RW            1    RW_IRAM2.bss        anon$$obj.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

        14          0          0          0          0        537   app_subghz_phy.o
        54          0          0          0          0       6706   dma.o
       128          4          0          0          0       6799   gpio.o
       154          4          0          0          0     495413   main.o
      4834        336        135          8        396      31164   radio.o
        24          0          0          0          0       3807   radio_board_if.o
      2854        224        176         12          0      50565   radio_driver.o
        48          0          0          0          0       9533   radio_fw.o
       224         14          0          0         56      30419   rtc.o
        64         26        312          0       2560        848   startup_stm32wle5xx.o
       684         68          0          0        792       8179   stm32_adv_trace.o
        88         14          0          8          0       2241   stm32_lpm.o
         0          0          0          0          0       3227   stm32_lpm_if.o
        32          0          0          0          0       1522   stm32_mem.o
       124         18         16         36          0       3273   stm32_seq.o
       106          6          0          0          0       4793   stm32_systime.o
       696         72          0          4          0       8946   stm32_timer.o
       576         12         77          8          0       3246   stm32_tiny_vsnprintf.o
        44          6          0         12          0       9834   stm32wlxx_hal.o
       192         14          0          0          0      33452   stm32wlxx_hal_cortex.o
      1128         52          0          0          0       6783   stm32wlxx_hal_dma.o
        26          0          0          0          0       1837   stm32wlxx_hal_exti.o
         0          0          0          0          0       5052   stm32wlxx_hal_flash.o
       642         40          0          0          0       3974   stm32wlxx_hal_gpio.o
         2          0          0          0          0        470   stm32wlxx_hal_msp.o
        16          4          0          0          0        555   stm32wlxx_hal_pwr.o
        16          6          0          0          0        584   stm32wlxx_hal_pwr_ex.o
      2394         84         28          0          0      46660   stm32wlxx_hal_rcc.o
       502          6          0          0          0      26716   stm32wlxx_hal_rcc_ex.o
       982         46          0          0          0       6481   stm32wlxx_hal_rtc.o
       210         28          0          0          0       4352   stm32wlxx_hal_rtc_ex.o
      1422         68          0          0          0      49003   stm32wlxx_hal_subghz.o
      3818        124         24          0          0      60214   stm32wlxx_hal_uart.o
       484          6         16          0          0       6833   stm32wlxx_hal_uart_ex.o
        84         30          0          0          0       7157   stm32wlxx_it.o
       328         30         28         48         24       8647   stm32wlxx_lm40x.o
       202          0          0          0          0       4139   stm32wlxx_lm40x_radio.o
        74          4          0          0         12       7484   subghz.o
      1704        640          0         12        564      13229   subghz_phy_app.o
       192         24          0          1          0      33647   sys_app.o
         2          0        160          4          0       1293   system_stm32wlxx.o
       484         80         64          8          0      38553   timer_if.o
       356         30          0          0        240       8466   usart.o
       256         44         16         12          0      14965   usart_if.o

    ----------------------------------------------------------------------
     26316       2164       1088        176      37412    1071598   Object Totals
         0          0         32          0      32768          0   (incl. Generated)
        52          0          4          3          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

         8          0          0          0          0         68   __main.o
         0          0          0          0          0          0   __rtentry.o
        12          0          0          0          0          0   __rtentry2.o
         6          0          0          0          0          0   __rtentry4.o
        52          8          0          0          0          0   __scatter.o
        26          0          0          0          0          0   __scatter_copy.o
        28          0          0          0          0          0   __scatter_zi.o
        12          0          0          0          0         72   exit.o
         6          0          0          0          0        152   heapauxi.o
         0          0          0          0          0          0   indicate_semi.o
         2          0          0          0          0          0   libinit.o
         2          0          0          0          0          0   libinit2.o
         2          0          0          0          0          0   libshutdown.o
         2          0          0          0          0          0   libshutdown2.o
         8          4          0          0         96         68   libspace.o
       238          0          0          0          0        100   lludivv7m.o
        68          0          0          0          0         68   rt_memclr.o
        78          0          0          0          0         80   rt_memclr_w.o
       138          0          0          0          0         68   rt_memcpy_v6.o
       100          0          0          0          0         80   rt_memcpy_w.o
         2          0          0          0          0          0   rtexit.o
        10          0          0          0          0          0   rtexit2.o
        62          0          0          0          0         76   strlen.o
       150          0          0          0          0         80   strncmp.o
        12          4          0          0          0         68   sys_exit.o
        74          0          0          0          0         80   sys_stackheap_outer.o
         2          0          0          0          0         68   use_no_semi.o

    ----------------------------------------------------------------------
      1108         16          0          0        100       1128   Library Totals
         8          0          0          0          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      1100         16          0          0         96       1128   c_w.l

    ----------------------------------------------------------------------
      1108         16          0          0        100       1128   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     27424       2180       1088        176      37512    1054626   Grand Totals
     27424       2180       1088        176      37512    1054626   ELF Image Totals
     27424       2180       1088        176          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                28512 (  27.84kB)
    Total RW  Size (RW Data + ZI Data)             37688 (  36.80kB)
    Total ROM Size (Code + RO Data + RW Data)      28688 (  28.02kB)

==============================================================================

