#

##

##

##

##

##

##

    猩ision Build Log
    Tool Versions:
    IDE-Version: 米Vision V5.14.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: 1 Administrator, 1, LIC=Q7GVE-5ECXL-17YRR-KVL4V-XVRY2-YK1LI

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.14.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.05 update 1 (build 106)
    Assembler:       Armasm.exe V5.05 update 1 (build 106)
    Linker/Locator:  ArmLink.exe V5.05 update 1 (build 106)
    Library Manager: ArmAr.exe V5.05 update 1 (build 106)
    Hex Converter:   FromElf.exe V5.05 update 1 (build 106)
    CPU DLL:         SARMCM3.DLL V5.14.0.0
    Dialog DLL:      DCM.DLL V1.13.1.0
    Target DLL:      STLink\ST-LINKIII-KEIL_SWO.dll V2.0.14.0_KEIL
    Dialog DLL:      TCM.DLL V1.14.4.0

    Project:
    C:\Users\gxy\Desktop\LM402-Pro-Kit_V1.0訧蹋婦\LM402-Pro-Kit_demo_V1.1\SubGHz_Phy_PingPong\MDK-ARM\SubGHz_Phy_PingPong.uvprojx
    Project File Date:  03/19/2025

    Output:
    Build target 'SubGHz_Phy_PingPong'
    compiling radio.c...
    linking...
    Program Size: Code=27424 RO-data=1088 RW-data=176 ZI-data=37512
    FromELF: creating hex file...
    "SubGHz_Phy_PingPong\SubGHz_Phy_PingPong.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.2.0.pack
                    ARM::CMSIS:CORE:3.40.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 3.40.0

    Collection of Component include folders:
      C:\Users\gxy\Desktop\LM402-Pro-Kit_V1.0訧蹋婦\LM402-Pro-Kit_demo_V1.1\SubGHz_Phy_PingPong\MDK-ARM\RTE
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.2.0\CMSIS\Include
      C:\Keil_v5\ARM\PACK\Keil\STM32WLxx_DFP\1.1.0

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:3.40.0
          Source file:   CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c